// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "ar9344.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	model = "TP-Link TL-WR841HP v2";
	compatible = "tplink,tl-wr841hp-v2", "qca,ar9344";

	aliases {
		led-boot = &led_system;
		led-failsafe = &led_system;
		led-running = &led_system;
		led-upgrade = &led_system;
		label-mac-device = &wmac;
	};

	keys {
		compatible = "gpio-keys";

		reset {
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 4 GPIO_ACTIVE_HIGH>;
			debounce-interval = <60>;
		};
	};

	leds {
		compatible = "gpio-leds";

		wan {
			label = "green:wan";
			gpios = <&gpio 11 GPIO_ACTIVE_LOW>;
		};

		lan1 {
			label = "green:lan1";
			gpios = <&gpio 12 GPIO_ACTIVE_LOW>;
		};

		lan2 {
			label = "green:lan2";
			gpios = <&gpio 13 GPIO_ACTIVE_LOW>;
		};

		lan3 {
			label = "green:lan3";
			gpios = <&gpio 14 GPIO_ACTIVE_LOW>;
		};

		lan4 {
			label = "green:lan4";
			gpios = <&gpio 15 GPIO_ACTIVE_LOW>;
		};

		wps {
			label = "green:wps";
			gpios = <&gpio 16 GPIO_ACTIVE_LOW>;
		};

		wlan {
			label = "green:wlan";
			gpios = <&gpio 21 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0tpt";
		};

		led_system: system {
			label = "green:system";
			gpios = <&gpio 22 GPIO_ACTIVE_LOW>;
			default-state = "on";
		};
	};
};

&ref {
	clock-frequency = <40000000>;
};

&spi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <25000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			uboot: partition@0 {
				label = "u-boot";
				reg = <0x000000 0x020000>;
				read-only;
			};

			partition@20000 {
				compatible = "tplink,firmware";
				label = "firmware";
				reg = <0x020000 0x7d0000>;
			};

			art: partition@7f0000 {
				label = "art";
				reg = <0x7f0000 0x010000>;
				read-only;
			};
		};
	};
};

&gpio {
	gpio_ext_lna0 {
		gpio-hog;
		gpios = <18 GPIO_ACTIVE_HIGH>;
		output-high;
		line-name = "tp-link:ext:lna0";
	};

	gpio_ext_lna1 {
		gpio-hog;
		gpios = <19 GPIO_ACTIVE_HIGH>;
		output-high;
		line-name = "tp-link:ext:lna1";
	};
};

&wmac {
	status = "okay";

	mtd-cal-data = <&art 0x1000>;

	nvmem-cells = <&macaddr_uboot_1fc00>;
	nvmem-cell-names = "mac-address";
};

&eth0 {
	status = "okay";

	phy-handle = <&swphy0>;

	nvmem-cells = <&macaddr_uboot_1fc00>;
	nvmem-cell-names = "mac-address";
	mac-address-increment = <1>;
};

&eth1 {
	status = "okay";

	nvmem-cells = <&macaddr_uboot_1fc00>;
	nvmem-cell-names = "mac-address";

	gmac-config {
		device = <&gmac>;
		switch-phy-swap = <1>;
	};
};

&uboot {
	compatible = "nvmem-cells";
	#address-cells = <1>;
	#size-cells = <1>;

	macaddr_uboot_1fc00: macaddr@1fc00 {
		reg = <0x1fc00 0x6>;
	};
};
