/dts-v1/;

#include "rtl839x.dtsi"

#include <dt-bindings/input/input.h>
#include <dt-bindings/gpio/gpio.h>

/ {
	compatible = "zyxel,gs1900-48", "realtek,rtl8393-soc";
	model = "Zyxel GS1900-48";

	aliases {
		led-boot = &led_sys;
		led-failsafe = &led_sys;
		led-running = &led_sys;
		led-upgrade = &led_sys;
	};

	memory@0 {
		device_type = "memory";
		reg = <0x0 0x8000000>;
	};

	leds {
		pinctrl-names = "default";
		pinctrl-0 = <&pinmux_disable_sys_led>;
		compatible = "gpio-leds";

		led_sys: sys {
			label = "green:sys";
			gpios = <&gpio0 0 GPIO_ACTIVE_HIGH>;
		};
	};

	gpio1: rtl8231-gpio {
		compatible = "realtek,rtl8231-gpio";
		#gpio-cells = <2>;
		indirect-access-bus-id = <3>;
		gpio-controller;
	};

	gpio-restart {
		compatible = "gpio-restart";
		gpios = <&gpio1 5 GPIO_ACTIVE_LOW>;
	};

	keys {
		compatible = "gpio-keys-polled";
		poll-interval = <20>;

		mode {
			label = "reset";
			gpios = <&gpio1 3 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};

	/* i2c of the left SFP cage: port 49 */
	i2c0: i2c-gpio-0 {
		compatible = "i2c-gpio";
		sda-gpios = <&gpio1 24 (GPIO_ACTIVE_HIGH | GPIO_OPEN_DRAIN)>;
		scl-gpios = <&gpio1 25 (GPIO_ACTIVE_HIGH | GPIO_OPEN_DRAIN)>;
		i2c-gpio,delay-us = <2>;
		#address-cells = <1>;
		#size-cells = <0>;
	};

	sfp0: sfp-p9 {
		compatible = "sff,sfp";
		i2c-bus = <&i2c0>;
		los-gpio = <&gpio1 27 GPIO_ACTIVE_HIGH>;
		tx-fault-gpio = <&gpio1 22 GPIO_ACTIVE_HIGH>;
		mod-def0-gpio = <&gpio1 26 GPIO_ACTIVE_LOW>;
		tx-disable-gpio = <&gpio1 23 GPIO_ACTIVE_HIGH>;
	};

	/* i2c of the right SFP cage: port 50 */
	i2c1: i2c-gpio-1 {
		compatible = "i2c-gpio";
		sda-gpios = <&gpio1 30 (GPIO_ACTIVE_HIGH | GPIO_OPEN_DRAIN)>;
		scl-gpios = <&gpio1 31 (GPIO_ACTIVE_HIGH | GPIO_OPEN_DRAIN)>;
		i2c-gpio,delay-us = <2>;
		#address-cells = <1>;
		#size-cells = <0>;
	};

	sfp1: sfp-p10 {
		compatible = "sff,sfp";
		i2c-bus = <&i2c1>;
		los-gpio = <&gpio1 33 GPIO_ACTIVE_HIGH>;
		tx-fault-gpio = <&gpio1 28 GPIO_ACTIVE_HIGH>;
		mod-def0-gpio = <&gpio1 32 GPIO_ACTIVE_LOW>;
		tx-disable-gpio = <&gpio1 29 GPIO_ACTIVE_HIGH>;
	};
};

&spi0 {
	status = "okay";
	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <10000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x0 0x40000>;
				read-only;
			};
			partition@40000 {
				label = "u-boot-env";
				reg = <0x40000 0x10000>;
				read-only;
			};
			partition@50000 {
				label = "u-boot-env2";
				reg = <0x50000 0x10000>;
				read-only;
			};
			partition@60000 {
				label = "jffs";
				reg = <0x60000 0x100000>;
			};
			partition@160000 {
				label = "jffs2";
				reg = <0x160000 0x100000>;
			};
			partition@260000 {
				label = "firmware";
				reg = <0x260000 0x6d0000>;
				compatible = "openwrt,uimage", "denx,uimage";
				openwrt,ih-magic = <0x83800000>;
			};
			partition@930000 {
				label = "runtime2";
				reg = <0x930000 0x6d0000>;
			};
		};
	};
};

&ethernet0 {
	mdio: mdio-bus {
		compatible = "realtek,rtl838x-mdio";
		regmap = <&ethernet0>;
		#address-cells = <1>;
		#size-cells = <0>;

		/* External phy RTL8218B #1 */
		EXTERNAL_PHY(0)
		EXTERNAL_PHY(1)
		EXTERNAL_PHY(2)
		EXTERNAL_PHY(3)
		EXTERNAL_PHY(4)
		EXTERNAL_PHY(5)
		EXTERNAL_PHY(6)
		EXTERNAL_PHY(7)

		/* External phy RTL8218B #2 */
		EXTERNAL_PHY(8)
		EXTERNAL_PHY(9)
		EXTERNAL_PHY(10)
		EXTERNAL_PHY(11)
		EXTERNAL_PHY(12)
		EXTERNAL_PHY(13)
		EXTERNAL_PHY(14)
		EXTERNAL_PHY(15)

		/* External phy RTL8218B #3 */
		EXTERNAL_PHY(16)
		EXTERNAL_PHY(17)
		EXTERNAL_PHY(18)
		EXTERNAL_PHY(19)
		EXTERNAL_PHY(20)
		EXTERNAL_PHY(21)
		EXTERNAL_PHY(22)
		EXTERNAL_PHY(23)

		/* External phy RTL8218B #4 */
		EXTERNAL_PHY(24)
		EXTERNAL_PHY(25)
		EXTERNAL_PHY(26)
		EXTERNAL_PHY(27)
		EXTERNAL_PHY(28)
		EXTERNAL_PHY(29)
		EXTERNAL_PHY(30)
		EXTERNAL_PHY(31)

		/* External phy RTL8218B #5 */
		EXTERNAL_PHY(32)
		EXTERNAL_PHY(33)
		EXTERNAL_PHY(34)
		EXTERNAL_PHY(35)
		EXTERNAL_PHY(36)
		EXTERNAL_PHY(37)
		EXTERNAL_PHY(38)
		EXTERNAL_PHY(39)

		/* External phy RTL8218B #6 */
		EXTERNAL_PHY(40)
		EXTERNAL_PHY(41)
		EXTERNAL_PHY(42)
		EXTERNAL_PHY(43)
		EXTERNAL_PHY(44)
		EXTERNAL_PHY(45)
		EXTERNAL_PHY(46)
		EXTERNAL_PHY(47)

		/* RTL8393 Internal SerDes */
		INTERNAL_PHY(48)
		INTERNAL_PHY(49)
	};
};

&switch0 {
	ports {
		#address-cells = <1>;
		#size-cells = <0>;

		SWITCH_PORT(0, 01, qsgmii)
		SWITCH_PORT(1, 02, qsgmii)
		SWITCH_PORT(2, 03, qsgmii)
		SWITCH_PORT(3, 04, qsgmii)
		SWITCH_PORT(4, 05, qsgmii)
		SWITCH_PORT(5, 06, qsgmii)
		SWITCH_PORT(6, 07, qsgmii)
		SWITCH_PORT(7, 08, qsgmii)

		SWITCH_PORT(8, 09, qsgmii)
		SWITCH_PORT(9, 10, qsgmii)
		SWITCH_PORT(10, 11, qsgmii)
		SWITCH_PORT(11, 12, qsgmii)
		SWITCH_PORT(12, 13, qsgmii)
		SWITCH_PORT(13, 14, qsgmii)
		SWITCH_PORT(14, 15, qsgmii)
		SWITCH_PORT(15, 16, qsgmii)

		SWITCH_PORT(16, 17, qsgmii)
		SWITCH_PORT(17, 18, qsgmii)
		SWITCH_PORT(18, 19, qsgmii)
		SWITCH_PORT(19, 20, qsgmii)
		SWITCH_PORT(20, 21, qsgmii)
		SWITCH_PORT(21, 22, qsgmii)
		SWITCH_PORT(22, 23, qsgmii)
		SWITCH_PORT(23, 24, qsgmii)

		SWITCH_PORT(24, 25, qsgmii)
		SWITCH_PORT(25, 26, qsgmii)
		SWITCH_PORT(26, 27, qsgmii)
		SWITCH_PORT(27, 28, qsgmii)
		SWITCH_PORT(28, 29, qsgmii)
		SWITCH_PORT(29, 30, qsgmii)
		SWITCH_PORT(30, 31, qsgmii)
		SWITCH_PORT(31, 32, qsgmii)

		SWITCH_PORT(32, 33, qsgmii)
		SWITCH_PORT(33, 34, qsgmii)
		SWITCH_PORT(34, 35, qsgmii)
		SWITCH_PORT(35, 36, qsgmii)
		SWITCH_PORT(36, 37, qsgmii)
		SWITCH_PORT(37, 38, qsgmii)
		SWITCH_PORT(38, 39, qsgmii)
		SWITCH_PORT(39, 40, qsgmii)

		SWITCH_PORT(40, 41, qsgmii)
		SWITCH_PORT(41, 42, qsgmii)
		SWITCH_PORT(42, 43, qsgmii)
		SWITCH_PORT(43, 44, qsgmii)
		SWITCH_PORT(44, 45, qsgmii)
		SWITCH_PORT(45, 46, qsgmii)
		SWITCH_PORT(46, 47, qsgmii)
		SWITCH_PORT(47, 48, qsgmii)

		/* SFP cages */
		port@48 {
			reg = <48>;
			label = "lan49";
			phy-mode = "sgmii";
			phy-handle = <&phy48>;
			sfp = <&sfp0>;

			fixed-link {
				speed = <1000>;
				full-duplex;
				pause;
			};

		};

		port@49 {
			reg = <49>;
			label = "lan50";
			phy-mode = "sgmii";
			phy-handle = <&phy49>;
			sfp = <&sfp1>;

			fixed-link {
				speed = <1000>;
				full-duplex;
				pause;
			};

		};

		/* CPU-Port */
		port@52 {
			ethernet = <&ethernet0>;
			reg = <52>;
			phy-mode = "qsgmii";
			fixed-link {
				speed = <1000>;
				full-duplex;
			};
		};
	};
};
