// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "mt7620a.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/mtd/partitions/uimage.h>

/ {
	compatible = "humax,e2", "ralink,mt7620a-soc";
	model = "HUMAX E2";

	aliases {
		led-boot = &led_power;
		led-failsafe = &led_power;
		led-running = &led_power;
		led-upgrade = &led_power;
		label-mac-device = &ethernet;
	};

	leds {
		compatible = "gpio-leds";

		led_power: power {
			label = "green:power";
			gpios = <&gpio1 3 GPIO_ACTIVE_LOW>;
		};

		pairing {
			label = "green:pairing";
			gpios = <&gpio1 8 GPIO_ACTIVE_LOW>;
		};

		wlan {
			label = "green:wlan";
			gpios = <&gpio1 9 GPIO_ACTIVE_LOW>;
		};

		lan {
			label = "green:lan";
			gpios = <&gpio1 4 GPIO_ACTIVE_LOW>;
		};

		wps {
			label = "green:wps";
			gpios = <&gpio1 5 GPIO_ACTIVE_LOW>;
		};
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			gpios = <&gpio1 1 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};
};

&gpio1 {
	status = "okay";
};

&spi0 {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <50000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x0 0x30000>;
				read-only;
			};

			partition@30000 {
				label = "u-boot-env";
				reg = <0x30000 0x10000>;
				read-only;
			};

			factory: partition@40000 {
				label = "factory";
				reg = <0x40000 0x30000>;
				read-only;

				compatible = "nvmem-cells";
				#address-cells = <1>;
				#size-cells = <1>;

				macaddr_factory_10007: macaddr@10007 {
					reg = <0x10007 0x6>;
				};
			};

			partition@70000 {
				compatible = "openwrt,uimage", "denx,uimage";
				openwrt,offset = <FW_EDIMAX_OFFSET>;
				openwrt,partition-magic = <FW_MAGIC_EDIMAX>;
				label = "firmware";
				reg = <0x70000 0x790000>;
			};
		};
	};
};

&ethernet {
	nvmem-cells = <&macaddr_factory_10007>;
	nvmem-cell-names = "mac-address";
};

&pcie {
	status = "okay";
};

&pcie0 {
	wifi@0,0 {
		compatible = "mediatek,mt76";
		reg = <0x0000 0 0 0 0>;
		mediatek,mtd-eeprom = <&factory 0x8000>;
		ieee80211-freq-limit = <5000000 6000000>;
	};
};

&wmac {
	ralink,mtd-eeprom = <&factory 0x0>;
};

&state_default {
	gpio {
		groups = "rgmii1";
		function = "gpio";
	};
};
