From 3ff26b29230c54fea2353b63124c589b61953e14 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <rafal@milecki.pl>
Date: Thu, 16 Sep 2021 14:03:53 +0200
Subject: [PATCH] net: dsa: b53: Improve flow control setup on BCM5301x
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

According to the Broadcom's reference driver flow control needs to be
enabled for any CPU switch port (5, 7 or 8 - depending on which one is
used). Current code makes it work only for the port 5. Use
dsa_is_cpu_port() which solved that problem.

Signed-off-by: Rafał Miłecki <rafal@milecki.pl>
Reviewed-by: Florian Fainelli <f.fainelli@gmail.com>
Tested-by: Florian Fainelli <f.fainelli@gmail.com>
Signed-off-by: Jakub Kicinski <kuba@kernel.org>
---
 drivers/net/dsa/b53/b53_common.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/net/dsa/b53/b53_common.c
+++ b/drivers/net/dsa/b53/b53_common.c
@@ -1226,7 +1226,7 @@ static void b53_adjust_link(struct dsa_s
 		return;
 
 	/* Enable flow control on BCM5301x's CPU port */
-	if (is5301x(dev) && port == dev->cpu_port)
+	if (is5301x(dev) && dsa_is_cpu_port(ds, port))
 		tx_pause = rx_pause = true;
 
 	if (phydev->pause) {
