// SPDX-License-Identifier: GPL-2.0-or-later

#include "qcom-ipq8065-smb208.dtsi"
#include <dt-bindings/input/input.h>

/ {
	model = "Askey RT4230W REV6";
	compatible = "askey,rt4230w-rev6", "qcom,ipq8065", "qcom,ipq8064";

	memory@0 {
		reg = <0x42000000 0x3e000000>;
		device_type = "memory";
	};

	aliases {
		led-boot = &ledctrl1;
		led-failsafe = &ledctrl1;
		led-running = &ledctrl3;
		led-upgrade = &ledctrl1;
	};

	chosen {
		bootargs = "rootfstype=squashfs noinitrd";
	};

	keys {
		compatible = "gpio-keys";
		pinctrl-0 = <&button_pins>;
		pinctrl-names = "default";

		reset {
			label = "reset";
			gpios = <&qcom_pinmux 54 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};

		wps {
			label = "wps";
			gpios = <&qcom_pinmux 68 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
		};
	};

	leds {
		compatible = "gpio-leds";
		pinctrl-0 = <&led_pins>;
		pinctrl-names = "default";

		ledctrl1: ledctrl1 {
			label = "ledctrl1";
			gpios = <&qcom_pinmux 22 GPIO_ACTIVE_HIGH>;
		};

		ledctrl2: ledctrl2 {
			label = "ledctrl2";
			gpios = <&qcom_pinmux 23 GPIO_ACTIVE_HIGH>;
			linux,default-trigger = "default-on";
		};

		ledctrl3: ledctrl3 {
			label = "ledctrl3";
			gpios = <&qcom_pinmux 24 GPIO_ACTIVE_HIGH>;
		};
	};
};

&qcom_pinmux {
	button_pins: button_pins {
		mux {
			pins = "gpio54", "gpio68";
			function = "gpio";
			drive-strength = <2>;
			bias-pull-up;
		};
	};

	led_pins: led_pins {
		mux {
			pins = "gpio22", "gpio23", "gpio24";
			function = "gpio";
			drive-strength = <2>;
			bias-pull-down;
		};
	};

	rgmii2_pins: rgmii2-pins {
		mux {
			pins = "gpio27", "gpio28", "gpio29", "gpio30", "gpio31",
				"gpio51", "gpio52", "gpio59", "gpio60", "gpio61", "gpio62";
			function = "rgmii2";
			drive-strength = <8>;
			bias-disable;
		};

		tx {
			pins = "gpio27", "gpio28", "gpio29", "gpio30", "gpio31", "gpio32";
			input-disable;
		};
	};

	spi_pins: spi_pins {
		cs {
			pins = "gpio20";
			drive-strength = <12>;
		};
	};
};

&gsbi5 {
	qcom,mode = <GSBI_PROT_SPI>;
	status = "okay";

	spi@1a280000 {
		status = "okay";

		pinctrl-0 = <&spi_pins>;
		pinctrl-names = "default";

		cs-gpios = <&qcom_pinmux 20 GPIO_ACTIVE_HIGH>;

		flash@0 {
			compatible = "everspin,mr25h256";
			#address-cells = <1>;
			#size-cells = <1>;
			spi-max-frequency = <40000000>;
			reg = <0>;
		};
	};
};

&nand {
	status = "okay";

	nand@0 {
		reg = <0>;
		compatible = "qcom,nandcs";

		nand-ecc-strength = <4>;
		nand-bus-width = <8>;
		nand-ecc-step-size = <512>;

		qcom,boot-partitions = <0x0 0x1180000 0x1340000 0x10c0000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "0:SBL1";
				reg = <0x0000000 0x0040000>;
				read-only;
			};

			partition@40000 {
				label = "0:MIBIB";
				reg = <0x0040000 0x0140000>;
				read-only;
			};

			partition@180000 {
				label = "0:SBL2";
				reg = <0x0180000 0x0140000>;
				read-only;
			};

			partition@2c0000 {
				label = "0:SBL3";
				reg = <0x02c0000 0x0280000>;
				read-only;
			};

			partition@540000 {
				label = "0:DDRCONFIG";
				reg = <0x0540000 0x0120000>;
				read-only;
			};

			partition@660000 {
				label = "0:SSD";
				reg = <0x0660000 0x0120000>;
				read-only;
			};

			partition@780000 {
				label = "0:TZ";
				reg = <0x0780000 0x0280000>;
				read-only;
			};

			partition@a00000 {
				label = "0:RPM";
				reg = <0x0a00000 0x0280000>;
				read-only;
			};

			partition@c80000 {
				label = "0:APPSBL";
				reg = <0x0c80000 0x0500000>;
				read-only;
			};

			partition@1180000 {
				label = "0:APPSBLENV";
				reg = <0x1180000 0x0080000>;
			};

			partition@1200000 {
				label = "0:ART";
				reg = <0x1200000 0x0140000>;
				read-only;
				compatible = "nvmem-cells";
				#address-cells = <1>;
				#size-cells = <1>;

				macaddr_ART_0: macaddr@0 {
					reg = <0x0 0x6>;
				};

				macaddr_ART_6: macaddr@6 {
					reg = <0x6 0x6>;
				};

				precal_ART_1000: precal@1000 {
					reg = <0x1000 0x2f20>;
				};

				precal_ART_5000: precal@5000 {
					reg = <0x5000 0x2f20>;
				};
			};

			partition@1340000 {
				label = "0:BOOTCONFIG";
				reg = <0x1340000 0x0060000>;
				read-only;
			};

			partition@13a0000 {
				label = "0:SBL2_1";
				reg = <0x13a0000 0x0140000>;
				read-only;
			};

			partition@14e0000 {
				label = "0:SBL3_1";
				reg = <0x14e0000 0x0280000>;
				read-only;
			};

			partition@1760000 {
				label = "0:DDRCONFIG_1";
				reg = <0x1760000 0x0120000>;
				read-only;
			};

			partition@1880000 {
				label = "0:SSD_1";
				reg = <0x1880000 0x0120000>;
				read-only;
			};

			partition@19a0000 {
				label = "0:TZ_1";
				reg = <0x19a0000 0x0280000>;
				read-only;
			};

			partition@1c20000 {
				label = "0:RPM_1";
				reg = <0x1c20000 0x0280000>;
				read-only;
			};

			partition@1ea0000 {
				label = "0:BOOTCONFIG1";
				reg = <0x1ea0000 0x0060000>;
				read-only;
			};

			partition@1f00000 {
				label = "0:APPSBL_1";
				reg = <0x1f00000 0x0500000>;
				read-only;
			};

			partition@2400000 {
				label = "ubi";
				reg = <0x2400000 0x1a000000>;
			};
		};
	};
};

&mdio0 {
	status = "okay";

	pinctrl-0 = <&mdio0_pins>;
	pinctrl-names = "default";

	phy0: ethernet-phy@0 {
		reg = <0x0>;
		qca,ar8327-initvals = <
			0x00004 0x7600000   /* PAD0_MODE */
			0x00008 0x1000000   /* PAD5_MODE */
			0x0000c 0x80        /* PAD6_MODE */
			0x000e4 0xaa545     /* MAC_POWER_SEL */
			0x000e0 0xc74164de  /* SGMII_CTRL */
			0x0007c 0x4e        /* PORT0_STATUS */
			0x00094 0x4e        /* PORT6_STATUS */
			0x00050 0xcf02cf02  /* LED_CTRL_0 */
			0x00054 0xc832c832  /* LED_CTRL_1 */
			>;
	};
};

&gmac0 {
	status = "okay";
	phy-mode = "rgmii";
	qcom,id = <0>;

	nvmem-cells = <&macaddr_ART_0>;
	nvmem-cell-names = "mac-address";

	pinctrl-0 = <&rgmii2_pins>;
	pinctrl-names = "default";

	fixed-link {
		speed = <1000>;
		full-duplex;
	};
};

&gmac1 {
	status = "okay";
	phy-mode = "sgmii";
	qcom,id = <1>;

	nvmem-cells = <&macaddr_ART_6>;
	nvmem-cell-names = "mac-address";

	fixed-link {
		speed = <1000>;
		full-duplex;
	};
};

&adm_dma {
	status = "okay";
};

&hs_phy_0 {
	status = "okay";
};

&ss_phy_0 {
	status = "okay";
};

&usb3_0 {
	status = "okay";
};

&hs_phy_1 {
	status = "okay";
};

&ss_phy_1 {
	status = "okay";
};

&usb3_1 {
	status = "okay";
};

&pcie0 {
	status = "okay";
	reset-gpio = <&qcom_pinmux 3 GPIO_ACTIVE_HIGH>;
	pinctrl-0 = <&pcie0_pins>;
	pinctrl-names = "default";

	bridge@0,0 {
		reg = <0x00000000 0 0 0 0>;
		#address-cells = <3>;
		#size-cells = <2>;
		ranges;

		wifi0: wifi@1,0 {
			compatible = "pci168c,0046";
			reg = <0x00010000 0 0 0 0>;

			nvmem-cells = <&precal_ART_1000>;
			nvmem-cell-names = "pre-calibration";
		};
	};
};

&pcie1 {
	status = "okay";
	reset-gpio = <&qcom_pinmux 48 GPIO_ACTIVE_HIGH>;
	pinctrl-0 = <&pcie1_pins>;
	pinctrl-names = "default";
	max-link-speed = <1>;

	bridge@0,0 {
		reg = <0x00000000 0 0 0 0>;
		#address-cells = <3>;
		#size-cells = <2>;
		ranges;

		wifi1: wifi@1,0 {
			compatible = "pci168c,0046";
			reg = <0x00010000 0 0 0 0>;

			nvmem-cells = <&precal_ART_5000>;
			nvmem-cell-names = "pre-calibration";
		};
	};
};
