// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "qca955x_senao_loader.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "engenius,ews660ap", "qca,qca9558";
	model = "EnGenius EWS660AP";

	aliases {
		label-mac-device = &eth0;
		led-boot = &led_wifi5g;
		led-failsafe = &led_wifi5g;
		led-upgrade = &led_wifi5g;
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			gpios = <&gpio 21 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
			linux,code = <KEY_RESTART>;
		};
	};

	leds {
		compatible = "gpio-leds";

		wifi2g {
			label = "green:wifi2g";
			gpios = <&gpio 14 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy1tpt";
		};

		led_wifi5g: wifi5g {
			label = "green:wifi5g";
			gpios = <&gpio 15 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0tpt";
		};
	};
};

&partitions {
	partition@ff0000 {
		label = "art";
		reg = <0xff0000 0x010000>;
		read-only;

		compatible = "nvmem-cells";
		#address-cells = <1>;
		#size-cells = <1>;

		macaddr_art_0: macaddr@0 {
			reg = <0x0 0x6>;
		};

		calibration_art_1000: calibration@1000 {
			reg = <0x1000 0x440>;
		};

		calibration_art_5000: calibration@5000 {
			reg = <0x5000 0x844>;
		};
	};
};

&mdio0 {
	status = "okay";

	phy1: ethernet-phy@1 {
		reg = <1>;
		eee-broken-100tx;
		eee-broken-1000t;
	};

	phy2: ethernet-phy@2 {
		reg = <2>;
		eee-broken-100tx;
		eee-broken-1000t;
		at803x-override-sgmii-link-check;
	};
};

&eth0 {
	status = "okay";

	nvmem-cells = <&macaddr_art_0>;
	nvmem-cell-names = "mac-address";

	phy-handle = <&phy1>;
	phy-mode = "rgmii-id";

	pll-data = <0x82000000 0x80000101 0x80001313>;
};

&eth1 {
	status = "okay";

	nvmem-cells = <&macaddr_art_0>;
	nvmem-cell-names = "mac-address";
	mac-address-increment = <1>;

	phy-handle = <&phy2>;

	pll-data = <0x03000000 0x00000101 0x00001313>;

	qca955x-sgmii-fixup;
};

&wmac {
	status = "okay";

	nvmem-cells = <&macaddr_art_0>, <&calibration_art_1000>;
	nvmem-cell-names = "mac-address", "calibration";
	mac-address-increment = <2>;
};

&ath10k_1 {
	status = "okay";

	nvmem-cells = <&macaddr_art_0>, <&calibration_art_5000>;
	nvmem-cell-names = "mac-address", "calibration";
	mac-address-increment = <3>;
};

&pcie1 {
	status = "okay";
};
