// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "mt7621.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>

/ {
	compatible = "rostelecom,rt-fe-1a", "mediatek,mt7621-soc";
	model = "Rostelecom RT-FE-1A";

	aliases {
		label-mac-device = &gmac0;

		led-boot = &led_status_green;
		led-failsafe = &led_status_green;
		led-running = &led_status_green;
		led-upgrade = &led_status_green;
	};

	leds {
		compatible = "gpio-leds";

		led-0 {
			color = <LED_COLOR_ID_BLUE>;
			function = LED_FUNCTION_WLAN;
			function-enumerator = <50>;
			gpios = <&gpio 7 GPIO_ACTIVE_HIGH>;
			linux,default-trigger = "phy1tpt";
		};

		led-1 {
			color = <LED_COLOR_ID_BLUE>;
			function = LED_FUNCTION_WLAN;
			function-enumerator = <24>;
			gpios = <&gpio 12 GPIO_ACTIVE_HIGH>;
			linux,default-trigger = "phy0tpt";
		};

		led_status_green: led-2 {
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_STATUS;
			gpios = <&gpio 18 GPIO_ACTIVE_LOW>;
		};
	};

	keys {
		compatible = "gpio-keys";

		button-0 {
			label = "wps";
			gpios = <&gpio 11 GPIO_ACTIVE_HIGH>;
			linux,code = <KEY_WPS_BUTTON>;
		};

		button-1 {
			label = "reset";
			gpios = <&gpio 14 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};

	ubi-concat {
		compatible = "mtd-concat";
		devices = <&ubiconcat0 &ubiconcat1 &ubiconcat2 \
			   &ubiconcat3>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "ubi";
				reg = <0x0 0x5420000>;
			};
		};
	};
};

&nand {
	status = "okay";

	partitions {
		compatible = "sercomm,sc-partitions", "fixed-partitions";
		#address-cells = <1>;
		#size-cells = <1>;

		partition@0 {
			label = "u-boot";
			reg = <0x0 0x100000>;
			sercomm,scpart-id = <0>;
			read-only;
		};

		partition@100000 {
			label = "dynamic partition map";
			reg = <0x100000 0x100000>;
			sercomm,scpart-id = <1>;
			read-only;
		};

		partition@200000 {
			label = "Factory";
			reg = <0x200000 0x100000>;
			sercomm,scpart-id = <2>;
			read-only;

			nvmem-layout {
				compatible = "fixed-layout";
				#address-cells = <1>;
				#size-cells = <1>;

				eeprom_2g: eeprom@0 {
					reg = <0x0 0x400>;
				};

				eeprom_5g: eeprom@8000 {
					reg = <0x8000 0x4da8>;
				};

				macaddr_label: macaddr@21000 {
					compatible = "mac-base";
					reg = <0x21000 0x6>;
					#nvmem-cell-cells = <1>;
				};
			};
		};

		partition@300000 {
			label = "Boot Flag";
			reg = <0x300000 0x100000>;
			sercomm,scpart-id = <3>;
		};

		partition@400000 {
			label = "kernel";
			reg = <0x400000 0x600000>;
			sercomm,scpart-id = <4>;
		};

		partition@a00000 {
			label = "Kernel 2";
			reg = <0xa00000 0x600000>;
			sercomm,scpart-id = <5>;
			read-only;
		};

		ubiconcat0: partition@1000000 {
			label = "File System 1";
			reg = <0x1000000 0x1800000>;
			sercomm,scpart-id = <6>;
		};

		partition@2800000 {
			label = "File System 2";
			reg = <0x2800000 0x1800000>;
			sercomm,scpart-id = <7>;
			read-only;
		};

		ubiconcat1: partition@4000000 {
			label = "Configuration/log";
			reg = <0x4000000 0x800000>;
			sercomm,scpart-id = <8>;
		};

		ubiconcat2: partition@4800000 {
			label = "application tmp buffer (Ftool)";
			reg = <0x4800000 0xc00000>;
			sercomm,scpart-id = <9>;
		};

		ubiconcat3: partition@5400000 {
			label = "free space (in stock firmware)";
			reg = <0x5400000 0x2820000>;
			sercomm,scpart-id = <10>;
		};
	};
};

&pcie {
	status = "okay";
};

&pcie0 {
	wifi@0,0 {
		compatible = "mediatek,mt76";
		reg = <0x0000 0 0 0 0>;
		ieee80211-freq-limit = <5000000 6000000>;

		nvmem-cells = <&eeprom_5g>, <&macaddr_label 3>;
		nvmem-cell-names = "eeprom", "mac-address";

		led {
			led-active-low;
		};
	};
};

&pcie1 {
	wifi@0,0 {
		compatible = "mediatek,mt76";
		reg = <0x0000 0 0 0 0>;
		ieee80211-freq-limit = <2400000 2500000>;

		nvmem-cells = <&eeprom_2g>, <&macaddr_label 2>;
		nvmem-cell-names = "eeprom", "mac-address";

		led {
			led-active-low;
		};
	};
};

&gmac0 {
	nvmem-cells = <&macaddr_label 0>;
	nvmem-cell-names = "mac-address";
};

&gmac1 {
	status = "okay";
	label = "wan";
	phy-handle = <&ethphy0>;

	nvmem-cells = <&macaddr_label 11>;
	nvmem-cell-names = "mac-address";
};

&mdio {
	ethphy0: ethernet-phy@0 {
		reg = <0>;
	};
};

&switch0 {
	ports {
		port@1 {
			status = "okay";
			label = "lan1";
		};

		port@2 {
			status = "okay";
			label = "lan2";
		};

		port@3 {
			status = "okay";
			label = "lan3";
		};

		port@4 {
			status = "okay";
			label = "lan4";
		};
	};
};

&state_default {
	gpio {
		groups = "jtag", "uart2", "uart3", "wdt";
		function = "gpio";
	};
};
