// SPDX-License-Identifier: GPL-2.0-or-later or MIT

#include <dt-bindings/input/input.h>
#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/leds/common.h>

/include/ "fsl/p1020si-pre.dtsi"
/ {
	model = "Hewlett-Packard MSM460";
	compatible = "hpe,msm460";

	aliases {
		led-boot = &system_green;
		led-failsafe = &system_green;
		led-running = &system_green;
		led-upgrade = &system_green;
		label-mac-device = &enet0;
	};

	chosen {
		/* Needed for initramfs */
		bootargs-override = "console=ttyS0,115200 ubi.mtd=5,2048";
		stdout-path = &serial0;
	};

	memory {
		device_type = "memory";
	};

	lbc: localbus@ffe05000 {
		reg = <0 0xffe05000 0 0x1000>;
		ranges = <0x0 0x0 0x0 0xec000000 0x04000000
			  0x1 0x0 0x0 0xff800000 0x00040000
			  0x2 0x0 0x0 0xffa00000 0x00020000
			  0x3 0x0 0x0 0xffb00000 0x00020000>;

		nand@1,0 {
			compatible = "fsl,p1020-fcm-nand", "fsl,elbc-fcm-nand";
			reg = <0x1 0x0 0x40000>;

			partitions {
				compatible = "fixed-partitions";
				#address-cells = <1>;
				#size-cells = <1>;

				partition@0 {
					reg = <0x0 0xc0000>;
					label = "u-boot";
					read-only;
				};

				partition@c0000 {
					reg = <0xc0000 0x40000>;
					label = "colubris-bid";
					read-only;

					nvmem-layout {
						compatible = "fixed-layout";
						#address-cells = <1>;
						#size-cells = <1>;

						macaddr_hwinfo_1f822: macaddr@1f822 {
							/* ETH */
							compatible = "mac-base";
							reg = <0x1f822 0x6>;
							#nvmem-cell-cells = <1>;
						};

						macaddr_hwinfo_1f9bd: macaddr@1f9bd {
							/* WLAN */
							compatible = "mac-base";
							reg = <0x1f9bd 0x6>;
							#nvmem-cell-cells = <1>;
						};
					};
				};

				/* uenv{0,1} and ubi occupy kernel and slash partitions */

				partition@100000 {
					reg = <0x100000 0x80000>;
					label = "uboot-env0";
				};

				partition@180000 {
					reg = <0x180000 0x80000>;
					label = "uboot-env1";
				};

				partition@200000 {
					reg = <0x200000 0x300000>;
					label = "reserved";
				};

				partition@500000 {
					reg = <0x500000 0x5f00000>;
					label = "ubi";
				};

				partition@6500000 {
					reg = <0x6500000 0x400000>;
					label = "pool";
					read-only;
				};

				partition@6900000 {
					reg = <0x6900000 0x15e0000>;
					label = "flash";
					read-only;
				};

				partition@7ee0000 {
					reg = <0x7ee0000 0x20000>;
					label = "pf";
					read-only;
				};

				/* BBT is at the end of the flash - 100000@7f00000 */
			};
		};
	};

	soc: soc@ffe00000 {
		ranges = <0x0 0x0 0xffe00000 0x100000>;

		i2c@3000 {
			status = "disabled";
		};

		gpio0: gpio-controller@fc00 {
		};

		mdio@24000 {
			phy0: ethernet-phy@0 {
				reg = <0x0>;
				reset-gpios = <&gpio0 4 GPIO_ACTIVE_LOW>;
				reset-assert-us = <10000>;
				reset-deassert-us = <10000>;
			};
		};

		enet0: ethernet@b0000 {
			phy-connection-type = "rgmii-id";
			phy-handle = <&phy0>;
			nvmem-cells = <&macaddr_hwinfo_1f822 0>;
			nvmem-cell-names = "mac-address";
		};

		enet1: ethernet@b1000 {
			status = "disabled";
		};

		enet2: ethernet@b2000 {
			status = "disabled";
		};

		usb@22000 {
			status = "disabled";
		};

		usb@23000 {
			status = "disabled";
		};
	};

	pci0: pcie@ffe09000 {
		ranges = <0x2000000 0x0 0xa0000000 0 0xa0000000 0x0 0x20000000
			  0x1000000 0x0 0x00000000 0 0xffc10000 0x0 0x10000>;
		reg = <0 0xffe09000 0 0x1000>;
		pcie@0 {
			ranges = <0x2000000 0x0 0xa0000000
				  0x2000000 0x0 0xa0000000
				  0x0 0x20000000

				  0x1000000 0x0 0x0
				  0x1000000 0x0 0x0
				  0x0 0x100000>;
		};
	};

	pci1: pcie@ffe0a000 {
		reg = <0 0xffe0a000 0 0x1000>;
		ranges = <0x2000000 0x0 0x80000000 0 0x80000000 0x0 0x20000000
			  0x1000000 0x0 0x00000000 0 0xffc00000 0x0 0x10000>;
		pcie@0 {
			ranges = <0x2000000 0x0 0x80000000
				  0x2000000 0x0 0x80000000
				  0x0 0x20000000

				  0x1000000 0x0 0x0
				  0x1000000 0x0 0x0
				  0x0 0x100000>;
		};
	};

	leds {
		compatible = "gpio-leds";

		system_green: power {
			gpios = <&gpio0 0 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_POWER;
			default-state = "on";
		};

		lan {
			gpios = <&gpio0 1 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_LAN;
		};

		radio1 {
			gpios = <&gpio0 2 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_WLAN;
			function-enumerator = <1>;
			linux,default-trigger = "phy0tpt";
		};

		radio2 {
			gpios = <&gpio0 3 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_WLAN;
			function-enumerator = <2>;
			linux,default-trigger = "phy1tpt";
		};
	};

	buttons {
		compatible = "gpio-keys";

		reset {
			label = "reset-btn";
			gpios = <&gpio0 5 GPIO_ACTIVE_HIGH>;
			linux,code = <KEY_RESTART>;
		};
	};
};
/include/ "fsl/p1020si-post.dtsi"
