From 20c9da8c7bab3bbc18e42ee0b2659c4b43aabad7 Mon Sep 17 00:00:00 2001
From: Joshua Emele <jemele@acm.org>
Date: Wed, 7 Nov 2018 16:07:40 -0800
Subject: [PATCH] lan78xx: Debounce link events to minimize poll storm

The bInterval is set to 4 (i.e. 8 microframes => 1ms) and the only bit
that the driver pays attention to is "link was reset". If there's a
flapping status bit in that endpoint data, (such as if PHY negotiation
needs a few tries to get a stable link) then polling at a slower rate
would act as a de-bounce.

See: https://github.com/raspberrypi/linux/issues/2447
---
 drivers/net/usb/lan78xx.c | 12 +++++++++++-
 1 file changed, 11 insertions(+), 1 deletion(-)
--- a/drivers/net/usb/lan78xx.c
+++ b/drivers/net/usb/lan78xx.c
@@ -434,6 +434,11 @@ static bool enable_tso;
 module_param(enable_tso, bool, 0644);
 MODULE_PARM_DESC(enable_tso, "Enables TCP segmentation offload");
 
+#define INT_URB_MICROFRAMES_PER_MS	8
+static int int_urb_interval_ms = 8;
+module_param(int_urb_interval_ms, int, 0);
+MODULE_PARM_DESC(int_urb_interval_ms, "Override usb interrupt urb interval");
+
 static int lan78xx_read_reg(struct lan78xx_net *dev, u32 index, u32 *data)
 {
 	u32 *buf = kmalloc(sizeof(u32), GFP_KERNEL);
@@ -3768,7 +3773,12 @@ static int lan78xx_probe(struct usb_inte
 	netdev->max_mtu = MAX_SINGLE_PACKET_SIZE;
 	netif_set_gso_max_size(netdev, MAX_SINGLE_PACKET_SIZE - MAX_HEADER);
 
-	period = ep_intr->desc.bInterval;
+	if (int_urb_interval_ms <= 0)
+		period = ep_intr->desc.bInterval;
+	else
+		period = int_urb_interval_ms * INT_URB_MICROFRAMES_PER_MS;
+
+	netif_notice(dev, probe, netdev, "int urb period %d\n", period);
 	maxp = usb_maxpacket(dev->udev, dev->pipe_intr, 0);
 	buf = kmalloc(maxp, GFP_KERNEL);
 	if (buf) {
