/* This file is released into the public domain */

#include "mt7620a_netgear_ex2700_wn3000rp-v3.dtsi"

/ {
	compatible = "netgear,wn3000rp-v3", "ralink,mt7620a-soc";
	model = "Netgear WN3000RP v3";

	aliases {
		led-boot = &led_power_green;
		led-failsafe = &led_power_green;
		led-running = &led_power_green;
		led-upgrade = &led_power_green;
	};

	leds {
		compatible = "gpio-leds";

		led_power_green: power_g {
			label = "green:power";
			gpios = <&gpio0 9 GPIO_ACTIVE_LOW>;
			default-state = "on";
		};

		power_r {
			label = "red:power";
			gpios = <&gpio0 11 GPIO_ACTIVE_LOW>;
		};

		client_g {
			label = "green:client";
			gpios = <&gpio0 13 GPIO_ACTIVE_LOW>;
		};

		client_r {
			label = "red:client";
			gpios = <&gpio0 10 GPIO_ACTIVE_LOW>;
		};

		router_g {
			label = "green:router";
			gpios = <&gpio0 12 GPIO_ACTIVE_LOW>;
		};

		router_r {
			label = "red:router";
			gpios = <&gpio0 14 GPIO_ACTIVE_LOW>;
		};

		wps {
			label = "green:wps";
			gpios = <&gpio1 15 GPIO_ACTIVE_LOW>;
		};

		l_arrow {
			label = "blue:leftarrow";
			gpios = <&gpio0 7 GPIO_ACTIVE_LOW>;
		};

		r_arrow {
			label = "blue:rightarrow";
			gpios = <&gpio0 8 GPIO_ACTIVE_LOW>;
		};
	};
};

&partitions {
	partition@0 {
		label = "u-boot";
		reg = <0x0 0x30000>;
		read-only;
	};

	partition@30000 {
		label = "u-boot-env";
		reg = <0x30000 0x10000>;
		read-only;
	};

	partition@40000 {
		compatible = "denx,uimage";
		label = "firmware";
		reg = <0x40000 0x7b0000>;
	};

	art: partition@7f0000 {
		label = "art";
		reg = <0x7f0000 0x10000>;
		read-only;
	};
};
