#!/bin/sh
# SPDX-License-Identifier: GPL-2.0 OR BSD-2-Clause

. /lib/functions/system.sh
. /lib/functions/uci-defaults.sh

bcm4908_setup_interfaces()
{
	local board="$1"

	case "$board" in
	asus,gt-ac5300)
		ucidef_set_interface_lan "lan1 lan2 lan5 lan6 sw"
		;;
	*)
		ucidef_set_interfaces_lan_wan "lan1 lan2 lan3 lan4" "wan"
		;;
	esac
}

board_config_update
board=$(board_name)
bcm4908_setup_interfaces "$board"
board_config_flush

exit 0
