#include "danube.dtsi"

#include <dt-bindings/input/input.h>

/ {
	compatible = "arcadyan,arv752dpw", "lantiq,xway", "lantiq,danube";
	model = "Arcor 802";

	chosen {
		bootargs = "console=ttyLTQ0,115200";
	};

	aliases {
		led-boot = &power_red;
		led-failsafe = &power_blue;
		led-running = &power_red;
		led-upgrade = &power_red;

		led-dsl = &internet_red;
		led-usb = &umts;
		led-wifi = &wifi;

		label-mac-device = &wifi0;
	};

	memory@0 {
		device_type = "memory";
		reg = <0x0 0x4000000>;
	};

	keys {
		compatible = "gpio-keys-polled";
		poll-interval = <100>;

		wps {
			label = "wps";
			gpios = <&gpio 11 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
		};
		restart {
			label = "restart";
			gpios = <&gpio 12 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_POWER>;
		};
		dsl {
			label = "dsl";
			gpios = <&gpio 13 GPIO_ACTIVE_LOW>;
			linux,code = <BTN_0>;
		};
		reset {
			label = "reset";
			gpios = <&gpio 30 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};

	leds {
		compatible = "gpio-leds";
		power_blue: power1 {
			label = "blue:power";
			gpios = <&gpio 3 GPIO_ACTIVE_LOW>;
		};
		internet_red: internet {
			label = "red:internet";
			gpios = <&gpio 4 GPIO_ACTIVE_LOW>;
		};
		message {
			label = "red:message";
			gpios = <&gpio 5 GPIO_ACTIVE_LOW>;
		};
		power_red: power {
			label = "red:power";
			gpios = <&gpio 6 GPIO_ACTIVE_LOW>;
			default-state = "keep";
		};
		voice1 {
			label = "red:voice";
			gpios = <&gpio 8 GPIO_ACTIVE_LOW>;
		};
		umts: umts {
			label = "red:umts";
			gpios = <&gpiomm 3 GPIO_ACTIVE_LOW>;
		};
		wifi: wifi {
			label = "red:wifi";
			gpios = <&gpiomm 4 GPIO_ACTIVE_LOW>;
		};
		fxs1 {
			label = "green:tae-n";
			gpios = <&gpiomm 5 GPIO_ACTIVE_LOW>;
		};
		fxs2 {
			label = "green:tae-u";
			gpios = <&gpiomm 6 GPIO_ACTIVE_LOW>;
		};
		fxo {
			label = "green:isdn";
			gpios = <&gpiomm 7 GPIO_ACTIVE_LOW>;
		};
		internet2 {
			label = "blue:internet";
			gpios = <&gpiomm 8 GPIO_ACTIVE_LOW>;
		};
		voice2 {
			label = "blue:voice";
			gpios = <&gpiomm 9 GPIO_ACTIVE_LOW>;
		};
	};

	usb_vbus: regulator-usb-vbus {
		compatible = "regulator-fixed";

		regulator-name = "USB_VBUS";

		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;

		gpio = <&gpiomm 0 GPIO_ACTIVE_HIGH>;
		enable-active-high;
	};
};

&gpio {
	pinctrl-names = "default";
	pinctrl-0 = <&state_default>;

	state_default: pinmux {
		ebu {
			lantiq,groups = "ebu cs1";
			lantiq,function = "ebu";
		};
		exin {
			lantiq,groups = "exin1";
			lantiq,function = "exin";
			lantiq,pull = <2>;
			lantiq,output = <0>;
		};
		pci_rst {
			lantiq,pins = "io21";
			lantiq,pull = <2>;
			lantiq,output = <1>;
		};
		leds {
			lantiq,pins = "io3", "io5", "io6", "io8";
			lantiq,output = <1>;
			lantiq,pull = <0>;
		};
		keys {
			lantiq,pins = "io11", "io12", "io13", "io28";
			lantiq,output = <0>;
			lantiq,pull = <2>;
			lantiq,open-drain = <1>;
		};
	};
};

&gsw {
	phy-mode = "rmii";
	mtd-mac-address = <&boardconfig 0x16>;
};

&localbus {
	flash@0 {
		compatible = "lantiq,nor";
		bank-width = <2>;
		reg = <0 0x0 0x800000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "uboot";
				reg = <0x00000 0x10000>;
				read-only;
			};

			partition@10000 {
				label = "u-boot-env";
				reg = <0x10000 0x10000>;
				read-only;
			};

			partition@20000 {
				label = "firmware";
				reg = <0x20000 0x7d0000>;
			};

			boardconfig: partition@7f0000 {
				label = "board_config";
				reg = <0x7f0000 0x10000>;
				read-only;
			};
		};
	};

	gpiomm: gpio@1 {
		compatible = "lantiq,gpio-mm";
		reg = <1 0x0 0x10 >;
		#address-cells = <1>;
		#size-cells = <1>;
		#gpio-cells = <2>;
		gpio-controller;
		lantiq,shadow = <0x3>;
	};
};

&pci0 {
	status = "okay";

	pinctrl-0 = <&pci_gnt1_pins>, <&pci_req1_pins>, <&pci_req2_pins>;
	pinctrl-names = "default";

	lantiq,external-clock;
	gpio-reset = <&gpio 21 GPIO_ACTIVE_HIGH>;
	interrupt-map = <0x7000 0 0 1 &icu0 135>;
	req-mask = <0x3>;

	wifi0: wifi@1814,0601 {
		compatible = "pci1814,0601";
		reg = <0x7000 0 0 0 0>;
		mtd-mac-address = <&boardconfig 0x16>;
		ralink,mtd-eeprom = <&boardconfig 0x410>;
		ralink,mtd-eeprom-swap;
	};
};

&usb_phy {
	status = "okay";
};

&usb {
	status = "okay";
	vbus-supply = <&usb_vbus>;
};

&vmmc {
	status = "okay";
	gpios = <&gpiomm 1 GPIO_ACTIVE_HIGH>;
};
