From 1cf854cd3531b10168b8f9aeb93bb0ab4b9a9003 Mon Sep 17 00:00:00 2001
From: MikeDK <m.kaplan@evva.com>
Date: Sun, 26 Jan 2020 23:33:54 +0100
Subject: [PATCH] Fix i2c-pwm-pca9685a overlay

---
 arch/arm/boot/dts/overlays/i2c-pwm-pca9685a-overlay.dts | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/arch/arm/boot/dts/overlays/i2c-pwm-pca9685a-overlay.dts
+++ b/arch/arm/boot/dts/overlays/i2c-pwm-pca9685a-overlay.dts
@@ -13,7 +13,7 @@
 			status = "okay";
 
 			pca: pca@40 {
-				compatible = "nxp,pca9685";
+				compatible = "nxp,pca9685-pwm";
 				#pwm-cells = <2>;
 				reg = <0x40>;
 				status = "okay";
