From d05cf625f27335320a2ad883b7f7c4cd638dca99 Mon Sep 17 00:00:00 2001
From: Yuantian Tang <andy.tang@nxp.com>
Date: Mon, 5 Nov 2018 17:25:32 +0800
Subject: [PATCH] arm64: dts: nxp: ls208xa: add more thermal zone support

Ls208xa has several thermal sensors. Add all the sensor id to dts
to enable them.

To make the dts cleaner, re-organize the nodes to split out the
common part so that it can be shared with other SoCs.

Signed-off-by: Yuantian Tang <andy.tang@nxp.com>
---
 arch/arm64/boot/dts/freescale/fsl-ls2080a.dtsi  |   8 +-
 arch/arm64/boot/dts/freescale/fsl-ls2088a.dtsi  |   8 +-
 arch/arm64/boot/dts/freescale/fsl-ls208xa.dtsi  |  70 ++++---
 arch/arm64/boot/dts/freescale/fsl-tmu-map1.dtsi |  99 ++++++++++
 arch/arm64/boot/dts/freescale/fsl-tmu-map2.dtsi |  99 ++++++++++
 arch/arm64/boot/dts/freescale/fsl-tmu-map3.dtsi |  99 ++++++++++
 arch/arm64/boot/dts/freescale/fsl-tmu.dtsi      | 251 ++++++++++++++++++++++++
 7 files changed, 590 insertions(+), 44 deletions(-)
 create mode 100644 arch/arm64/boot/dts/freescale/fsl-tmu-map1.dtsi
 create mode 100644 arch/arm64/boot/dts/freescale/fsl-tmu-map2.dtsi
 create mode 100644 arch/arm64/boot/dts/freescale/fsl-tmu-map3.dtsi
 create mode 100644 arch/arm64/boot/dts/freescale/fsl-tmu.dtsi

--- a/arch/arm64/boot/dts/freescale/fsl-ls2080a.dtsi
+++ b/arch/arm64/boot/dts/freescale/fsl-ls2080a.dtsi
@@ -12,7 +12,7 @@
 #include "fsl-ls208xa.dtsi"
 
 &cpu {
-	cpu0: cpu@0 {
+	cooling_map0: cpu0: cpu@0 {
 		device_type = "cpu";
 		compatible = "arm,cortex-a57";
 		reg = <0x0>;
@@ -32,7 +32,7 @@
 		#cooling-cells = <2>;
 	};
 
-	cpu2: cpu@100 {
+	cooling_map1: cpu2: cpu@100 {
 		device_type = "cpu";
 		compatible = "arm,cortex-a57";
 		reg = <0x100>;
@@ -52,7 +52,7 @@
 		#cooling-cells = <2>;
 	};
 
-	cpu4: cpu@200 {
+	cooling_map2: cpu4: cpu@200 {
 		device_type = "cpu";
 		compatible = "arm,cortex-a57";
 		reg = <0x200>;
@@ -72,7 +72,7 @@
 		#cooling-cells = <2>;
 	};
 
-	cpu6: cpu@300 {
+	cooling_map3: cpu6: cpu@300 {
 		device_type = "cpu";
 		compatible = "arm,cortex-a57";
 		reg = <0x300>;
--- a/arch/arm64/boot/dts/freescale/fsl-ls2088a.dtsi
+++ b/arch/arm64/boot/dts/freescale/fsl-ls2088a.dtsi
@@ -12,7 +12,7 @@
 #include "fsl-ls208xa.dtsi"
 
 &cpu {
-	cpu0: cpu@0 {
+	cooling_map0: cpu0: cpu@0 {
 		device_type = "cpu";
 		compatible = "arm,cortex-a72";
 		reg = <0x0>;
@@ -32,7 +32,7 @@
 		#cooling-cells = <2>;
 	};
 
-	cpu2: cpu@100 {
+	cooling_map1: cpu2: cpu@100 {
 		device_type = "cpu";
 		compatible = "arm,cortex-a72";
 		reg = <0x100>;
@@ -52,7 +52,7 @@
 		#cooling-cells = <2>;
 	};
 
-	cpu4: cpu@200 {
+	cooling_map2: cpu4: cpu@200 {
 		device_type = "cpu";
 		compatible = "arm,cortex-a72";
 		reg = <0x200>;
@@ -72,7 +72,7 @@
 		#cooling-cells = <2>;
 	};
 
-	cpu6: cpu@300 {
+	cooling_map3: cpu6: cpu@300 {
 		device_type = "cpu";
 		compatible = "arm,cortex-a72";
 		reg = <0x300>;
--- a/arch/arm64/boot/dts/freescale/fsl-ls208xa.dtsi
+++ b/arch/arm64/boot/dts/freescale/fsl-ls208xa.dtsi
@@ -77,42 +77,7 @@
 		mask = <0x2>;
 	};
 
-	thermal-zones {
-		cpu_thermal: cpu-thermal {
-			polling-delay-passive = <1000>;
-			polling-delay = <5000>;
-
-			thermal-sensors = <&tmu 4>;
-
-			trips {
-				cpu_alert: cpu-alert {
-					temperature = <75000>;
-					hysteresis = <2000>;
-					type = "passive";
-				};
-				cpu_crit: cpu-crit {
-					temperature = <85000>;
-					hysteresis = <2000>;
-					type = "critical";
-				};
-			};
-
-			cooling-maps {
-				map0 {
-					trip = <&cpu_alert>;
-					cooling-device =
-						<&cpu0 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
-						<&cpu1 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
-						<&cpu2 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
-						<&cpu3 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
-						<&cpu4 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
-						<&cpu5 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
-						<&cpu6 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
-						<&cpu7 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>;
-				};
-			};
-		};
-	};
+	#include "fsl-tmu.dtsi"
 
 	timer: timer {
 		compatible = "arm,armv8-timer";
@@ -907,3 +872,36 @@
 		};
 	};
 };
+
+#include "fsl-tmu-map1.dtsi"
+#include "fsl-tmu-map2.dtsi"
+#include "fsl-tmu-map3.dtsi"
+&thermal_zones {
+	thermal-zone1 {
+		status = "okay";
+	};
+
+	thermal-zone2{
+		status = "okay";
+	};
+
+	thermal-zone3{
+		status = "okay";
+	};
+
+	thermal-zone4{
+		status = "okay";
+	};
+
+	thermal-zone5{
+		status = "okay";
+	};
+
+	thermal-zone6{
+		status = "okay";
+	};
+
+	thermal-zone7 {
+		status = "okay";
+	};
+};
--- /dev/null
+++ b/arch/arm64/boot/dts/freescale/fsl-tmu-map1.dtsi
@@ -0,0 +1,99 @@
+// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
+/*
+ * Device Tree Include file for Thermal Monitor Unit.
+ *
+ * Copyright 2018 NXP
+ *
+ * Tang Yuantian <andy.tang@nxp.com>
+ *
+ */
+
+&thermal_zones {
+	thermal-zone0 {
+		cooling-maps {
+			map1 {
+				trip = <&alert0>;
+				cooling-device =
+					<&cooling_map1 THERMAL_NO_LIMIT
+					THERMAL_NO_LIMIT>;
+			};
+		};
+	};
+
+	thermal-zone1 {
+		cooling-maps {
+			map1 {
+				trip = <&alert1>;
+				cooling-device =
+					<&cooling_map1 THERMAL_NO_LIMIT
+					THERMAL_NO_LIMIT>;
+			};
+		};
+	};
+
+	thermal-zone2 {
+		cooling-maps {
+			map1 {
+				trip = <&alert2>;
+				cooling-device =
+					<&cooling_map1 THERMAL_NO_LIMIT
+					THERMAL_NO_LIMIT>;
+			};
+		};
+	};
+
+	thermal-zone3 {
+		cooling-maps {
+			map1 {
+				trip = <&alert3>;
+				cooling-device =
+					<&cooling_map1 THERMAL_NO_LIMIT
+					THERMAL_NO_LIMIT>;
+			};
+		};
+	};
+
+	thermal-zone4 {
+		cooling-maps {
+			map1 {
+				trip = <&alert4>;
+				cooling-device =
+					<&cooling_map1 THERMAL_NO_LIMIT
+					THERMAL_NO_LIMIT>;
+			};
+		};
+	};
+
+	thermal-zone5 {
+		cooling-maps {
+			map1 {
+				trip = <&alert5>;
+				cooling-device =
+					<&cooling_map1 THERMAL_NO_LIMIT
+					THERMAL_NO_LIMIT>;
+			};
+		};
+	};
+
+	thermal-zone6 {
+		cooling-maps {
+			map1 {
+				trip = <&alert6>;
+				cooling-device =
+					<&cooling_map1 THERMAL_NO_LIMIT
+					THERMAL_NO_LIMIT>;
+			};
+		};
+	};
+
+	thermal-zone7 {
+		cooling-maps {
+			map1 {
+				trip = <&alert7>;
+				cooling-device =
+					<&cooling_map1 THERMAL_NO_LIMIT
+					THERMAL_NO_LIMIT>;
+			};
+		};
+	};
+};
--- /dev/null
+++ b/arch/arm64/boot/dts/freescale/fsl-tmu-map2.dtsi
@@ -0,0 +1,99 @@
+// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
+/*
+ * Device Tree Include file for Thermal Monitor Unit.
+ *
+ * Copyright 2018 NXP
+ *
+ * Tang Yuantian <andy.tang@nxp.com>
+ *
+ */
+
+&thermal_zones {
+	thermal-zone0 {
+		cooling-maps {
+			map2 {
+				trip = <&alert0>;
+				cooling-device =
+					<&cooling_map2 THERMAL_NO_LIMIT
+					THERMAL_NO_LIMIT>;
+			};
+		};
+	};
+
+	thermal-zone1 {
+		cooling-maps {
+			map2 {
+				trip = <&alert1>;
+				cooling-device =
+					<&cooling_map2 THERMAL_NO_LIMIT
+					THERMAL_NO_LIMIT>;
+			};
+		};
+	};
+
+	thermal-zone2 {
+		cooling-maps {
+			map2 {
+				trip = <&alert2>;
+				cooling-device =
+					<&cooling_map2 THERMAL_NO_LIMIT
+					THERMAL_NO_LIMIT>;
+			};
+		};
+	};
+
+	thermal-zone3 {
+		cooling-maps {
+			map2 {
+				trip = <&alert3>;
+				cooling-device =
+					<&cooling_map2 THERMAL_NO_LIMIT
+					THERMAL_NO_LIMIT>;
+			};
+		};
+	};
+
+	thermal-zone4 {
+		cooling-maps {
+			map2 {
+				trip = <&alert4>;
+				cooling-device =
+					<&cooling_map2 THERMAL_NO_LIMIT
+					THERMAL_NO_LIMIT>;
+			};
+		};
+	};
+
+	thermal-zone5 {
+		cooling-maps {
+			map2 {
+				trip = <&alert5>;
+				cooling-device =
+					<&cooling_map2 THERMAL_NO_LIMIT
+					THERMAL_NO_LIMIT>;
+			};
+		};
+	};
+
+	thermal-zone6 {
+		cooling-maps {
+			map2 {
+				trip = <&alert6>;
+				cooling-device =
+					<&cooling_map2 THERMAL_NO_LIMIT
+					THERMAL_NO_LIMIT>;
+			};
+		};
+	};
+
+	thermal-zone7 {
+		cooling-maps {
+			map2 {
+				trip = <&alert7>;
+				cooling-device =
+					<&cooling_map2 THERMAL_NO_LIMIT
+					THERMAL_NO_LIMIT>;
+			};
+		};
+	};
+};
--- /dev/null
+++ b/arch/arm64/boot/dts/freescale/fsl-tmu-map3.dtsi
@@ -0,0 +1,99 @@
+// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
+/*
+ * Device Tree Include file for Thermal Monitor Unit.
+ *
+ * Copyright 2018 NXP
+ *
+ * Tang Yuantian <andy.tang@nxp.com>
+ *
+ */
+
+&thermal_zones {
+	thermal-zone0 {
+		cooling-maps {
+			map3 {
+				trip = <&alert0>;
+				cooling-device =
+					<&cooling_map3 THERMAL_NO_LIMIT
+					THERMAL_NO_LIMIT>;
+			};
+		};
+	};
+
+	thermal-zone1 {
+		cooling-maps {
+			map3 {
+				trip = <&alert1>;
+				cooling-device =
+					<&cooling_map3 THERMAL_NO_LIMIT
+					THERMAL_NO_LIMIT>;
+			};
+		};
+	};
+
+	thermal-zone2 {
+		cooling-maps {
+			map3 {
+				trip = <&alert2>;
+				cooling-device =
+					<&cooling_map3 THERMAL_NO_LIMIT
+					THERMAL_NO_LIMIT>;
+			};
+		};
+	};
+
+	thermal-zone3 {
+		cooling-maps {
+			map3 {
+				trip = <&alert3>;
+				cooling-device =
+					<&cooling_map3 THERMAL_NO_LIMIT
+					THERMAL_NO_LIMIT>;
+			};
+		};
+	};
+
+	thermal-zone4 {
+		cooling-maps {
+			map3 {
+				trip = <&alert4>;
+				cooling-device =
+					<&cooling_map3 THERMAL_NO_LIMIT
+					THERMAL_NO_LIMIT>;
+			};
+		};
+	};
+
+	thermal-zone5 {
+		cooling-maps {
+			map3 {
+				trip = <&alert5>;
+				cooling-device =
+					<&cooling_map3 THERMAL_NO_LIMIT
+					THERMAL_NO_LIMIT>;
+			};
+		};
+	};
+
+	thermal-zone6 {
+		cooling-maps {
+			map3 {
+				trip = <&alert6>;
+				cooling-device =
+					<&cooling_map3 THERMAL_NO_LIMIT
+					THERMAL_NO_LIMIT>;
+			};
+		};
+	};
+
+	thermal-zone7 {
+		cooling-maps {
+			map3 {
+				trip = <&alert7>;
+				cooling-device =
+					<&cooling_map3 THERMAL_NO_LIMIT
+					THERMAL_NO_LIMIT>;
+			};
+		};
+	};
+};
--- /dev/null
+++ b/arch/arm64/boot/dts/freescale/fsl-tmu.dtsi
@@ -0,0 +1,251 @@
+// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
+/*
+ * Device Tree Include file for Thermal Monitor Unit.
+ *
+ * Copyright 2018 NXP
+ *
+ * Tang Yuantian <andy.tang@nxp.com>
+ *
+ */
+
+thermal_zones: thermal-zones {
+	thermal_zone0: thermal-zone0 {
+		polling-delay-passive = <1000>;
+		polling-delay = <5000>;
+		thermal-sensors = <&tmu 0>;
+		status = "disabled";
+
+		trips {
+			alert0: alert0 {
+				temperature = <75000>;
+				hysteresis = <2000>;
+				type = "passive";
+			};
+
+			crit0: crit0 {
+				temperature = <85000>;
+				hysteresis = <2000>;
+				type = "critical";
+			};
+		};
+
+		cooling-maps {
+			map0 {
+				trip = <&alert0>;
+				cooling-device =
+					<&cooling_map0 THERMAL_NO_LIMIT
+					THERMAL_NO_LIMIT>;
+			};
+		};
+	};
+
+	thermal-zone1 {
+		polling-delay-passive = <1000>;
+		polling-delay = <5000>;
+		thermal-sensors = <&tmu 1>;
+		status = "disabled";
+
+		trips {
+			alert1: alert1 {
+				temperature = <75000>;
+				hysteresis = <2000>;
+				type = "passive";
+			};
+
+			crit1: crit1 {
+				temperature = <85000>;
+				hysteresis = <2000>;
+				type = "critical";
+			};
+		};
+
+		cooling-maps {
+			map0 {
+				trip = <&alert1>;
+				cooling-device =
+					<&cooling_map0 THERMAL_NO_LIMIT
+					THERMAL_NO_LIMIT>;
+			};
+		};
+	};
+
+	thermal-zone2 {
+		polling-delay-passive = <1000>;
+		polling-delay = <5000>;
+		thermal-sensors = <&tmu 2>;
+		status = "disabled";
+
+		trips {
+			alert2: alert2 {
+				temperature = <75000>;
+				hysteresis = <2000>;
+				type = "passive";
+			};
+
+			crit2: crit2 {
+				temperature = <85000>;
+				hysteresis = <2000>;
+				type = "critical";
+			};
+		};
+
+		cooling-maps {
+			map0 {
+				trip = <&alert2>;
+				cooling-device =
+					<&cooling_map0 THERMAL_NO_LIMIT
+					THERMAL_NO_LIMIT>;
+			};
+		};
+	};
+
+	thermal-zone3 {
+		polling-delay-passive = <1000>;
+		polling-delay = <5000>;
+		thermal-sensors = <&tmu 3>;
+		status = "disabled";
+
+		trips {
+			alert3: alert3 {
+				temperature = <75000>;
+				hysteresis = <2000>;
+				type = "passive";
+			};
+
+			crit3: crit3 {
+				temperature = <85000>;
+				hysteresis = <2000>;
+				type = "critical";
+			};
+		};
+
+		cooling-maps {
+			map0 {
+				trip = <&alert3>;
+				cooling-device =
+					<&cooling_map0 THERMAL_NO_LIMIT
+					THERMAL_NO_LIMIT>;
+			};
+		};
+	};
+
+	thermal-zone4 {
+		polling-delay-passive = <1000>;
+		polling-delay = <5000>;
+		thermal-sensors = <&tmu 4>;
+		status = "disabled";
+
+		trips {
+			alert4: alert4 {
+				temperature = <75000>;
+				hysteresis = <2000>;
+				type = "passive";
+			};
+
+			crit4: crit4 {
+				temperature = <85000>;
+				hysteresis = <2000>;
+				type = "critical";
+			};
+		};
+
+		cooling-maps {
+			map0 {
+				trip = <&alert4>;
+				cooling-device =
+					<&cooling_map0 THERMAL_NO_LIMIT
+					THERMAL_NO_LIMIT>;
+			};
+		};
+	};
+
+	thermal-zone5 {
+		polling-delay-passive = <1000>;
+		polling-delay = <5000>;
+		thermal-sensors = <&tmu 5>;
+		status = "disabled";
+
+		trips {
+			alert5: alert5 {
+				temperature = <75000>;
+				hysteresis = <2000>;
+				type = "passive";
+			};
+
+			crit5: crit5 {
+				temperature = <85000>;
+				hysteresis = <2000>;
+				type = "critical";
+			};
+		};
+
+		cooling-maps {
+			map0 {
+				trip = <&alert5>;
+				cooling-device =
+					<&cooling_map0 THERMAL_NO_LIMIT
+					THERMAL_NO_LIMIT>;
+			};
+		};
+	};
+
+	thermal-zone6 {
+		polling-delay-passive = <1000>;
+		polling-delay = <5000>;
+		thermal-sensors = <&tmu 6>;
+		status = "disabled";
+
+		trips {
+			alert6: alert6 {
+				temperature = <75000>;
+				hysteresis = <2000>;
+				type = "passive";
+			};
+
+			crit6: crit6 {
+				temperature = <85000>;
+				hysteresis = <2000>;
+				type = "critical";
+			};
+		};
+
+		cooling-maps {
+			map0 {
+				trip = <&alert6>;
+				cooling-device =
+					<&cooling_map0 THERMAL_NO_LIMIT
+					THERMAL_NO_LIMIT>;
+			};
+		};
+	};
+
+	thermal-zone7 {
+		polling-delay-passive = <1000>;
+		polling-delay = <5000>;
+		thermal-sensors = <&tmu 7>;
+		status = "disabled";
+
+		trips {
+			alert7: alert7 {
+				temperature = <75000>;
+				hysteresis = <2000>;
+				type = "passive";
+			};
+
+			crit7: crit7 {
+				temperature = <85000>;
+				hysteresis = <2000>;
+				type = "critical";
+			};
+		};
+
+		cooling-maps {
+			map0 {
+				trip = <&alert7>;
+				cooling-device =
+					<&cooling_map0 THERMAL_NO_LIMIT
+					THERMAL_NO_LIMIT>;
+			};
+		};
+	};
+};
