From f825cdc8bfde7616a14e2163f16303a8973031d2 Mon Sep 17 00:00:00 2001
From: Robert Marko <robert.marko@sartura.hr>
Date: Wed, 7 Oct 2020 17:38:48 +0200
Subject: [PATCH] net: phy: Add Qualcom QCA807x driver

This adds driver for the Qualcomm QCA8072 and QCA8075 PHY-s.

They are 2 or 5 port IEEE 802.3 clause 22 compliant 10BASE-Te, 100BASE-TX and 1000BASE-T PHY-s.

They feature 2 SerDes, one for PSGMII or QSGMII connection with MAC, while second one is SGMII for connection to MAC or fiber.

Both models have a combo port that supports 1000BASE-X and 100BASE-FX fiber.

Each PHY inside of QCA807x series has 4 digitally controlled output only pins that natively drive LED-s.
But some vendors used these to driver generic LED-s controlled by userspace,
so lets enable registering each PHY as GPIO controller and add driver for it.

These are commonly used in Qualcomm IPQ40xx, IPQ60xx and IPQ807x boards.

Signed-off-by: Robert Marko <robert.marko@sartura.hr>
---
 drivers/net/phy/Kconfig  | 6 ++++++
 drivers/net/phy/Makefile | 1 +
 2 files changed, 7 insertions(+)

--- a/drivers/net/phy/Kconfig
+++ b/drivers/net/phy/Kconfig
@@ -537,6 +537,12 @@ config NXP_TJA11XX_PHY
 	---help---
 	  Currently supports the NXP TJA1100 and TJA1101 PHY.
 
+config QCA807X_PHY
+	tristate "Qualcomm QCA807X PHYs"
+	depends on OF_MDIO
+	help
+	  Currently supports the QCA8072 and QCA8075 models.
+
 config QSEMI_PHY
 	tristate "Quality Semiconductor PHYs"
 	---help---
--- a/drivers/net/phy/Makefile
+++ b/drivers/net/phy/Makefile
@@ -103,6 +103,7 @@ obj-$(CONFIG_MICROSEMI_PHY)	+= mscc.o
 obj-$(CONFIG_NATIONAL_PHY)	+= national.o
 obj-$(CONFIG_NXP_TJA11XX_PHY)	+= nxp-tja11xx.o
 obj-$(CONFIG_QSEMI_PHY)		+= qsemi.o
+obj-$(CONFIG_QCA807X_PHY)		+= qca807x.o
 obj-$(CONFIG_REALTEK_PHY)	+= realtek.o
 obj-$(CONFIG_RENESAS_PHY)	+= uPD60620.o
 obj-$(CONFIG_ROCKCHIP_PHY)	+= rockchip.o
