// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "qca955x.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "dlink,dap-2695-a1", "qca,qca9558";
	model = "D-link DAP-2695-A1";

	aliases {
		led-boot = &led_power_red;
		led-failsafe = &led_power_red;
		led-running = &led_power_green;
		led-upgrade = &led_power_red;
	};

	leds {
		compatible = "gpio-leds";

		led_power_green: power_green {
			label = "green:power";
			gpios = <&gpio 23 GPIO_ACTIVE_LOW>;
			default-state = "on";
		};

		led_power_red: power_red {
			label = "red:power";
			gpios = <&gpio 14 GPIO_ACTIVE_LOW>;
		};

		wifi2g {
			label = "green:wifi2g";
			gpios = <&gpio 13 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy1tpt";
		};
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 17 GPIO_ACTIVE_LOW>;
		};
	};
};

&spi {
	status = "okay";

	flash@0 {
		#address-cells = <1>;
		#size-cells = <1>;
		compatible = "mx25l12805d";
		reg = <0>;
		spi-max-frequency = <25000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x000000 0x040000>;
				read-only;
			};

			partition@40000 {
				label = "bdcfg";
				reg = <0x040000 0x010000>;
				read-only;
			};

			partition@50000 {
				label = "rgdb";
				reg = <0x050000 0x010000>;
				read-only;
			};

			partition@60000 {
				label = "langpack";
				reg = <0x060000 0x010000>;
				read-only;
			};

			partition@70000 {
				compatible = "wrg";
				label = "firmware";
				reg = <0x070000 0xf00000>;
			};

			partition@f70000 {
				label = "captival";
				reg = <0xf70000 0x070000>;
				read-only;
			};

			partition@fe0000 {
				label = "certificate";
				reg = <0xfe0000 0x010000>;
				read-only;
			};

			art: partition@ff0000 {
				label = "art";
				reg = <0xff0000 0x010000>;
				read-only;
			};
		};
	};
};

&mdio0 {
	status = "okay";

	phy0: ethernet-phy@0 {
		reg = <0>;

		qca,ar8327-initvals = <
			0x04 0x07600000 /* PORT0_PAD_CTRL */
			0x0c 0x00080080 /* PORT6_PAD_CTRL */
			0x7c 0x0000007e /* PORT0_STATUS */
			0x94 0x0000007e /* PORT6_STATUS */
		>;
	};
};

&eth0 {
	status = "okay";

	phy-handle = <&phy0>;
	pll-data = <0x56000000 0x00000101 0x00001616>;

	fixed-link {
		speed = <1000>;
		full-duplex;
	};
};

&eth1 {
	status = "okay";

	phy-mask = <0>;
	pll-data = <0x03000101 0x00000101 0x00001616>;

	fixed-link {
		speed = <1000>;
		full-duplex;
	};
};

&pcie0 {
	status = "okay";
};

&uart {
	status = "okay";
};

&wmac {
	status = "okay";

	qca,no-eeprom;
};
