// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "qca955x.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	aliases {
		led-boot = &led_power_green;
		led-failsafe = &led_power_amber;
		led-running = &led_power_green;
		led-upgrade = &led_power_amber;
		label-mac-device = &eth0;
	};

	led_spi {
		compatible = "spi-gpio";
		#address-cells = <1>;
		#size-cells = <0>;

		sck-gpios = <&gpio 18 GPIO_ACTIVE_HIGH>;
		mosi-gpios = <&gpio 15 GPIO_ACTIVE_HIGH>;
		num-chipselects = <0>;

		led_gpio: led_gpio@0 {
			compatible = "nxp,74lvc594";
			reg = <0>;
			gpio-controller;
			#gpio-cells = <2>;
			registers-number = <1>;
			spi-max-frequency = <500000>;

			gpio_latch_bit {
				gpio-hog;
				gpios = <4 GPIO_ACTIVE_HIGH>;
				output-high;
				line-name = "gpio-latch-bit";
			};
		};
	};

	leds {
		compatible = "gpio-leds";

		led_power_green: power_green {
			label = "green:power";
			gpios = <&gpio 19 GPIO_ACTIVE_LOW>;
		};

		led_power_amber: power_amber {
			label = "amber:power";
			gpios = <&gpio 20 GPIO_ACTIVE_LOW>;
		};

		left_blue {
			label = "blue:left";
			gpios = <&led_gpio 7 GPIO_ACTIVE_LOW>;
		};

		right_blue {
			label = "blue:right";
			gpios = <&led_gpio 6 GPIO_ACTIVE_LOW>;
		};

		wps_green {
			label = "green:wps";
			gpios = <&led_gpio 5 GPIO_ACTIVE_LOW>;
		};

		client_red {
			label = "red:client";
			gpios = <&led_gpio 3 GPIO_ACTIVE_LOW>;
		};

		client_green {
			label = "green:client";
			gpios = <&led_gpio 2 GPIO_ACTIVE_LOW>;
		};

		router_red {
			label = "red:router";
			gpios = <&led_gpio 1 GPIO_ACTIVE_LOW>;
		};

		router_green {
			label = "green:router";
			gpios = <&led_gpio 0 GPIO_ACTIVE_LOW>;
		};
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "Reset button";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 11 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};

		wps {
			label = "WPS button";
			linux,code = <KEY_WPS_BUTTON>;
			gpios = <&gpio 22 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};

		extender_apmode {
			label = "EXTENDER/APMODE switch";
			gpios = <&gpio 23 GPIO_ACTIVE_LOW>;
			linux,code = <BTN_0>;
			linux,input-type = <EV_SW>;
			debounce-interval = <60>;
		};
	};
};

&pcie0 {
	status = "okay";
};

&uart {
	status = "okay";
};

&pll {
	clocks = <&extosc>;
};

&spi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <25000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			uboot: partition@0 {
				label = "u-boot";
				reg = <0x000000 0x040000>;
				read-only;
			};

			partition@40000 {
				label = "u-boot-env";
				reg = <0x040000 0x010000>;
			};

			caldata: partition@50000 {
				label = "caldata";
				reg = <0x050000 0x010000>;
				read-only;
			};

			partition@60000 {
				label = "caldata-backup";
				reg = <0x060000 0x010000>;
				read-only;
			};

			partition@70000 {
				label = "config";
				reg = <0x070000 0x010000>;
			};

			partition@80000 {
				label = "pot";
				reg = <0x080000 0x010000>;
			};

			partition@90000 {
				label = "firmware";
				reg = <0x090000 0xf30000>;
				compatible = "denx,uimage";
			};

			partition@fc0000 {
				label = "language";
				reg = <0xfc0000 0x040000>;
			};
		};
	};
};

&wmac {
	status = "okay";

	mtd-cal-data = <&caldata 0x1000>;
	mtd-mac-address = <&caldata 0x06>;
};

&mdio0 {
	status = "okay";

	phy4: ethernet-phy@4 {
		reg = <4>;
		phy-mode = "rgmii";
	};
};

&eth0 {
	status = "okay";

	mtd-mac-address = <&caldata 0x00>;

	phy-handle = <&phy4>;
	phy-mode = "rgmii-rxid";

	pll-data = <0x86000000 0x80000101 0x80001313>;
};
