// SPDX-License-Identifier: GPL-2.0-or-later or MIT

/include/ "fsl/p1010si-pre.dtsi"

/ {
	model = "Sophos RED 15w Rev.1";
	compatible = "sophos,red-15w-rev1";

	aliases {
		led-boot = &system_green;
		led-failsafe = &system_red;
		led-running = &system_green;
		led-upgrade = &system_red;
	};

	memory {
		device_type = "memory";
	};

	leds {
		compatible = "gpio-leds";

		system_green: system_green {
			gpios = <&gpio0 7 0>;
			label = "red-15w-rev1:green:system";
		};

		system_red: system_red {
			gpios = <&gpio0 3 0>;
			label = "red-15w-rev1:red:system";
		};

		router {
			gpios = <&gpio0 5 1>;
			label = "red-15w-rev1:green:router";
		};

		internet {
			gpios = <&gpio0 4 1>;
			label = "red-15w-rev1:green:internet";
		};

		tunnel {
			gpios = <&gpio0 8 1>;
			label = "red-15w-rev1:green:tunnel";
		};
	};

	soc: soc@ffe00000 {
		ranges = <0x0 0x0 0xffe00000 0x100000>;

		i2c@3000 {
			eeprom@50 {
				compatible = "st,24c256";
				reg = <0x50>;
			};
		};

		i2c@3100 {
			eeprom@52 {
				compatible = "atmel,24c01";
				reg = < 0x52 >;
			};
		};

		gpio0: gpio-controller@fc00 {
		};

		usb@22000 {
			phy_type = "utmi";
			dr_mode = "host";
		};

		mdio@24000 {
			phy0: ethernet-phy@0 {
				reg = <0x0>;
			};
		};

		mdio@25000 {
			tbi_phy: tbi-phy@11 {
				reg = <0x11>;
			};
		};

		mdio@26000 {
			status = "disabled";
		};

		enet0: ethernet@b0000 {
			phy-connection-type = "rgmii-id";

			fixed-link {
				speed = <1000>;
				full-duplex;
			};
		};

		enet1: ethernet@b1000 {
			phy-handle = <&phy0>;
			phy-connection-type = "sgmii";

			tbi-handle = <&tbi_phy>;
		};

		enet2: ethernet@b2000 {
			status = "disabled";
		};

		sdhc@2e000 {
			status = "disabled";
		};
	};

	ifc: ifc@ffe1e000 {
		reg = <0x0 0xffe1e000 0 0x2000>;

		/* NOR, NAND Flashes and CPLD on board */
		ranges = <0x0 0x0 0x0 0xee000000 0x02000000
			0x1 0x0 0x0 0xff800000 0x00010000
			0x3 0x0 0x0 0xffb00000 0x00000020>;

		nand@1,0 {
			compatible = "fsl,ifc-nand";
			reg = <0x1 0x0 0x10000>;

			partitions {
				compatible = "fixed-partitions";
				#address-cells = <1>;
				#size-cells = <1>;

				/*
				 * Original partition layout:
				 * 0x000000000000-0x000000100000 : "NAND U-Boot Image"
				 * 0x000000100000-0x000000200000 : "NAND U-Boot Environment"
				 * 0x000000200000-0x000000300000 : "Provisioning"
				 *  - OS-Image 1
				 * 0x000000300000-0x000000400000 : "fdt1"
				 * 0x000000400000-0x000000c00000 : "uimage1"
				 * 0x000000c00000-0x000001c00000 : "rootfs1"
				 *  - OS-Image 2
				 * 0x000001c00000-0x000001d00000 : "fdt2"
				 * 0x000001d00000-0x000002500000 : "uimage2"
				 * 0x000002500000-0x000003500000 : "rootfs2"
				 *  - Empty
				 * 0x000003500000-0x000008000000 : "data"
				 */

				partition@0 {
					reg = <0x0 0x100000>;
					label = "u-boot";
					read-only;
				};

				partition@100000 {
					reg = <0x100000 0x100000>;
					label = "u-boot-env";
				};

				partition@200000 {
					reg = <0x200000 0x100000>;
					label = "provisioning";
					read-only;
				};

				partition@300000 {
					reg = <0x300000 0x800000>;
					label = "kernel";
				};

				partition@b00000 {
					reg = <0xb00000 0x7500000>;
					label = "ubi";
				};

				oem-partition@300000 {
					reg = <0x300000 0x1900000>;
					label = "sophos-os1";
				};

				oem-partition@1c00000 {
					reg = <0x1c00000 0x1900000>;
					label = "sophos-os2";
				};

				oem-partition@3500000 {
					reg = <0x3500000 0x4b00000>;
					label = "sophos-data";
				};
			};
		};
	};

	pci0: pcie@ffe09000 {
		status = "disabled";
	};

	pci1: pcie@ffe0a000 {
		reg = <0 0xffe0a000 0 0x1000>;
		ranges = <0x2000000 0x0 0x80000000 0 0x80000000 0x0 0x20000000
			  0x1000000 0x0 0x00000000 0 0xffc00000 0x0 0x10000>;
		pcie@0 {
			ranges = <0x2000000 0x0 0x80000000
				  0x2000000 0x0 0x80000000
				  0x0 0x20000000

				  0x1000000 0x0 0x0
				  0x1000000 0x0 0x0
				  0x0 0x100000>;
		};
	};
};

/include/ "fsl/p1010si-post.dtsi"
