#!/bin/sh

. /lib/functions.sh
. /lib/functions/uci-defaults.sh
. /lib/functions/system.sh

mediatek_setup_interfaces()
{
	local board="$1"

	case $board in
	bananapi,bpi-r64-rootdisk|\
	bananapi,bpi-r64)
		ucidef_set_interfaces_lan_wan "lan0 lan1 lan2 lan3" wan
		;;
	mediatek,mt7622-rfb1)
		ucidef_set_interfaces_lan_wan "lan1 lan2 lan3 lan4" wan
		;;
	*)
		ucidef_add_switch "switch0" \
				  "0:lan" "1:lan" "2:lan" "3:lan" "4:wan" "6u@eth0" "5u@eth1"
		;;
	esac
}

mediatek_setup_macs()
{
	local board="$1"

	case $board in
	esac
}

board_config_update
board=$(board_name)
mediatek_setup_interfaces $board
mediatek_setup_macs $board
board_config_flush

exit 0
