#include "bcm6362.dtsi"

#include <dt-bindings/input/input.h>

/ {
	model = "Huawei HG253s v2";
	compatible = "huawei,hg253s-v2", "brcm,bcm6362";

	aliases {
		led-boot = &led_phone_green;
		led-failsafe = &led_phone_green;
		led-upgrade = &led_phone_green;
	};

	chosen {
		bootargs = "rootfstype=squashfs,ubifs noinitrd console=ttyS0,115200";
		stdout-path = "serial0:115200n8";
	};

	keys {
		compatible = "gpio-keys-polled";
		#address-cells = <1>;
		#size-cells = <0>;
		poll-interval = <20>;

		reset {
			label = "reset";
			gpios = <&pinctrl 24 1>;
			linux,code = <KEY_RESTART>;
			debounce-interval = <60>;
		};

		wlan {
			label = "wlan";
			gpios = <&pinctrl 25 1>;
			linux,code = <KEY_WLAN>;
			debounce-interval = <60>;
		};

		wps {
			label = "wps";
			gpios = <&pinctrl 26 1>;
			linux,code = <KEY_WPS_BUTTON>;
			debounce-interval = <60>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led_phone_green: led@28 {
			label = "green:phone";
			gpios = <&pinctrl 28 1>;
		};

		led@30 {
			label = "green:usb";
			gpios = <&pinctrl 30 1>;
		};
	};
};

&leds {
	status = "okay";

	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_leds>;

	led@3 {
		reg = <3>;
		active-low;
		label = "green:internet";
	};

	led@5 {
		reg = <5>;
		active-low;
		label = "green:wifi";
	};
};

&lsspi {
	switch@0 {
		compatible = "brcm,bcm53125";
		reg = <0>;
		spi-max-frequency = <781000>;

		lede,alias = "eth0";

		ports {
			#address-cells = <1>;
			#size-cells = <0>;

			lan@1 {
				reg = <1>;
				label = "lan4";
			};

			lan@2 {
				reg = <2>;
				label = "lan3";
			};

			lan@3 {
				reg = <3>;
				label = "lan2";
			};

			lan@4 {
				reg = <4>;
				label = "lan1";
			};

			cpu@8 {
				reg = <8>;
				label = "cpu";

				fixed-link {
					speed = <1000>;
					full-duplex;
					asym-pause;
					pause;
				};
			};
		};
	};
};

&nflash {
	status = "okay";

	nandcs@0 {
		compatible = "brcm,nandcs";
		#size-cells = <1>;
		#address-cells = <1>;
		reg = <0>;
		nand-ecc-step-size = <512>;
		nand-ecc-strength = <15>;
		nand-on-flash-bbt;
		brcm,nand-oob-sector-size = <64>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "cferom";
				reg = <0x0000000 0x0020000>;
				read-only;
			};

			partition@20000 {
				compatible = "brcm,wfi";
				label = "wfi";
				reg = <0x0020000 0x7d80000>;
			};

			partition@7da0000 {
				label = "nvram";
				reg = <0x7da0000 0x160000>;
			};
		};
	};
};

&pinctrl {
	pinctrl_leds: leds {
		function = "led";
		pins = "gpio3", "gpio5";
	};
};

&uart0 {
	status = "okay";
};
