// SPDX-License-Identifier: GPL-2.0-or-later

#include "rt5350.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "zyxel,keenetic-lite-b", "ralink,rt5350-soc";
	model = "ZyXEL Keenetic Lite Rev.B";

	aliases {
		led-boot = &led_power;
		led-failsafe = &led_power;
		led-running = &led_power;
		led-upgrade = &led_power;
	};

	leds {
		compatible = "gpio-leds";

		led_power: power {
			label = "green:power";
			gpios = <&gpio0 9 GPIO_ACTIVE_LOW>;
		};

		wps {
			label = "green:wps";
			gpios = <&gpio0 14 GPIO_ACTIVE_LOW>;
		};
	};

	keys {
		compatible = "gpio-keys";

		wps {
			label = "wps";
			gpios = <&gpio0 0 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
		};

		reset {
			label = "reset";
			gpios = <&gpio0 10 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};
};

&spi0 {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <60000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x0 0x30000>;
				read-only;
			};

			partition@30000 {
				label = "u-boot-env";
				reg = <0x30000 0x10000>;
				read-only;
			};

			factory: partition@40000 {
				label = "factory";
				reg = <0x40000 0x10000>;
				read-only;
			};

			partition@50000 {
				compatible = "denx,uimage";
				label = "firmware";
				reg = <0x50000 0x7b0000>;
			};
		};
	};
};

&state_default {
	gpio {
		groups = "uartf";
		function = "gpio";
	};
};

&ethernet {
	mtd-mac-address = <&factory 0x28>;
};

&esw {
	mediatek,portmap = <0x2f>;
	mediatek,led_polarity = <0x17>;
};

&wmac {
	ralink,led-polarity = <1>;
	ralink,mtd-eeprom = <&factory 0x0>;
};
