--- a/drivers/net/wireless/ath/ath9k/channel.c
+++ b/drivers/net/wireless/ath/ath9k/channel.c
@@ -15,6 +15,7 @@
  */
 
 #include "ath9k.h"
+#include "hsr.h"
 
 /* Set/change channels.  If the channel is really being changed, it's done
  * by reseting the chip.  To accomplish this we must first cleanup any pending
@@ -22,6 +23,7 @@
  */
 static int ath_set_channel(struct ath_softc *sc)
 {
+	struct device_node *np = sc->dev->of_node;
 	struct ath_hw *ah = sc->sc_ah;
 	struct ath_common *common = ath9k_hw_common(ah);
 	struct ieee80211_hw *hw = sc->hw;
@@ -42,6 +44,11 @@ static int ath_set_channel(struct ath_so
 	ath_dbg(common, CONFIG, "Set channel: %d MHz width: %d\n",
 		chan->center_freq, chandef->width);
 
+	if (of_property_read_bool(np, "ubnt,hsr")) {
+		ath9k_hsr_enable(ah, chandef->width, chan->center_freq);
+		ath9k_hsr_status(ah);
+	}
+
 	/* update survey stats for the old channel before switching */
 	spin_lock_irqsave(&common->cc_lock, flags);
 	ath_update_survey_stats(sc);
--- /dev/null
+++ b/drivers/net/wireless/ath/ath9k/hsr.c
@@ -0,0 +1,247 @@
+/*
+ *
+ * The MIT License (MIT)
+ *
+ * Copyright (c) 2015 Kirill Berezin
+ *
+ * Permission is hereby granted, free of charge, to any person obtaining a copy
+ * of this software and associated documentation files (the "Software"), to deal
+ * in the Software without restriction, including without limitation the rights
+ * to use, copy, modify, merge, publish, distribute, sublicense, and/or sell
+ * copies of the Software, and to permit persons to whom the Software is
+ * furnished to do so, subject to the following conditions:
+ *
+ * The above copyright notice and this permission notice shall be included in
+ * all copies or substantial portions of the Software.
+ *
+ * THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS OR
+ * IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF MERCHANTABILITY,
+ * FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL THE
+ * AUTHORS OR COPYRIGHT HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER
+ * LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING FROM,
+ * OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR OTHER DEALINGS IN THE
+ * SOFTWARE.
+ *
+ */
+
+#include <linux/io.h>
+#include <linux/slab.h>
+#include <linux/module.h>
+#include <linux/time.h>
+#include <linux/bitops.h>
+#include <linux/etherdevice.h>
+#include <linux/rtnetlink.h>
+#include <asm/unaligned.h>
+
+#include "hw.h"
+#include "ath9k.h"
+
+#define HSR_GPIO_CSN 8
+#define HSR_GPIO_CLK 6
+#define HSR_GPIO_DOUT 7
+#define HSR_GPIO_DIN 5
+
+/* delays are in useconds */
+#define HSR_DELAY_HALF_TICK 100
+#define HSR_DELAY_PRE_WRITE 75
+#define HSR_DELAY_FINAL 20000
+#define HSR_DELAY_TRAILING 200
+
+void ath9k_hsr_init(struct ath_hw *ah)
+{
+	ath9k_hw_gpio_request_in(ah, HSR_GPIO_DIN, NULL);
+	ath9k_hw_gpio_request_out(ah, HSR_GPIO_CSN, NULL,
+				  AR_GPIO_OUTPUT_MUX_AS_OUTPUT);
+	ath9k_hw_gpio_request_out(ah, HSR_GPIO_CLK, NULL,
+				  AR_GPIO_OUTPUT_MUX_AS_OUTPUT);
+	ath9k_hw_gpio_request_out(ah, HSR_GPIO_DOUT, NULL,
+				  AR_GPIO_OUTPUT_MUX_AS_OUTPUT);
+
+	ath9k_hw_set_gpio(ah, HSR_GPIO_CSN, 1);
+	ath9k_hw_set_gpio(ah, HSR_GPIO_CLK, 0);
+	ath9k_hw_set_gpio(ah, HSR_GPIO_DOUT, 0);
+
+	udelay(HSR_DELAY_TRAILING);
+}
+
+static u32 ath9k_hsr_write_byte(struct ath_hw *ah, int delay, u32 value)
+{
+	struct ath_common *common = ath9k_hw_common(ah);
+	int i;
+	u32 rval = 0;
+
+	udelay(delay);
+
+	ath9k_hw_set_gpio(ah, HSR_GPIO_CLK, 0);
+	udelay(HSR_DELAY_HALF_TICK);
+
+	ath9k_hw_set_gpio(ah, HSR_GPIO_CSN, 0);
+	udelay(HSR_DELAY_HALF_TICK);
+
+	for (i = 0; i < 8; ++i) {
+		rval = rval << 1;
+
+		/* pattern is left to right, that is 7-th bit runs first */
+		ath9k_hw_set_gpio(ah, HSR_GPIO_DOUT, (value >> (7 - i)) & 0x1);
+		udelay(HSR_DELAY_HALF_TICK);
+
+		ath9k_hw_set_gpio(ah, HSR_GPIO_CLK, 1);
+		udelay(HSR_DELAY_HALF_TICK);
+
+		rval |= ath9k_hw_gpio_get(ah, HSR_GPIO_DIN);
+
+		ath9k_hw_set_gpio(ah, HSR_GPIO_CLK, 0);
+		udelay(HSR_DELAY_HALF_TICK);
+	}
+
+	ath9k_hw_set_gpio(ah, HSR_GPIO_CSN, 1);
+	udelay(HSR_DELAY_HALF_TICK);
+
+	ath_dbg(common, CONFIG, "ath9k_hsr_write_byte: write byte %d return value is %d %c\n",
+		value, rval, rval > 32 ? rval : '-');
+
+	return rval & 0xff;
+}
+
+static int ath9k_hsr_write_a_chain(struct ath_hw *ah, char *chain, int items)
+{
+	int status = 0;
+	int i = 0;
+	int err;
+
+	/* a preamble */
+	ath9k_hsr_write_byte(ah, HSR_DELAY_PRE_WRITE, 0);
+	status = ath9k_hsr_write_byte(ah, HSR_DELAY_PRE_WRITE, 0);
+
+	/* clear HSR's reply buffer */
+	if (status) {
+		int loop = 0;
+
+		for (loop = 0; (loop < 42) && status; ++loop)
+			status = ath9k_hsr_write_byte(ah, HSR_DELAY_PRE_WRITE,
+						      0);
+
+		if (loop >= 42) {
+			ATH_DBG_WARN(1,
+				     "ath9k_hsr_write_a_chain: can't clear an output buffer after a 42 cycles.\n");
+			return -1;
+		}
+	}
+
+	for (i = 0; (i < items) && (chain[i] != 0); ++i)
+		ath9k_hsr_write_byte(ah, HSR_DELAY_PRE_WRITE, (u32)chain[i]);
+
+	ath9k_hsr_write_byte(ah, HSR_DELAY_PRE_WRITE, 0);
+	mdelay(HSR_DELAY_FINAL / 1000);
+
+	/* reply */
+	memset(chain, 0, items);
+
+	ath9k_hsr_write_byte(ah, HSR_DELAY_PRE_WRITE, 0);
+	udelay(HSR_DELAY_TRAILING);
+
+	for (i = 0; i < (items - 1); ++i) {
+		u32 ret;
+
+		ret = ath9k_hsr_write_byte(ah, HSR_DELAY_PRE_WRITE, 0);
+		if (ret != 0)
+			chain[i] = (char)ret;
+		else
+			break;
+
+		udelay(HSR_DELAY_TRAILING);
+	}
+
+	if (i <= 1)
+		return 0;
+
+	err = kstrtoint(chain + 1, 10, &i);
+	if (err)
+		return err;
+
+	return i;
+}
+
+int ath9k_hsr_disable(struct ath_hw *ah)
+{
+	char cmd[10] = {'b', '4', '0', 0, 0, 0, 0, 0, 0, 0};
+	int ret;
+
+	ret = ath9k_hsr_write_a_chain(ah, cmd, sizeof(cmd));
+	if ((ret > 0) && (*cmd == 'B'))
+		return 0;
+
+	return -1;
+}
+
+int ath9k_hsr_enable(struct ath_hw *ah, int bw, int fq)
+{
+	char cmd[10];
+	int ret;
+
+	/* Bandwidth argument is 0 sometimes. Assume default 802.11bgn
+	 * 20MHz on invalid values
+	 */
+	if ((bw != 5) && (bw != 10) && (bw != 20) && (bw != 40))
+		bw = 20;
+
+	memset(cmd, 0, sizeof(cmd));
+	*cmd = 'b';
+	snprintf(cmd + 1, 3, "%02d", bw);
+
+	ret = ath9k_hsr_write_a_chain(ah, cmd, sizeof(cmd));
+	if ((*cmd != 'B') || (ret != bw)) {
+		ATH_DBG_WARN(1,
+			     "ath9k_hsr_enable: failed changing bandwidth -> set (%d,%d) reply (%d, %d)\n",
+			     'b', bw, *cmd, ret);
+		return -1;
+	}
+
+	memset(cmd, 0, sizeof(cmd));
+	*cmd = 'x';
+	ret = ath9k_hsr_write_a_chain(ah, cmd, sizeof(cmd));
+	if (*cmd != 'X') {
+		ATH_DBG_WARN(1,
+			     "ath9k_hsr_enable: failed 'x' command -> reply (%d, %d)\n",
+			     *cmd, ret);
+		return -1;
+	}
+
+	memset(cmd, 0, sizeof(cmd));
+	*cmd = 'm';
+	ret = ath9k_hsr_write_a_chain(ah, cmd, sizeof(cmd));
+	if (*cmd != 'M') {
+		ATH_DBG_WARN(1,
+			     "ath9k_hsr_enable: failed 'm' command -> reply (%d, %d)\n",
+			     *cmd, ret);
+		return  -1;
+	}
+
+	memset(cmd, 0, sizeof(cmd));
+	*cmd = 'f';
+	snprintf(cmd + 1, 6, "%05d", fq);
+	ret = ath9k_hsr_write_a_chain(ah, cmd, sizeof(cmd));
+	if ((*cmd != 'F') && (ret != fq)) {
+		ATH_DBG_WARN(1,
+			     "ath9k_hsr_enable: failed set frequency -> reply (%d, %d)\n",
+			     *cmd, ret);
+		return -1;
+	}
+
+	return 0;
+}
+
+int ath9k_hsr_status(struct ath_hw *ah)
+{
+	char cmd[10] = {'s', 0, 0, 0, 0, 0, 0, 0, 0, 0};
+	int ret;
+
+	ret = ath9k_hsr_write_a_chain(ah, cmd, sizeof(cmd));
+	if (*cmd != 'S') {
+		ATH_DBG_WARN(1, "ath9k_hsr_status: returned %d,%d\n", *cmd,
+			     ret);
+		return -1;
+	}
+
+	return 0;
+}
--- /dev/null
+++ b/drivers/net/wireless/ath/ath9k/hsr.h
@@ -0,0 +1,48 @@
+/*
+ * The MIT License (MIT)
+ *
+ * Copyright (c) 2015 Kirill Berezin
+ *
+ * Permission is hereby granted, free of charge, to any person obtaining a copy
+ * of this software and associated documentation files (the "Software"), to deal
+ * in the Software without restriction, including without limitation the rights
+ * to use, copy, modify, merge, publish, distribute, sublicense, and/or sell
+ * copies of the Software, and to permit persons to whom the Software is
+ * furnished to do so, subject to the following conditions:
+ *
+ * The above copyright notice and this permission notice shall be included in
+ * all copies or substantial portions of the Software.
+ *
+ * THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS OR
+ * IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF MERCHANTABILITY,
+ * FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL THE
+ * AUTHORS OR COPYRIGHT HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER
+ * LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING FROM,
+ * OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR OTHER DEALINGS IN THE
+ * SOFTWARE.
+ */
+
+#ifndef HSR_H
+#define HSR_H
+
+#ifdef CPTCFG_ATH9K_UBNTHSR
+
+void ath9k_hsr_init(struct ath_hw *ah);
+int ath9k_hsr_disable(struct ath_hw *ah);
+int ath9k_hsr_enable(struct ath_hw *ah, int bw, int fq);
+int ath9k_hsr_status(struct ath_hw *ah);
+
+#else
+static inline void ath9k_hsr_init(struct ath_hw *ah) {}
+
+static inline int ath9k_hsr_enable(struct ath_hw *ah, int bw, int fq)
+{
+	return 0;
+}
+
+static inline int ath9k_hsr_disable(struct ath_hw *ah) { return 0; }
+static inline int ath9k_hsr_status(struct ath_hw *ah) { return 0; }
+
+#endif
+
+#endif /* HSR_H */
--- a/drivers/net/wireless/ath/ath9k/main.c
+++ b/drivers/net/wireless/ath/ath9k/main.c
@@ -18,6 +18,7 @@
 #include <linux/delay.h>
 #include "ath9k.h"
 #include "btcoex.h"
+#include "hsr.h"
 
 u8 ath9k_parse_mpdudensity(u8 mpdudensity)
 {
@@ -649,6 +650,7 @@ void ath_reset_work(struct work_struct *
 static int ath9k_start(struct ieee80211_hw *hw)
 {
 	struct ath_softc *sc = hw->priv;
+	struct device_node *np = sc->dev->of_node;
 	struct ath_hw *ah = sc->sc_ah;
 	struct ath_common *common = ath9k_hw_common(ah);
 	struct ieee80211_channel *curchan = sc->cur_chan->chandef.chan;
@@ -727,6 +729,11 @@ static int ath9k_start(struct ieee80211_
 					  AR_GPIO_OUTPUT_MUX_AS_OUTPUT);
 	}
 
+	if (of_property_read_bool(np, "ubnt,hsr")) {
+		ath9k_hsr_init(ah);
+		ath9k_hsr_disable(ah);
+	}
+
 	/*
 	 * Reset key cache to sane defaults (all entries cleared) instead of
 	 * semi-random values after suspend/resume.
--- a/drivers/net/wireless/ath/ath9k/Makefile
+++ b/drivers/net/wireless/ath/ath9k/Makefile
@@ -17,6 +17,7 @@ ath9k-$(CPTCFG_ATH9K_DFS_CERTIFIED) += d
 ath9k-$(CPTCFG_ATH9K_TX99) += tx99.o
 ath9k-$(CPTCFG_ATH9K_WOW) += wow.o
 ath9k-$(CPTCFG_ATH9K_HWRNG) += rng.o
+ath9k-$(CPTCFG_ATH9K_UBNTHSR) += hsr.o
 
 ath9k-$(CPTCFG_ATH9K_DEBUGFS) += debug.o
 
--- a/local-symbols
+++ b/local-symbols
@@ -112,6 +112,7 @@ ATH9K_WOW=
 ATH9K_RFKILL=
 ATH9K_CHANNEL_CONTEXT=
 ATH9K_PCOEM=
+ATH9K_UBNTHSR=
 ATH9K_PCI_NO_EEPROM=
 ATH9K_HTC=
 ATH9K_HTC_DEBUGFS=
--- a/drivers/net/wireless/ath/ath9k/Kconfig
+++ b/drivers/net/wireless/ath/ath9k/Kconfig
@@ -60,6 +60,19 @@ config ATH9K_AHB
 	  Say Y, if you have a SoC with a compatible built-in
 	  wireless MAC. Say N if unsure.
 
+config ATH9K_UBNTHSR
+	bool "Ubiquiti UniFi Outdoor Plus HSR support"
+	depends on ATH9K
+	---help---
+	  This options enables code to control the HSR RF
+	  filter in the receive path of the Ubiquiti UniFi
+	  Outdoor Plus access point.
+
+	  Say Y if you want to use the access point. The
+	  code will only be used if the device is detected,
+	  so it does not harm other setup other than occupying
+	  a bit of memory.
+
 config ATH9K_DEBUGFS
 	bool "Atheros ath9k debugging"
 	depends on ATH9K && DEBUG_FS
