// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "ar7242.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/mtd/partitions/uimage.h>

/ {
	compatible = "engenius,eap350-v1", "qca,ar7242";
	model = "EnGenius EAP350 v1";

	aliases {
		label-mac-device = &eth0;
		led-boot = &led_power;
		led-failsafe = &led_power;
		led-running = &led_power;
		led-upgrade = &led_power;
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			gpios = <&gpio 0 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
			linux,code = <KEY_RESTART>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led_power: power {
			label = "blue:power";
			gpios = <&gpio 17 GPIO_ACTIVE_HIGH>;
			default-state = "on";
		};
	};

	ath9k-leds {
		compatible = "gpio-leds";

		wlan {
			label = "blue:wlan";
			gpios = <&ath9k 1 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0tpt";
		};
	};

	virtual_flash {
		compatible = "mtd-concat";

		devices = <&fwconcat0 &fwconcat1>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				compatible = "openwrt,uimage", "denx,uimage";
				openwrt,ih-magic = <IH_MAGIC_OKLI>;
				label = "firmware";
				reg = <0x0 0x0>;
			};
		};
	};
};

&uart {
	status = "okay";
};

&spi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <20000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x0 0x40000>;
				read-only;
			};

			partition@40000 {
				label = "u-boot-env";
				reg = <0x40000 0x10000>;
			};

			partition@50000 {
				label = "custom";
				reg = <0x50000 0x50000>;
				read-only;
			};

			partition@a0000 {
				label = "loader";
				reg = <0xa0000 0x10000>;
				read-only;
			};

			fwconcat1: partition@b0000 {
				label = "fwconcat1";
				reg = <0xb0000 0xf0000>;
			};

			partition@1a0000 {
				label = "fakeroot";
				reg = <0x1a0000 0x10000>;
				read-only;
			};

			fwconcat0: partition@1b0000 {
				label = "fwconcat0";
				reg = <0x1b0000 0x4c0000>;
			};

			partition@670000 {
				label = "failsafe";
				reg = <0x670000 0x180000>;
				read-only;
			};

			art: partition@7f0000 {
				label = "art";
				reg = <0x7f0000 0x10000>;
				read-only;
			};
		};
	};
};

&mdio0 {
	status = "okay";

	phy4: ethernet-phy@4 {
		reg = <4>;
		eee-broken-100tx;
		eee-broken-1000t;
	};
};

&eth0 {
	status = "okay";

	mtd-mac-address = <&art 0x0>;

	phy-handle = <&phy4>;
	phy-mode = "rgmii-id";

	pll-data = <0x02000000 0x00000101 0x00001313>;
};

&pcie {
	status = "okay";

	ath9k: wifi@0,0,0 {
		compatible = "pci168c,002a";
		reg = <0x0 0 0 0 0>;
		mtd-mac-address = <&art 0x0>;
		mtd-mac-address-increment = <1>;
		qca,no-eeprom;
		#gpio-cells = <2>;
		gpio-controller;
	};
};
