--- a/arch/arm/mach-mvebu/Kconfig
+++ b/arch/arm/mach-mvebu/Kconfig
@@ -69,6 +69,7 @@ config MACH_ARMADA_38X
 	select HAVE_SMP
 	select MACH_MVEBU_V7
 	select PINCTRL_ARMADA_38X
+	select ARCH_WANT_LIBATA_LEDS
 	help
 	  Say 'Y' here if you want your kernel to support boards based
 	  on the Marvell Armada 380/385 SoC with device tree.
