From 73f63c66bf80bebd46d38a2660078dbe3fe11170 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <rafal@milecki.pl>
Date: Thu, 14 Jan 2021 12:02:28 +0100
Subject: [PATCH] phy: phy-brcm-usb: select SOC_BRCMSTB on brcmstb only
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

BCM4908 doesn't need brcmstb SoC stuff compiled.

Signed-off-by: Rafał Miłecki <rafal@milecki.pl>
---
 drivers/phy/broadcom/Kconfig | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/phy/broadcom/Kconfig
+++ b/drivers/phy/broadcom/Kconfig
@@ -86,7 +86,7 @@ config PHY_BRCM_USB
 	depends on ARCH_BCM4908 || ARCH_BRCMSTB
 	depends on OF
 	select GENERIC_PHY
-	select SOC_BRCMSTB
+	select SOC_BRCMSTB if ARCH_BRCMSTB
 	default ARCH_BCM4908
 	default ARCH_BRCMSTB
 	help
