From 2d1c30a79cb9d390d2425852ff8c9527c31b3ab8 Mon Sep 17 00:00:00 2001
From: Maxime Ripard <maxime@cerno.tech>
Date: Wed, 12 Feb 2020 14:21:45 +0100
Subject: [PATCH] clk: bcm: rpi: Switch to clk_hw_register_clkdev

Since we don't care about retrieving the clk_lookup structure pointer
returned by clkdev_hw_create, we can just use the clk_hw_register_clkdev
function.

Cc: Michael Turquette <mturquette@baylibre.com>
Cc: linux-clk@vger.kernel.org
Acked-by: Nicolas Saenz Julienne <nsaenzjulienne@suse.de>
Reviewed-by: Stephen Boyd <sboyd@kernel.org>
Signed-off-by: Maxime Ripard <maxime@cerno.tech>
---
 drivers/clk/bcm/clk-raspberrypi.c | 11 +++++------
 1 file changed, 5 insertions(+), 6 deletions(-)

--- a/drivers/clk/bcm/clk-raspberrypi.c
+++ b/drivers/clk/bcm/clk-raspberrypi.c
@@ -237,7 +237,6 @@ static struct clk_fixed_factor raspberry
 
 static int raspberrypi_register_pllb_arm(struct raspberrypi_clk *rpi)
 {
-	struct clk_lookup *pllb_arm_lookup;
 	int ret;
 
 	ret = devm_clk_hw_register(rpi->dev, &raspberrypi_clk_pllb_arm.hw);
@@ -246,11 +245,11 @@ static int raspberrypi_register_pllb_arm
 		return ret;
 	}
 
-	pllb_arm_lookup = clkdev_hw_create(&raspberrypi_clk_pllb_arm.hw,
-					   NULL, "cpu0");
-	if (!pllb_arm_lookup) {
-		dev_err(rpi->dev, "Failed to initialize pllb_arm_lookup\n");
-		return -ENOMEM;
+	ret = clk_hw_register_clkdev(&raspberrypi_clk_pllb_arm.hw,
+				     NULL, "cpu0");
+	if (ret) {
+		dev_err(rpi->dev, "Failed to initialize clkdev\n");
+		return ret;
 	}
 
 	return 0;
