#include "danube.dtsi"

#include <dt-bindings/input/input.h>

/ {
	compatible = "arcadyan,arv7506pw11", "lantiq,xway", "lantiq,danube";
	model = "Alice/O2 IAD 4421";

	chosen {
		bootargs = "console=ttyLTQ0,115200";
	};

	aliases {
		led-boot = &power;
		led-failsafe = &power_red;
		led-running = &power;
		led-upgrade = &power;

		led-dsl = &dsl;
		led-internet = &internet;
		led-wifi = &wlan;
	};

	memory@0 {
		device_type = "memory";
		reg = <0x0 0x4000000>;
	};

	keys {
		compatible = "gpio-keys-polled";
		poll-interval = <100>;

		rfkill {
			label = "rfkill";
			gpios = <&gpio 11 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RFKILL>;
		};
		reset {
			label = "reset";
			gpios = <&gpio 30 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};

	leds {
		compatible = "gpio-leds";
		wlan: wlan {
			label = "green:wlan";
			gpios = <&gpio 2 GPIO_ACTIVE_LOW>;
		};
		power: power {
			label = "green:power";
			gpios = <&gpio 3 GPIO_ACTIVE_LOW>;
			default-state = "keep";
		};
		dsl: dsl {
			label = "green:dsl";
			gpios = <&gpio 4 GPIO_ACTIVE_LOW>;
		};
		internet: internet {
			label = "green:internet";
			gpios = <&gpio 5 GPIO_ACTIVE_LOW>;
		};
		power_red: power_red {
			label = "red:power";
			gpios = <&gpio 6 GPIO_ACTIVE_LOW>;
		};
		internet_red {
			label = "red:internet";
			gpios = <&gpio 7 GPIO_ACTIVE_LOW>;
		};
		info {
			label = "green:info";
			gpios = <&gpio 8 GPIO_ACTIVE_LOW>;
		};
		telefon {
			label = "green:telefon";
			gpios = <&gpio 9 GPIO_ACTIVE_LOW>;
		};
		info_red {
			label = "red:info";
			gpios = <&gpio 20 GPIO_ACTIVE_LOW>;
		};
	};
};

&gpio {
	pinctrl-names = "default";
	pinctrl-0 = <&state_default>;

	state_default: pinmux {
		pci_rst {
			lantiq,pins = "io21";
			lantiq,pull = <2>;
			lantiq,output = <1>;
		};
	};
};

/* GPIO 19: switch reset */
&gsw {
	phy-mode = "rmii";
	mtd-mac-address = <&boardconfig 0x16>;
};

&localbus {
	flash@0 {
		compatible = "lantiq,nor";
		bank-width = <2>;
		reg = <0 0x0 0x800000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "uboot";
				reg = <0x00000 0x40000>;
				read-only;
			};

			partition@40000 {
				label = "u-boot-env";
				reg = <0x40000 0x10000>;
				read-only;
			};

			partition@50000 {
				label = "firmware";
				reg = <0x50000 0x7a0000>;
			};

			boardconfig: partition@7f0000 {
				label = "board_config";
				reg = <0x7f0000 0x10000>;
				read-only;
			};
		};
	};
};

&pci0 {
	status = "okay";

	pinctrl-0 = <&pci_gnt1_pins>, <&pci_req1_pins>;
	pinctrl-names = "default";

	lantiq,external-clock;
	gpio-reset = <&gpio 21 GPIO_ACTIVE_HIGH>;

	wifi@1814,3592 {
		compatible = "pci1814,3592";
		reg = <0x7000 0 0 0 0>;
		ralink,mtd-eeprom = <&boardconfig 0x410>;
		ralink,mtd-eeprom-swap;
		mtd-mac-address = <&boardconfig 0x16>;
		mtd-mac-address-increment = <1>;
	};
};
