From d91be214849b0efa6a75ce4a2d1fb469c26b416b Mon Sep 17 00:00:00 2001
From: notro <notro@tronnes.org>
Date: Thu, 10 Jul 2014 13:59:47 +0200
Subject: [PATCH] pinctrl-bcm2835: Set base to 0 give expected gpio
 numbering

Signed-off-by: Noralf Tronnes <notro@tronnes.org>
---
 drivers/pinctrl/bcm/pinctrl-bcm2835.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/pinctrl/bcm/pinctrl-bcm2835.c
+++ b/drivers/pinctrl/bcm/pinctrl-bcm2835.c
@@ -350,7 +350,7 @@ static const struct gpio_chip bcm2835_gp
 	.get = bcm2835_gpio_get,
 	.set = bcm2835_gpio_set,
 	.set_config = gpiochip_generic_config,
-	.base = -1,
+	.base = 0,
 	.ngpio = BCM2835_NUM_GPIOS,
 	.can_sleep = false,
 };
