// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include <dt-bindings/leds/common.h>

#include "ar9344_dlink_dir-8x5.dtsi"

/ {
	model = "D-LINK DIR-825 C1";
	compatible = "dlink,dir-825-c1", "qca,ar9344";

	aliases {
		led-boot = &led_power_orange;
		led-failsafe = &led_power_orange;
		led-running = &led_power_blue;
		led-upgrade = &led_power_orange;
	};

	leds {
		compatible = "gpio-leds";

		pinctrl-names = "default";
		pinctrl-0 = <&enable_gpio_11>;

		led_power_blue: power_blue {
			function = LED_FUNCTION_POWER;
			color = <LED_COLOR_ID_BLUE>;
			gpios = <&gpio 22 GPIO_ACTIVE_LOW>;
		};

		usb {
			function = LED_FUNCTION_USB;
			color = <LED_COLOR_ID_BLUE>;
			gpios = <&gpio 11 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "usbport";
			trigger-sources = <&hub_port>;
		};

		wan_blue {
			function = LED_FUNCTION_WAN;
			color = <LED_COLOR_ID_BLUE>;
			gpios = <&gpio 18 GPIO_ACTIVE_LOW>;
		};

		wlan2g {
			label = "blue:wlan2g";
			gpios = <&gpio 13 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0tpt";
		};

		wps {
			function = LED_FUNCTION_WPS;
			color = <LED_COLOR_ID_BLUE>;
			gpios = <&gpio 15 GPIO_ACTIVE_LOW>;
		};

		led_power_orange: power_orange {
			function = LED_FUNCTION_POWER;
			color = <LED_COLOR_ID_ORANGE>;
			gpios = <&gpio 14 GPIO_ACTIVE_LOW>;
		};

		wan_orange {
			function = LED_FUNCTION_WAN;
			color = <LED_COLOR_ID_ORANGE>;
			gpios = <&gpio 19 GPIO_ACTIVE_LOW>;
		};
	};

	leds-ath9k {
		compatible = "gpio-leds";

		wlan5g {
			label = "blue:wlan5g";
			gpios = <&ath9k 0 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy1tpt";
		};
	};
};

&pinmux {
	enable_gpio_11: pinmux_enable_gpio_11 {
		pinctrl-single,bits = <0x8 0x0 0xff000000>;
	};
};
