#include "qcom-ipq8064-v2.0.dtsi"

#include <dt-bindings/input/input.h>
#include <dt-bindings/soc/qcom,tcsr.h>

/ {
	model = "Edgecore ECW5410";
	compatible = "edgecore,ecw5410", "qcom,ipq8064";

	reserved-memory {
		nss@40000000 {
			reg = <0x40000000 0x1000000>;
			no-map;
		};

		smem: smem@41000000 {
			reg = <0x41000000 0x200000>;
			no-map;
		};

		wifi_dump@44000000 {
			reg = <0x44000000 0x600000>;
			no-map;
		};
	};

	cpus {
		idle-states {
			CPU_SPC: spc {
				status = "disabled";
			};
		};
	};

	aliases {
		serial1 = &gsbi1_serial;
		ethernet0 = &gmac2;
		ethernet1 = &gmac3;

		led-boot = &led_power_green;
		led-failsafe = &led_power_red;
		led-running = &led_power_green;
		led-upgrade = &led_power_green;
	};

	chosen {
		bootargs-append = " console=ttyMSM0,115200n8 root=/dev/ubiblock0_1";
	};

	keys {
		compatible = "gpio-keys";
		pinctrl-0 = <&button_pins>;
		pinctrl-names = "default";

		reset {
			label = "reset";
			gpios = <&qcom_pinmux 25 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
			debounce-interval = <60>;
			wakeup-source;
		};
	};

	leds {
		compatible = "gpio-leds";
		pinctrl-0 = <&led_pins>;
		pinctrl-names = "default";

		led_power_green: power_green {
			label = "green:power";
			gpios = <&qcom_pinmux 16 GPIO_ACTIVE_HIGH>;
		};

		wlan2g_green {
			label = "green:wlan2g";
			gpios = <&qcom_pinmux 23 GPIO_ACTIVE_LOW>;
		};

		wlan2g_yellow {
			label = "yellow:wlan2g";
			gpios = <&qcom_pinmux 24 GPIO_ACTIVE_LOW>;
		};

		wlan5g_green {
			label = "green:wlan5g";
			gpios = <&qcom_pinmux 26 GPIO_ACTIVE_LOW>;
		};

		led_power_red: power_red {
			label = "red:power";
			gpios = <&qcom_pinmux 28 GPIO_ACTIVE_LOW>;
		};

		wlan5g_yellow {
			label = "yellow:wlan5g";
			gpios = <&qcom_pinmux 59 GPIO_ACTIVE_LOW>;
		};
	};
};


&qcom_pinmux {
	spi_pins: spi_pins {
		mux {
			pins = "gpio18", "gpio19";
			function = "gsbi5";
			drive-strength = <10>;
			bias-pull-down;
		};

		clk {
			pins = "gpio21";
			function = "gsbi5";
			drive-strength = <12>;
			bias-pull-down;
		};

		cs {
			pins = "gpio20";
			function = "gpio";
			drive-strength = <10>;
			bias-pull-up;
		};
	};

	led_pins: led_pins {
		mux {
			pins = "gpio16", "gpio23", "gpio24", "gpio26",
				   "gpio28", "gpio59";
			function = "gpio";
			drive-strength = <2>;
			bias-pull-up;
		};
	};

	button_pins: button_pins {
		mux {
			pins = "gpio25";
			function = "gpio";
			drive-strength = <2>;
			bias-pull-up;
		};
	};

	uart1_pins: uart1_pins {
		mux {
			pins = "gpio51", "gpio52", "gpio53", "gpio54";
			function = "gsbi1";
			drive-strength = <12>;
			bias-none;
		};
	};
};

&gsbi1 {
	qcom,mode = <GSBI_PROT_UART_W_FC>;
	status = "okay";

	serial@12450000 {
		status = "okay";

		pinctrl-0 = <&uart1_pins>;
		pinctrl-names = "default";
	};
};

&gsbi5 {
	qcom,mode = <GSBI_PROT_SPI>;
	status = "okay";

	spi4: spi@1a280000 {
		status = "okay";
		spi-max-frequency = <50000000>;

		pinctrl-0 = <&spi_pins>;
		pinctrl-names = "default";

		cs-gpios = <&qcom_pinmux 20 GPIO_ACTIVE_HIGH>;

		m25p80@0 {
			compatible = "jedec,spi-nor";
			#address-cells = <1>;
			#size-cells = <1>;
			spi-max-frequency = <50000000>;
			reg = <0>;

			partitions {
				compatible = "qcom,smem-part";
			};
		};
	};
};

&hs_phy_0 {		/* USB3 port 0 HS phy */
	status = "okay";
};

&hs_phy_1 {		/* USB3 port 1 HS phy */
	status = "okay";
};

&ss_phy_0 {		/* USB3 port 0 SS phy */
	status = "okay";
};

&ss_phy_1 {		/* USB3 port 1 SS phy */
	status = "okay";
};

&usb3_0 {
	status = "okay";
};

&usb3_1 {
	status = "okay";
};

&pcie1 {
	status = "okay";

	/delete-property/ pinctrl-0;
	/delete-property/ pinctrl-names;
	/delete-property/ perst-gpios;

	bridge@0,0 {
		reg = <0x00000000 0 0 0 0>;
		#address-cells = <3>;
		#size-cells = <2>;
		ranges;

		wifi@1,0 {
			compatible = "qcom,ath10k";
			status = "okay";
			reg = <0x00010000 0 0 0 0>;
			qcom,ath10k-calibration-variant = "Edgecore-ECW5410-L";
		};
	};
};

&pcie2 {
	status = "okay";

	/delete-property/ pinctrl-0;
	/delete-property/ pinctrl-names;
	/delete-property/ perst-gpios;

	bridge@0,0 {
		reg = <0x00000000 0 0 0 0>;
		#address-cells = <3>;
		#size-cells = <2>;
		ranges;

		wifi@1,0 {
			compatible = "qcom,ath10k";
			status = "okay";
			reg = <0x00010000 0 0 0 0>;
			qcom,ath10k-calibration-variant = "Edgecore-ECW5410-L";
		};
	};
};

&nand {
	status = "okay";

	pinctrl-0 = <&nand_pins>;
	pinctrl-names = "default";

	nand@0 {
		compatible = "qcom,nandcs";

		reg = <0>;

		nand-ecc-strength = <4>;
		nand-bus-width = <8>;
		nand-ecc-step-size = <512>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			rootfs1@0 {
				label = "rootfs1";
				reg = <0x0000000 0x4000000>;
			};

			rootfs2@4000000 {
				label = "rootfs2";
				reg = <0x4000000 0x4000000>;
			};
		};
	};
};

&mdio0 {
	status = "okay";

	pinctrl-0 = <&mdio0_pins>;
	pinctrl-names = "default";

	phy0: ethernet-phy@0 {
		reg = <0>;
	};

	phy1: ethernet-phy@1 {
		reg = <1>;
	};
};

&gmac2 {
	status = "okay";

	qcom,id = <2>;
	mdiobus = <&mdio0>;

	phy-mode = "sgmii";
	phy-handle = <&phy1>;
};

&gmac3 {
	status = "okay";

	qcom,id = <3>;
	mdiobus = <&mdio0>;

	phy-mode = "sgmii";
	phy-handle = <&phy0>;
};

&adm_dma {
	status = "okay";
};
