From 7acd8ef92e8789e10b5d736d73cea3b625087f26 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Pali=20Roh=C3=A1r?= <pali@kernel.org>
Date: Wed, 8 Dec 2021 06:07:44 +0100
Subject: [PATCH] PCI: aardvark: Add support for PME interrupts
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Currently enabling PCI_EXP_RTSTA_PME bit in PCI_EXP_RTCTL register does
nothing. This is because PCIe PME driver expects to receive PCIe interrupt
defined in PCI_EXP_FLAGS_IRQ register, but aardvark hardware does not
trigger PCIe INTx/MSI interrupt for PME event, rather it triggers custom
aardvark interrupt which this driver is not processing yet.

Fix this issue by handling PME interrupt in advk_pcie_handle_int() and
chaining it to PCIe interrupt 0 with generic_handle_domain_irq() (since
aardvark sets PCI_EXP_FLAGS_IRQ to zero). With this change PCIe PME driver
finally starts receiving PME interrupt.

Signed-off-by: Pali Rohár <pali@kernel.org>
Signed-off-by: Marek Behún <kabel@kernel.org>
---
 drivers/pci/controller/pci-aardvark.c | 13 +++++++++++++
 1 file changed, 13 insertions(+)

--- a/drivers/pci/controller/pci-aardvark.c
+++ b/drivers/pci/controller/pci-aardvark.c
@@ -1488,6 +1488,19 @@ static void advk_pcie_handle_int(struct
 	isr1_mask = advk_readl(pcie, PCIE_ISR1_MASK_REG);
 	isr1_status = isr1_val & ((~isr1_mask) & PCIE_ISR1_ALL_MASK);
 
+	/* Process PME interrupt */
+	if (isr0_status & PCIE_MSG_PM_PME_MASK) {
+		/*
+		 * Do not clear PME interrupt bit in ISR0, it is cleared by IRQ
+		 * receiver by writing to the PCI_EXP_RTSTA register of emulated
+		 * root bridge. Aardvark HW returns zero for PCI_EXP_FLAGS_IRQ,
+		 * so use PCIe interrupt 0.
+		 */
+		virq = irq_find_mapping(pcie->irq_domain, 0);
+		if (generic_handle_irq(virq) == -EINVAL)
+			dev_err_ratelimited(&pcie->pdev->dev, "unhandled PME IRQ\n");
+	}
+
 	/* Process ERR interrupt */
 	if (isr0_status & PCIE_ISR0_ERR_MASK) {
 		advk_writel(pcie, PCIE_ISR0_ERR_MASK, PCIE_ISR0_REG);
