From fd577b41421bc24e2d04cab96d387301b649eb14 Mon Sep 17 00:00:00 2001
From: Florian Fainelli <f.fainelli@gmail.com>
Date: Mon, 9 Nov 2020 17:20:17 -0800
Subject: [PATCH] ARM: dts: BCM5301X: Provide defaults ports container node
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Provide an empty 'ports' container node with the correct #address-cells
and #size-cells properties. This silences the following warning:

arch/arm/boot/dts/bcm4708-asus-rt-ac56u.dt.yaml:
ethernet-switch@18007000: 'oneOf' conditional failed, one must be fixed:
        'ports' is a required property
        'ethernet-ports' is a required property
        From schema:
Documentation/devicetree/bindings/net/dsa/b53.yaml

Acked-by: Rafał Miłecki <rafal@milecki.pl>
Signed-off-by: Florian Fainelli <f.fainelli@gmail.com>
---
 arch/arm/boot/dts/bcm4708-luxul-xap-1510.dts     | 3 ---
 arch/arm/boot/dts/bcm4708-luxul-xwc-1000.dts     | 3 ---
 arch/arm/boot/dts/bcm4708-smartrg-sr400ac.dts    | 3 ---
 arch/arm/boot/dts/bcm47081-luxul-xap-1410.dts    | 3 ---
 arch/arm/boot/dts/bcm47081-luxul-xwr-1200.dts    | 3 ---
 arch/arm/boot/dts/bcm47094-linksys-panamera.dts  | 3 ---
 arch/arm/boot/dts/bcm47094-luxul-xap-1610.dts    | 3 ---
 arch/arm/boot/dts/bcm47094-luxul-xwc-2000.dts    | 3 ---
 arch/arm/boot/dts/bcm47094-luxul-xwr-3100.dts    | 3 ---
 arch/arm/boot/dts/bcm47094-luxul-xwr-3150-v1.dts | 3 ---
 arch/arm/boot/dts/bcm5301x.dtsi                  | 4 ++++
 arch/arm/boot/dts/bcm953012er.dts                | 3 ---
 12 files changed, 4 insertions(+), 33 deletions(-)

--- a/arch/arm/boot/dts/bcm4708-luxul-xap-1510.dts
+++ b/arch/arm/boot/dts/bcm4708-luxul-xap-1510.dts
@@ -61,9 +61,6 @@
 	status = "okay";
 
 	ports {
-		#address-cells = <1>;
-		#size-cells = <0>;
-
 		port@0 {
 			reg = <0>;
 			label = "poe";
--- a/arch/arm/boot/dts/bcm4708-luxul-xwc-1000.dts
+++ b/arch/arm/boot/dts/bcm4708-luxul-xwc-1000.dts
@@ -68,9 +68,6 @@
 	status = "okay";
 
 	ports {
-		#address-cells = <1>;
-		#size-cells = <0>;
-
 		port@4 {
 			reg = <4>;
 			label = "lan";
--- a/arch/arm/boot/dts/bcm4708-smartrg-sr400ac.dts
+++ b/arch/arm/boot/dts/bcm4708-smartrg-sr400ac.dts
@@ -122,9 +122,6 @@
 	status = "okay";
 
 	ports {
-		#address-cells = <1>;
-		#size-cells = <0>;
-
 		port@0 {
 			reg = <0>;
 			label = "lan4";
--- a/arch/arm/boot/dts/bcm47081-luxul-xap-1410.dts
+++ b/arch/arm/boot/dts/bcm47081-luxul-xap-1410.dts
@@ -61,9 +61,6 @@
 	status = "okay";
 
 	ports {
-		#address-cells = <1>;
-		#size-cells = <0>;
-
 		port@4 {
 			reg = <4>;
 			label = "poe";
--- a/arch/arm/boot/dts/bcm47081-luxul-xwr-1200.dts
+++ b/arch/arm/boot/dts/bcm47081-luxul-xwr-1200.dts
@@ -109,9 +109,6 @@
 	status = "okay";
 
 	ports {
-		#address-cells = <1>;
-		#size-cells = <0>;
-
 		port@0 {
 			reg = <0>;
 			label = "lan4";
--- a/arch/arm/boot/dts/bcm47094-linksys-panamera.dts
+++ b/arch/arm/boot/dts/bcm47094-linksys-panamera.dts
@@ -201,9 +201,6 @@
 	dsa,member = <0 0>;
 
 	ports {
-		#address-cells = <1>;
-		#size-cells = <0>;
-
 		port@1 {
 			reg = <1>;
 			label = "lan7";
--- a/arch/arm/boot/dts/bcm47094-luxul-xap-1610.dts
+++ b/arch/arm/boot/dts/bcm47094-luxul-xap-1610.dts
@@ -59,9 +59,6 @@
 	status = "okay";
 
 	ports {
-		#address-cells = <1>;
-		#size-cells = <0>;
-
 		port@0 {
 			reg = <0>;
 			label = "poe";
--- a/arch/arm/boot/dts/bcm47094-luxul-xwc-2000.dts
+++ b/arch/arm/boot/dts/bcm47094-luxul-xwc-2000.dts
@@ -57,9 +57,6 @@
 	status = "okay";
 
 	ports {
-		#address-cells = <1>;
-		#size-cells = <0>;
-
 		port@0 {
 			reg = <0>;
 			label = "lan";
--- a/arch/arm/boot/dts/bcm47094-luxul-xwr-3100.dts
+++ b/arch/arm/boot/dts/bcm47094-luxul-xwr-3100.dts
@@ -108,9 +108,6 @@
 	status = "okay";
 
 	ports {
-		#address-cells = <1>;
-		#size-cells = <0>;
-
 		port@0 {
 			reg = <0>;
 			label = "lan4";
--- a/arch/arm/boot/dts/bcm47094-luxul-xwr-3150-v1.dts
+++ b/arch/arm/boot/dts/bcm47094-luxul-xwr-3150-v1.dts
@@ -83,9 +83,6 @@
 	status = "okay";
 
 	ports {
-		#address-cells = <1>;
-		#size-cells = <0>;
-
 		port@0 {
 			reg = <0>;
 			label = "lan4";
--- a/arch/arm/boot/dts/bcm5301x.dtsi
+++ b/arch/arm/boot/dts/bcm5301x.dtsi
@@ -492,6 +492,10 @@
 		status = "disabled";
 
 		/* ports are defined in board DTS */
+		ports {
+			#address-cells = <1>;
+			#size-cells = <0>;
+		};
 	};
 
 	rng: rng@18004000 {
--- a/arch/arm/boot/dts/bcm953012er.dts
+++ b/arch/arm/boot/dts/bcm953012er.dts
@@ -69,9 +69,6 @@
 	status = "okay";
 
 	ports {
-		#address-cells = <1>;
-		#size-cells = <0>;
-
 		port@0 {
 			reg = <0>;
 			label = "port0";
