From 201880cacf1498dd4c6749780163157148d0445d Mon Sep 17 00:00:00 2001
From: Weijie Gao <weijie.gao@mediatek.com>
Date: Wed, 31 Aug 2022 19:04:57 +0800
Subject: [PATCH 21/32] pinctrl: mediatek: add pinctrl driver for MT7986 SoC

This patch adds pinctrl and gpio support for MT7986 SoC

Reviewed-by: Simon Glass <sjg@chromium.org>
Signed-off-by: Weijie Gao <weijie.gao@mediatek.com>
---
 drivers/pinctrl/mediatek/Kconfig          |   4 +
 drivers/pinctrl/mediatek/Makefile         |   1 +
 drivers/pinctrl/mediatek/pinctrl-mt7986.c | 775 ++++++++++++++++++++++
 3 files changed, 780 insertions(+)
 create mode 100644 drivers/pinctrl/mediatek/pinctrl-mt7986.c

--- a/drivers/pinctrl/mediatek/Kconfig
+++ b/drivers/pinctrl/mediatek/Kconfig
@@ -20,6 +20,10 @@ config PINCTRL_MT7981
 	bool "MT7981 SoC pinctrl driver"
 	select PINCTRL_MTK
 
+config PINCTRL_MT7986
+	bool "MT7986 SoC pinctrl driver"
+	select PINCTRL_MTK
+
 config PINCTRL_MT8512
 	bool "MT8512 SoC pinctrl driver"
 	select PINCTRL_MTK
--- a/drivers/pinctrl/mediatek/Makefile
+++ b/drivers/pinctrl/mediatek/Makefile
@@ -7,6 +7,7 @@ obj-$(CONFIG_PINCTRL_MT7622) += pinctrl-
 obj-$(CONFIG_PINCTRL_MT7623) += pinctrl-mt7623.o
 obj-$(CONFIG_PINCTRL_MT7629) += pinctrl-mt7629.o
 obj-$(CONFIG_PINCTRL_MT7981) += pinctrl-mt7981.o
+obj-$(CONFIG_PINCTRL_MT7986) += pinctrl-mt7986.o
 obj-$(CONFIG_PINCTRL_MT8512) += pinctrl-mt8512.o
 obj-$(CONFIG_PINCTRL_MT8516) += pinctrl-mt8516.o
 obj-$(CONFIG_PINCTRL_MT8518) += pinctrl-mt8518.o
--- /dev/null
+++ b/drivers/pinctrl/mediatek/pinctrl-mt7986.c
@@ -0,0 +1,775 @@
+// SPDX-License-Identifier: GPL-2.0
+/*
+ * The MT7986 driver based on Linux generic pinctrl binding.
+ *
+ * Copyright (C) 2022 MediaTek Inc.
+ * Author: Sam Shih <sam.shih@mediatek.com>
+ */
+
+#include <dm.h>
+#include "pinctrl-mtk-common.h"
+
+#define MT7986_TYPE0_PIN(_number, _name)	\
+	MTK_TYPED_PIN(_number, _name, DRV_GRP4, IO_TYPE_GRP0)
+
+#define MT7986_TYPE1_PIN(_number, _name)	\
+	MTK_TYPED_PIN(_number, _name, DRV_GRP4, IO_TYPE_GRP1)
+
+#define PIN_FIELD_GPIO(_s_pin, _e_pin, _s_addr, _x_addrs, _s_bit, _x_bits)	\
+	PIN_FIELD_BASE_CALC(_s_pin, _e_pin, GPIO_BASE, _s_addr, _x_addrs,	\
+			    _s_bit, _x_bits, 32, 0)
+
+#define PIN_FIELD_BASE(_s_pin, _e_pin, _i_base, _s_addr, _x_addrs, _s_bit,	\
+		       _x_bits)							\
+	PIN_FIELD_BASE_CALC(_s_pin, _e_pin, _i_base, _s_addr, _x_addrs, _s_bit,	\
+	_x_bits, 32, 0)
+
+/**
+ * enum - Locking variants of the iocfg bases
+ *
+ * MT7986 have multiple bases to program pin configuration listed as the below:
+ * iocfg_rt:0x11c30000, iocfg_rb:0x11c40000, iocfg_lt:0x11e20000,
+ * iocfg_lb:0x11e30000, iocfg_tr:0x11f00000, iocfg_tl:0x11f10000,
+ * _i_based could be used to indicate what base the pin should be mapped into.
+ *
+ * Each iocfg register base control different group of pads on the SoC
+ *
+ *
+ *  chip carrier
+ *
+ *      A  B  C  D  E  F  G  H
+ *    +------------------------+
+ *  8 | o  o  o  o  o  o  o  o |
+ *  7 | o  o  o  o  o  o  o  o |
+ *  6 | o  o  o  o  o  o  o  o |
+ *  5 | o  o  o  o  o  o  o  o |
+ *  4 | o  o  o  o  o  o  o  o |
+ *  3 | o  o  o  o  o  o  o  o |
+ *  2 | o  o  o  o  o  o  o  o |
+ *  1 | o  o  o  o  o  o  o  o |
+ *    +------------------------+
+ *
+ *  inside Chip carrier
+ *
+ *      A  B  C  D  E  F  G  H
+ *    +------------------------+
+ *  8 |                        |
+ *  7 |        TL  TR          |
+ *  6 |      +---------+       |
+ *  5 |   LT |         | RT    |
+ *  4 |      |         |       |
+ *  3 |   LB |         | RB    |
+ *  2 |      +---------+       |
+ *  1 |                        |
+ *    +------------------------+
+ *
+ */
+
+enum {
+	GPIO_BASE,
+	IOCFG_RT_BASE,
+	IOCFG_RB_BASE,
+	IOCFG_LT_BASE,
+	IOCFG_LB_BASE,
+	IOCFG_TR_BASE,
+	IOCFG_TL_BASE,
+};
+
+static const char *const mt7986_pinctrl_register_base_names[] = {
+	"gpio", "iocfg_rt", "iocfg_rb", "iocfg_lt", "iocfg_lb", "iocfg_tr",
+	"iocfg_tl",
+};
+
+static const struct mtk_pin_field_calc mt7986_pin_mode_range[] = {
+	PIN_FIELD_GPIO(0, 100, 0x300, 0x10, 0, 4),
+};
+
+static const struct mtk_pin_field_calc mt7986_pin_dir_range[] = {
+	PIN_FIELD_GPIO(0, 100, 0x0, 0x10, 0, 1),
+};
+
+static const struct mtk_pin_field_calc mt7986_pin_di_range[] = {
+	PIN_FIELD_GPIO(0, 100, 0x200, 0x10, 0, 1),
+};
+
+static const struct mtk_pin_field_calc mt7986_pin_do_range[] = {
+	PIN_FIELD_GPIO(0, 100, 0x100, 0x10, 0, 1),
+};
+
+static const struct mtk_pin_field_calc mt7986_pin_ies_range[] = {
+	PIN_FIELD_BASE(0, 0, IOCFG_RB_BASE, 0x40, 0x10, 17, 1),
+	PIN_FIELD_BASE(1, 2, IOCFG_LT_BASE, 0x20, 0x10, 10, 1),
+	PIN_FIELD_BASE(3, 4, IOCFG_LB_BASE, 0x20, 0x10, 0, 1),
+	PIN_FIELD_BASE(5, 6, IOCFG_RB_BASE, 0x40, 0x10, 0, 1),
+	PIN_FIELD_BASE(7, 10, IOCFG_LT_BASE, 0x20, 0x10, 0, 1),
+	PIN_FIELD_BASE(11, 14, IOCFG_RB_BASE, 0x40, 0x10, 8, 1),
+	PIN_FIELD_BASE(15, 20, IOCFG_RB_BASE, 0x40, 0x10, 2, 1),
+	PIN_FIELD_BASE(21, 23, IOCFG_RT_BASE, 0x30, 0x10, 12, 1),
+	PIN_FIELD_BASE(24, 24, IOCFG_RT_BASE, 0x30, 0x10, 18, 1),
+	PIN_FIELD_BASE(25, 25, IOCFG_RT_BASE, 0x30, 0x10, 17, 1),
+	PIN_FIELD_BASE(26, 27, IOCFG_RT_BASE, 0x30, 0x10, 15, 1),
+	PIN_FIELD_BASE(28, 29, IOCFG_RT_BASE, 0x30, 0x10, 19, 1),
+	PIN_FIELD_BASE(30, 30, IOCFG_RT_BASE, 0x30, 0x10, 23, 1),
+	PIN_FIELD_BASE(31, 31, IOCFG_RT_BASE, 0x30, 0x10, 22, 1),
+	PIN_FIELD_BASE(32, 32, IOCFG_RT_BASE, 0x30, 0x10, 21, 1),
+	PIN_FIELD_BASE(33, 33, IOCFG_LT_BASE, 0x20, 0x10, 4, 1),
+	PIN_FIELD_BASE(34, 34, IOCFG_LT_BASE, 0x20, 0x10, 8, 1),
+	PIN_FIELD_BASE(35, 35, IOCFG_LT_BASE, 0x20, 0x10, 7, 1),
+	PIN_FIELD_BASE(36, 37, IOCFG_LT_BASE, 0x20, 0x10, 5, 1),
+	PIN_FIELD_BASE(38, 38, IOCFG_LT_BASE, 0x20, 0x10, 9, 1),
+	PIN_FIELD_BASE(39, 40, IOCFG_RB_BASE, 0x40, 0x10, 18, 1),
+	PIN_FIELD_BASE(41, 41, IOCFG_RB_BASE, 0x40, 0x10, 12, 1),
+	PIN_FIELD_BASE(42, 43, IOCFG_RB_BASE, 0x40, 0x10, 22, 1),
+	PIN_FIELD_BASE(44, 45, IOCFG_RB_BASE, 0x40, 0x10, 20, 1),
+	PIN_FIELD_BASE(46, 47, IOCFG_RB_BASE, 0x40, 0x10, 26, 1),
+	PIN_FIELD_BASE(48, 49, IOCFG_RB_BASE, 0x40, 0x10, 24, 1),
+	PIN_FIELD_BASE(50, 57, IOCFG_RT_BASE, 0x30, 0x10, 2, 1),
+	PIN_FIELD_BASE(58, 58, IOCFG_RT_BASE, 0x30, 0x10, 1, 1),
+	PIN_FIELD_BASE(59, 59, IOCFG_RT_BASE, 0x30, 0x10, 0, 1),
+	PIN_FIELD_BASE(60, 61, IOCFG_RT_BASE, 0x30, 0x10, 10, 1),
+	PIN_FIELD_BASE(62, 62, IOCFG_RB_BASE, 0x40, 0x10, 15, 1),
+	PIN_FIELD_BASE(63, 63, IOCFG_RB_BASE, 0x40, 0x10, 14, 1),
+	PIN_FIELD_BASE(64, 64, IOCFG_RB_BASE, 0x40, 0x10, 13, 1),
+	PIN_FIELD_BASE(65, 65, IOCFG_RB_BASE, 0x40, 0x10, 16, 1),
+	PIN_FIELD_BASE(66, 68, IOCFG_LB_BASE, 0x20, 0x10, 2, 1),
+	PIN_FIELD_BASE(69, 69, IOCFG_TR_BASE, 0x30, 0x10, 1, 1),
+	PIN_FIELD_BASE(70, 70, IOCFG_TR_BASE, 0x30, 0x10, 0, 1),
+	PIN_FIELD_BASE(71, 71, IOCFG_TR_BASE, 0x30, 0x10, 16, 1),
+	PIN_FIELD_BASE(72, 73, IOCFG_TR_BASE, 0x30, 0x10, 14, 1),
+	PIN_FIELD_BASE(74, 74, IOCFG_TR_BASE, 0x30, 0x10, 4, 1),
+	PIN_FIELD_BASE(75, 77, IOCFG_TR_BASE, 0x30, 0x10, 6, 1),
+	PIN_FIELD_BASE(78, 79, IOCFG_TR_BASE, 0x30, 0x10, 2, 1),
+	PIN_FIELD_BASE(80, 84, IOCFG_TR_BASE, 0x30, 0x10, 9, 1),
+	PIN_FIELD_BASE(85, 85, IOCFG_TR_BASE, 0x30, 0x10, 5, 1),
+	PIN_FIELD_BASE(86, 86, IOCFG_TL_BASE, 0x30, 0x10, 1, 1),
+	PIN_FIELD_BASE(87, 87, IOCFG_TL_BASE, 0x30, 0x10, 0, 1),
+	PIN_FIELD_BASE(88, 88, IOCFG_TL_BASE, 0x30, 0x10, 14, 1),
+	PIN_FIELD_BASE(89, 90, IOCFG_TL_BASE, 0x30, 0x10, 12, 1),
+	PIN_FIELD_BASE(91, 94, IOCFG_TL_BASE, 0x30, 0x10, 4, 1),
+	PIN_FIELD_BASE(95, 96, IOCFG_TL_BASE, 0x30, 0x10, 2, 1),
+	PIN_FIELD_BASE(97, 100, IOCFG_TL_BASE, 0x30, 0x10, 8, 1),
+};
+
+static const struct mtk_pin_field_calc mt7986_pin_smt_range[] = {
+	PIN_FIELD_BASE(0, 0, IOCFG_RB_BASE, 0xf0, 0x10, 17, 1),
+	PIN_FIELD_BASE(1, 2, IOCFG_LT_BASE, 0x90, 0x10, 10, 1),
+	PIN_FIELD_BASE(3, 4, IOCFG_LB_BASE, 0x90, 0x10, 0, 1),
+	PIN_FIELD_BASE(5, 6, IOCFG_RB_BASE, 0xf0, 0x10, 0, 1),
+	PIN_FIELD_BASE(7, 10, IOCFG_LT_BASE, 0x90, 0x10, 0, 1),
+	PIN_FIELD_BASE(11, 14, IOCFG_RB_BASE, 0xf0, 0x10, 8, 1),
+	PIN_FIELD_BASE(15, 20, IOCFG_RB_BASE, 0xf0, 0x10, 2, 1),
+	PIN_FIELD_BASE(21, 23, IOCFG_RT_BASE, 0xc0, 0x10, 12, 1),
+	PIN_FIELD_BASE(24, 24, IOCFG_RT_BASE, 0xc0, 0x10, 18, 1),
+	PIN_FIELD_BASE(25, 25, IOCFG_RT_BASE, 0xc0, 0x10, 17, 1),
+	PIN_FIELD_BASE(26, 27, IOCFG_RT_BASE, 0xc0, 0x10, 15, 1),
+	PIN_FIELD_BASE(28, 29, IOCFG_RT_BASE, 0xc0, 0x10, 19, 1),
+	PIN_FIELD_BASE(30, 30, IOCFG_RT_BASE, 0xc0, 0x10, 23, 1),
+	PIN_FIELD_BASE(31, 31, IOCFG_RT_BASE, 0xc0, 0x10, 22, 1),
+	PIN_FIELD_BASE(32, 32, IOCFG_RT_BASE, 0xc0, 0x10, 21, 1),
+	PIN_FIELD_BASE(33, 33, IOCFG_LT_BASE, 0x90, 0x10, 4, 1),
+	PIN_FIELD_BASE(34, 34, IOCFG_LT_BASE, 0x90, 0x10, 8, 1),
+	PIN_FIELD_BASE(35, 35, IOCFG_LT_BASE, 0x90, 0x10, 7, 1),
+	PIN_FIELD_BASE(36, 37, IOCFG_LT_BASE, 0x90, 0x10, 5, 1),
+	PIN_FIELD_BASE(38, 38, IOCFG_LT_BASE, 0x90, 0x10, 9, 1),
+	PIN_FIELD_BASE(39, 40, IOCFG_RB_BASE, 0xf0, 0x10, 18, 1),
+	PIN_FIELD_BASE(41, 41, IOCFG_RB_BASE, 0xf0, 0x10, 12, 1),
+	PIN_FIELD_BASE(42, 43, IOCFG_RB_BASE, 0xf0, 0x10, 22, 1),
+	PIN_FIELD_BASE(44, 45, IOCFG_RB_BASE, 0xf0, 0x10, 20, 1),
+	PIN_FIELD_BASE(46, 47, IOCFG_RB_BASE, 0xf0, 0x10, 26, 1),
+	PIN_FIELD_BASE(48, 49, IOCFG_RB_BASE, 0xf0, 0x10, 24, 1),
+	PIN_FIELD_BASE(50, 57, IOCFG_RT_BASE, 0xc0, 0x10, 2, 1),
+	PIN_FIELD_BASE(58, 58, IOCFG_RT_BASE, 0xc0, 0x10, 1, 1),
+	PIN_FIELD_BASE(59, 59, IOCFG_RT_BASE, 0xc0, 0x10, 0, 1),
+	PIN_FIELD_BASE(60, 61, IOCFG_RT_BASE, 0xc0, 0x10, 10, 1),
+	PIN_FIELD_BASE(62, 62, IOCFG_RB_BASE, 0xf0, 0x10, 15, 1),
+	PIN_FIELD_BASE(63, 63, IOCFG_RB_BASE, 0xf0, 0x10, 14, 1),
+	PIN_FIELD_BASE(64, 64, IOCFG_RB_BASE, 0xf0, 0x10, 13, 1),
+	PIN_FIELD_BASE(65, 65, IOCFG_RB_BASE, 0xf0, 0x10, 16, 1),
+	PIN_FIELD_BASE(66, 68, IOCFG_LB_BASE, 0x90, 0x10, 2, 1),
+	PIN_FIELD_BASE(69, 69, IOCFG_TR_BASE, 0x80, 0x10, 1, 1),
+	PIN_FIELD_BASE(70, 70, IOCFG_TR_BASE, 0x80, 0x10, 0, 1),
+	PIN_FIELD_BASE(71, 71, IOCFG_TR_BASE, 0x80, 0x10, 16, 1),
+	PIN_FIELD_BASE(72, 73, IOCFG_TR_BASE, 0x80, 0x10, 14, 1),
+	PIN_FIELD_BASE(74, 74, IOCFG_TR_BASE, 0x80, 0x10, 4, 1),
+	PIN_FIELD_BASE(75, 77, IOCFG_TR_BASE, 0x80, 0x10, 6, 1),
+	PIN_FIELD_BASE(78, 79, IOCFG_TR_BASE, 0x80, 0x10, 2, 1),
+	PIN_FIELD_BASE(80, 84, IOCFG_TR_BASE, 0x80, 0x10, 9, 1),
+	PIN_FIELD_BASE(85, 85, IOCFG_TR_BASE, 0x80, 0x10, 5, 1),
+	PIN_FIELD_BASE(86, 86, IOCFG_TL_BASE, 0x70, 0x10, 1, 1),
+	PIN_FIELD_BASE(87, 87, IOCFG_TL_BASE, 0x70, 0x10, 0, 1),
+	PIN_FIELD_BASE(88, 88, IOCFG_TL_BASE, 0x70, 0x10, 14, 1),
+	PIN_FIELD_BASE(89, 90, IOCFG_TL_BASE, 0x70, 0x10, 12, 1),
+	PIN_FIELD_BASE(91, 94, IOCFG_TL_BASE, 0x70, 0x10, 4, 1),
+	PIN_FIELD_BASE(95, 96, IOCFG_TL_BASE, 0x70, 0x10, 2, 1),
+	PIN_FIELD_BASE(97, 100, IOCFG_TL_BASE, 0x70, 0x10, 8, 1),
+};
+
+static const struct mtk_pin_field_calc mt7986_pin_pu_range[] = {
+	PIN_FIELD_BASE(69, 69, IOCFG_TR_BASE, 0x50, 0x10, 1, 1),
+	PIN_FIELD_BASE(70, 70, IOCFG_TR_BASE, 0x50, 0x10, 0, 1),
+	PIN_FIELD_BASE(71, 71, IOCFG_TR_BASE, 0x50, 0x10, 16, 1),
+	PIN_FIELD_BASE(72, 73, IOCFG_TR_BASE, 0x50, 0x10, 14, 1),
+	PIN_FIELD_BASE(74, 74, IOCFG_TR_BASE, 0x50, 0x10, 4, 1),
+	PIN_FIELD_BASE(75, 77, IOCFG_TR_BASE, 0x50, 0x10, 6, 1),
+	PIN_FIELD_BASE(78, 79, IOCFG_TR_BASE, 0x50, 0x10, 2, 1),
+	PIN_FIELD_BASE(80, 84, IOCFG_TR_BASE, 0x50, 0x10, 9, 1),
+	PIN_FIELD_BASE(85, 85, IOCFG_TR_BASE, 0x50, 0x10, 5, 1),
+	PIN_FIELD_BASE(86, 86, IOCFG_TL_BASE, 0x50, 0x10, 1, 1),
+	PIN_FIELD_BASE(87, 87, IOCFG_TL_BASE, 0x50, 0x10, 0, 1),
+	PIN_FIELD_BASE(88, 88, IOCFG_TL_BASE, 0x50, 0x10, 14, 1),
+	PIN_FIELD_BASE(89, 90, IOCFG_TL_BASE, 0x50, 0x10, 12, 1),
+	PIN_FIELD_BASE(91, 94, IOCFG_TL_BASE, 0x50, 0x10, 4, 1),
+	PIN_FIELD_BASE(95, 96, IOCFG_TL_BASE, 0x50, 0x10, 2, 1),
+	PIN_FIELD_BASE(97, 100, IOCFG_TL_BASE, 0x50, 0x10, 8, 1),
+};
+
+static const struct mtk_pin_field_calc mt7986_pin_pd_range[] = {
+	PIN_FIELD_BASE(69, 69, IOCFG_TR_BASE, 0x40, 0x10, 1, 1),
+	PIN_FIELD_BASE(70, 70, IOCFG_TR_BASE, 0x40, 0x10, 0, 1),
+	PIN_FIELD_BASE(71, 71, IOCFG_TR_BASE, 0x40, 0x10, 16, 1),
+	PIN_FIELD_BASE(72, 73, IOCFG_TR_BASE, 0x40, 0x10, 14, 1),
+	PIN_FIELD_BASE(74, 74, IOCFG_TR_BASE, 0x40, 0x10, 4, 1),
+	PIN_FIELD_BASE(75, 77, IOCFG_TR_BASE, 0x40, 0x10, 6, 1),
+	PIN_FIELD_BASE(78, 79, IOCFG_TR_BASE, 0x40, 0x10, 2, 1),
+	PIN_FIELD_BASE(80, 84, IOCFG_TR_BASE, 0x40, 0x10, 9, 1),
+	PIN_FIELD_BASE(85, 85, IOCFG_TR_BASE, 0x40, 0x10, 5, 1),
+	PIN_FIELD_BASE(86, 86, IOCFG_TL_BASE, 0x40, 0x10, 1, 1),
+	PIN_FIELD_BASE(87, 87, IOCFG_TL_BASE, 0x40, 0x10, 0, 1),
+	PIN_FIELD_BASE(88, 88, IOCFG_TL_BASE, 0x40, 0x10, 14, 1),
+	PIN_FIELD_BASE(89, 90, IOCFG_TL_BASE, 0x40, 0x10, 12, 1),
+	PIN_FIELD_BASE(91, 94, IOCFG_TL_BASE, 0x40, 0x10, 4, 1),
+	PIN_FIELD_BASE(95, 96, IOCFG_TL_BASE, 0x40, 0x10, 2, 1),
+	PIN_FIELD_BASE(97, 100, IOCFG_TL_BASE, 0x40, 0x10, 8, 1),
+};
+
+static const struct mtk_pin_field_calc mt7986_pin_drv_range[] = {
+	PIN_FIELD_BASE(0, 0, IOCFG_RB_BASE, 0x10, 0x10, 21, 3),
+	PIN_FIELD_BASE(1, 2, IOCFG_LT_BASE, 0x10, 0x10, 0, 3),
+	PIN_FIELD_BASE(3, 4, IOCFG_LB_BASE, 0x00, 0x10, 0, 1),
+	PIN_FIELD_BASE(5, 5, IOCFG_RB_BASE, 0x00, 0x10, 0, 3),
+	PIN_FIELD_BASE(6, 6, IOCFG_RB_BASE, 0x00, 0x10, 21, 3),
+	PIN_FIELD_BASE(7, 10, IOCFG_LT_BASE, 0x00, 0x10, 0, 3),
+	PIN_FIELD_BASE(11, 12, IOCFG_RB_BASE, 0x00, 0x10, 24, 3),
+	PIN_FIELD_BASE(13, 14, IOCFG_RB_BASE, 0x10, 0x10, 0, 3),
+	PIN_FIELD_BASE(15, 20, IOCFG_RB_BASE, 0x00, 0x10, 3, 3),
+	PIN_FIELD_BASE(21, 23, IOCFG_RT_BASE, 0x10, 0x10, 6, 3),
+	PIN_FIELD_BASE(24, 24, IOCFG_RT_BASE, 0x10, 0x10, 24, 3),
+	PIN_FIELD_BASE(25, 25, IOCFG_RT_BASE, 0x10, 0x10, 21, 3),
+	PIN_FIELD_BASE(26, 27, IOCFG_RT_BASE, 0x10, 0x10, 15, 3),
+	PIN_FIELD_BASE(28, 28, IOCFG_RT_BASE, 0x10, 0x10, 27, 3),
+	PIN_FIELD_BASE(29, 29, IOCFG_RT_BASE, 0x20, 0x10, 0, 3),
+	PIN_FIELD_BASE(30, 30, IOCFG_RT_BASE, 0x20, 0x10, 9, 3),
+	PIN_FIELD_BASE(31, 31, IOCFG_RT_BASE, 0x20, 0x10, 6, 3),
+	PIN_FIELD_BASE(32, 32, IOCFG_RT_BASE, 0x20, 0x10, 3, 3),
+	PIN_FIELD_BASE(33, 33, IOCFG_LT_BASE, 0x00, 0x10, 12, 3),
+	PIN_FIELD_BASE(34, 34, IOCFG_LT_BASE, 0x00, 0x10, 24, 3),
+	PIN_FIELD_BASE(35, 35, IOCFG_LT_BASE, 0x00, 0x10, 21, 3),
+	PIN_FIELD_BASE(36, 37, IOCFG_LT_BASE, 0x00, 0x10, 15, 3),
+	PIN_FIELD_BASE(38, 38, IOCFG_LT_BASE, 0x00, 0x10, 27, 3),
+	PIN_FIELD_BASE(39, 39, IOCFG_RB_BASE, 0x10, 0x10, 27, 3),
+	PIN_FIELD_BASE(40, 40, IOCFG_RB_BASE, 0x20, 0x10, 0, 3),
+	PIN_FIELD_BASE(41, 41, IOCFG_RB_BASE, 0x10, 0x10, 6, 3),
+	PIN_FIELD_BASE(42, 43, IOCFG_RB_BASE, 0x20, 0x10, 9, 3),
+	PIN_FIELD_BASE(44, 45, IOCFG_RB_BASE, 0x20, 0x10, 3, 3),
+	PIN_FIELD_BASE(46, 47, IOCFG_RB_BASE, 0x20, 0x10, 21, 3),
+	PIN_FIELD_BASE(48, 49, IOCFG_RB_BASE, 0x20, 0x10, 15, 3),
+	PIN_FIELD_BASE(50, 57, IOCFG_RT_BASE, 0x00, 0x10, 6, 3),
+	PIN_FIELD_BASE(58, 58, IOCFG_RT_BASE, 0x00, 0x10, 3, 3),
+	PIN_FIELD_BASE(59, 59, IOCFG_RT_BASE, 0x00, 0x10, 0, 3),
+	PIN_FIELD_BASE(60, 61, IOCFG_RT_BASE, 0x10, 0x10, 0, 3),
+	PIN_FIELD_BASE(62, 62, IOCFG_RB_BASE, 0x10, 0x10, 15, 3),
+	PIN_FIELD_BASE(63, 63, IOCFG_RB_BASE, 0x10, 0x10, 12, 3),
+	PIN_FIELD_BASE(64, 64, IOCFG_RB_BASE, 0x10, 0x10, 9, 3),
+	PIN_FIELD_BASE(65, 65, IOCFG_RB_BASE, 0x10, 0x10, 18, 3),
+	PIN_FIELD_BASE(66, 68, IOCFG_LB_BASE, 0x00, 0x10, 2, 3),
+	PIN_FIELD_BASE(69, 69, IOCFG_TR_BASE, 0x00, 0x10, 3, 3),
+	PIN_FIELD_BASE(70, 70, IOCFG_TR_BASE, 0x00, 0x10, 0, 3),
+	PIN_FIELD_BASE(71, 71, IOCFG_TR_BASE, 0x10, 0x10, 18, 3),
+	PIN_FIELD_BASE(72, 73, IOCFG_TR_BASE, 0x10, 0x10, 12, 3),
+	PIN_FIELD_BASE(74, 77, IOCFG_TR_BASE, 0x00, 0x10, 15, 3),
+	PIN_FIELD_BASE(78, 79, IOCFG_TR_BASE, 0x00, 0x10, 6, 3),
+	PIN_FIELD_BASE(80, 80, IOCFG_TR_BASE, 0x00, 0x10, 27, 3),
+	PIN_FIELD_BASE(81, 84, IOCFG_TR_BASE, 0x10, 0x10, 0, 3),
+	PIN_FIELD_BASE(85, 85, IOCFG_TR_BASE, 0x00, 0x10, 12, 3),
+	PIN_FIELD_BASE(86, 86, IOCFG_TL_BASE, 0x00, 0x10, 3, 3),
+	PIN_FIELD_BASE(87, 87, IOCFG_TL_BASE, 0x00, 0x10, 0, 3),
+	PIN_FIELD_BASE(88, 88, IOCFG_TL_BASE, 0x10, 0x10, 12, 3),
+	PIN_FIELD_BASE(89, 90, IOCFG_TL_BASE, 0x10, 0x10, 6, 3),
+	PIN_FIELD_BASE(91, 94, IOCFG_TL_BASE, 0x00, 0x10, 12, 3),
+	PIN_FIELD_BASE(95, 96, IOCFG_TL_BASE, 0x00, 0x10, 6, 3),
+	PIN_FIELD_BASE(97, 98, IOCFG_TL_BASE, 0x00, 0x10, 24, 3),
+	PIN_FIELD_BASE(99, 100, IOCFG_TL_BASE, 0x10, 0x10, 2, 3),
+};
+
+static const struct mtk_pin_field_calc mt7986_pin_pupd_range[] = {
+	PIN_FIELD_BASE(0, 0, IOCFG_RB_BASE, 0x60, 0x10, 17, 1),
+	PIN_FIELD_BASE(1, 2, IOCFG_LT_BASE, 0x30, 0x10, 10, 1),
+	PIN_FIELD_BASE(3, 4, IOCFG_LB_BASE, 0x40, 0x10, 0, 1),
+	PIN_FIELD_BASE(5, 6, IOCFG_RB_BASE, 0x60, 0x10, 0, 1),
+	PIN_FIELD_BASE(7, 10, IOCFG_LT_BASE, 0x30, 0x10, 0, 1),
+	PIN_FIELD_BASE(11, 14, IOCFG_RB_BASE, 0x60, 0x10, 8, 1),
+	PIN_FIELD_BASE(15, 20, IOCFG_RB_BASE, 0x60, 0x10, 2, 1),
+	PIN_FIELD_BASE(21, 23, IOCFG_RT_BASE, 0x40, 0x10, 12, 1),
+	PIN_FIELD_BASE(24, 24, IOCFG_RT_BASE, 0x40, 0x10, 18, 1),
+	PIN_FIELD_BASE(25, 25, IOCFG_RT_BASE, 0x40, 0x10, 17, 1),
+	PIN_FIELD_BASE(26, 27, IOCFG_RT_BASE, 0x40, 0x10, 15, 1),
+	PIN_FIELD_BASE(28, 29, IOCFG_RT_BASE, 0x40, 0x10, 19, 1),
+	PIN_FIELD_BASE(30, 30, IOCFG_RT_BASE, 0x40, 0x10, 23, 1),
+	PIN_FIELD_BASE(31, 31, IOCFG_RT_BASE, 0x40, 0x10, 22, 1),
+	PIN_FIELD_BASE(32, 32, IOCFG_RT_BASE, 0x40, 0x10, 21, 1),
+	PIN_FIELD_BASE(33, 33, IOCFG_LT_BASE, 0x30, 0x10, 4, 1),
+	PIN_FIELD_BASE(34, 34, IOCFG_LT_BASE, 0x30, 0x10, 8, 1),
+	PIN_FIELD_BASE(35, 35, IOCFG_LT_BASE, 0x30, 0x10, 7, 1),
+	PIN_FIELD_BASE(36, 37, IOCFG_LT_BASE, 0x30, 0x10, 5, 1),
+	PIN_FIELD_BASE(38, 38, IOCFG_LT_BASE, 0x30, 0x10, 9, 1),
+	PIN_FIELD_BASE(39, 40, IOCFG_RB_BASE, 0x60, 0x10, 18, 1),
+	PIN_FIELD_BASE(41, 41, IOCFG_RB_BASE, 0x60, 0x10, 12, 1),
+	PIN_FIELD_BASE(42, 43, IOCFG_RB_BASE, 0x60, 0x10, 23, 1),
+	PIN_FIELD_BASE(44, 45, IOCFG_RB_BASE, 0x60, 0x10, 21, 1),
+	PIN_FIELD_BASE(46, 47, IOCFG_RB_BASE, 0x60, 0x10, 27, 1),
+	PIN_FIELD_BASE(48, 49, IOCFG_RB_BASE, 0x60, 0x10, 25, 1),
+	PIN_FIELD_BASE(50, 57, IOCFG_RT_BASE, 0x40, 0x10, 2, 1),
+	PIN_FIELD_BASE(58, 58, IOCFG_RT_BASE, 0x40, 0x10, 1, 1),
+	PIN_FIELD_BASE(59, 59, IOCFG_RT_BASE, 0x40, 0x10, 0, 1),
+	PIN_FIELD_BASE(60, 61, IOCFG_RT_BASE, 0x40, 0x10, 10, 1),
+	PIN_FIELD_BASE(62, 62, IOCFG_RB_BASE, 0x60, 0x10, 15, 1),
+	PIN_FIELD_BASE(63, 63, IOCFG_RB_BASE, 0x60, 0x10, 14, 1),
+	PIN_FIELD_BASE(64, 64, IOCFG_RB_BASE, 0x60, 0x10, 13, 1),
+	PIN_FIELD_BASE(65, 65, IOCFG_RB_BASE, 0x60, 0x10, 16, 1),
+	PIN_FIELD_BASE(66, 68, IOCFG_LB_BASE, 0x40, 0x10, 2, 1),
+};
+
+static const struct mtk_pin_field_calc mt7986_pin_r0_range[] = {
+	PIN_FIELD_BASE(0, 0, IOCFG_RB_BASE, 0x70, 0x10, 17, 1),
+	PIN_FIELD_BASE(1, 2, IOCFG_LT_BASE, 0x40, 0x10, 10, 1),
+	PIN_FIELD_BASE(3, 4, IOCFG_LB_BASE, 0x50, 0x10, 0, 1),
+	PIN_FIELD_BASE(5, 6, IOCFG_RB_BASE, 0x70, 0x10, 0, 1),
+	PIN_FIELD_BASE(7, 10, IOCFG_LT_BASE, 0x40, 0x10, 0, 1),
+	PIN_FIELD_BASE(11, 14, IOCFG_RB_BASE, 0x70, 0x10, 8, 1),
+	PIN_FIELD_BASE(15, 20, IOCFG_RB_BASE, 0x70, 0x10, 2, 1),
+	PIN_FIELD_BASE(21, 23, IOCFG_RT_BASE, 0x50, 0x10, 12, 1),
+	PIN_FIELD_BASE(24, 24, IOCFG_RT_BASE, 0x50, 0x10, 18, 1),
+	PIN_FIELD_BASE(25, 25, IOCFG_RT_BASE, 0x50, 0x10, 17, 1),
+	PIN_FIELD_BASE(26, 27, IOCFG_RT_BASE, 0x50, 0x10, 15, 1),
+	PIN_FIELD_BASE(28, 29, IOCFG_RT_BASE, 0x50, 0x10, 19, 1),
+	PIN_FIELD_BASE(30, 30, IOCFG_RT_BASE, 0x50, 0x10, 23, 1),
+	PIN_FIELD_BASE(31, 31, IOCFG_RT_BASE, 0x50, 0x10, 22, 1),
+	PIN_FIELD_BASE(32, 32, IOCFG_RT_BASE, 0x50, 0x10, 21, 1),
+	PIN_FIELD_BASE(33, 33, IOCFG_LT_BASE, 0x40, 0x10, 4, 1),
+	PIN_FIELD_BASE(34, 34, IOCFG_LT_BASE, 0x40, 0x10, 8, 1),
+	PIN_FIELD_BASE(35, 35, IOCFG_LT_BASE, 0x40, 0x10, 7, 1),
+	PIN_FIELD_BASE(36, 37, IOCFG_LT_BASE, 0x40, 0x10, 5, 1),
+	PIN_FIELD_BASE(38, 38, IOCFG_LT_BASE, 0x40, 0x10, 9, 1),
+	PIN_FIELD_BASE(39, 40, IOCFG_RB_BASE, 0x70, 0x10, 18, 1),
+	PIN_FIELD_BASE(41, 41, IOCFG_RB_BASE, 0x70, 0x10, 12, 1),
+	PIN_FIELD_BASE(42, 43, IOCFG_RB_BASE, 0x70, 0x10, 23, 1),
+	PIN_FIELD_BASE(44, 45, IOCFG_RB_BASE, 0x70, 0x10, 21, 1),
+	PIN_FIELD_BASE(46, 47, IOCFG_RB_BASE, 0x70, 0x10, 27, 1),
+	PIN_FIELD_BASE(48, 49, IOCFG_RB_BASE, 0x70, 0x10, 25, 1),
+	PIN_FIELD_BASE(50, 57, IOCFG_RT_BASE, 0x50, 0x10, 2, 1),
+	PIN_FIELD_BASE(58, 58, IOCFG_RT_BASE, 0x50, 0x10, 1, 1),
+	PIN_FIELD_BASE(59, 59, IOCFG_RT_BASE, 0x50, 0x10, 0, 1),
+	PIN_FIELD_BASE(60, 61, IOCFG_RT_BASE, 0x50, 0x10, 10, 1),
+	PIN_FIELD_BASE(62, 62, IOCFG_RB_BASE, 0x70, 0x10, 15, 1),
+	PIN_FIELD_BASE(63, 63, IOCFG_RB_BASE, 0x70, 0x10, 14, 1),
+	PIN_FIELD_BASE(64, 64, IOCFG_RB_BASE, 0x70, 0x10, 13, 1),
+	PIN_FIELD_BASE(65, 65, IOCFG_RB_BASE, 0x70, 0x10, 16, 1),
+	PIN_FIELD_BASE(66, 68, IOCFG_LB_BASE, 0x50, 0x10, 2, 1),
+};
+
+static const struct mtk_pin_field_calc mt7986_pin_r1_range[] = {
+	PIN_FIELD_BASE(0, 0, IOCFG_RB_BASE, 0x80, 0x10, 17, 1),
+	PIN_FIELD_BASE(1, 2, IOCFG_LT_BASE, 0x50, 0x10, 10, 1),
+	PIN_FIELD_BASE(3, 4, IOCFG_LB_BASE, 0x60, 0x10, 0, 1),
+	PIN_FIELD_BASE(5, 6, IOCFG_RB_BASE, 0x80, 0x10, 0, 1),
+	PIN_FIELD_BASE(7, 10, IOCFG_LT_BASE, 0x50, 0x10, 0, 1),
+	PIN_FIELD_BASE(11, 14, IOCFG_RB_BASE, 0x80, 0x10, 8, 1),
+	PIN_FIELD_BASE(15, 20, IOCFG_RB_BASE, 0x80, 0x10, 2, 1),
+	PIN_FIELD_BASE(21, 23, IOCFG_RT_BASE, 0x60, 0x10, 12, 1),
+	PIN_FIELD_BASE(24, 24, IOCFG_RT_BASE, 0x60, 0x10, 18, 1),
+	PIN_FIELD_BASE(25, 25, IOCFG_RT_BASE, 0x60, 0x10, 17, 1),
+	PIN_FIELD_BASE(26, 27, IOCFG_RT_BASE, 0x60, 0x10, 15, 1),
+	PIN_FIELD_BASE(28, 29, IOCFG_RT_BASE, 0x60, 0x10, 19, 1),
+	PIN_FIELD_BASE(30, 30, IOCFG_RT_BASE, 0x60, 0x10, 23, 1),
+	PIN_FIELD_BASE(31, 31, IOCFG_RT_BASE, 0x60, 0x10, 22, 1),
+	PIN_FIELD_BASE(32, 32, IOCFG_RT_BASE, 0x60, 0x10, 21, 1),
+	PIN_FIELD_BASE(33, 33, IOCFG_LT_BASE, 0x50, 0x10, 4, 1),
+	PIN_FIELD_BASE(34, 34, IOCFG_LT_BASE, 0x50, 0x10, 8, 1),
+	PIN_FIELD_BASE(35, 35, IOCFG_LT_BASE, 0x50, 0x10, 7, 1),
+	PIN_FIELD_BASE(36, 37, IOCFG_LT_BASE, 0x50, 0x10, 5, 1),
+	PIN_FIELD_BASE(38, 38, IOCFG_LT_BASE, 0x50, 0x10, 9, 1),
+	PIN_FIELD_BASE(39, 40, IOCFG_RB_BASE, 0x80, 0x10, 18, 1),
+	PIN_FIELD_BASE(41, 41, IOCFG_RB_BASE, 0x80, 0x10, 12, 1),
+	PIN_FIELD_BASE(42, 43, IOCFG_RB_BASE, 0x80, 0x10, 23, 1),
+	PIN_FIELD_BASE(44, 45, IOCFG_RB_BASE, 0x80, 0x10, 21, 1),
+	PIN_FIELD_BASE(46, 47, IOCFG_RB_BASE, 0x80, 0x10, 27, 1),
+	PIN_FIELD_BASE(48, 49, IOCFG_RB_BASE, 0x80, 0x10, 25, 1),
+	PIN_FIELD_BASE(50, 57, IOCFG_RT_BASE, 0x60, 0x10, 2, 1),
+	PIN_FIELD_BASE(58, 58, IOCFG_RT_BASE, 0x60, 0x10, 1, 1),
+	PIN_FIELD_BASE(59, 59, IOCFG_RT_BASE, 0x60, 0x10, 0, 1),
+	PIN_FIELD_BASE(60, 61, IOCFG_RT_BASE, 0x60, 0x10, 10, 1),
+	PIN_FIELD_BASE(62, 62, IOCFG_RB_BASE, 0x80, 0x10, 15, 1),
+	PIN_FIELD_BASE(63, 63, IOCFG_RB_BASE, 0x80, 0x10, 14, 1),
+	PIN_FIELD_BASE(64, 64, IOCFG_RB_BASE, 0x80, 0x10, 13, 1),
+	PIN_FIELD_BASE(65, 65, IOCFG_RB_BASE, 0x80, 0x10, 16, 1),
+	PIN_FIELD_BASE(66, 68, IOCFG_LB_BASE, 0x60, 0x10, 2, 1),
+};
+
+static const struct mtk_pin_reg_calc mt7986_reg_cals[] = {
+	[PINCTRL_PIN_REG_MODE] = MTK_RANGE(mt7986_pin_mode_range),
+	[PINCTRL_PIN_REG_DIR] = MTK_RANGE(mt7986_pin_dir_range),
+	[PINCTRL_PIN_REG_DI] = MTK_RANGE(mt7986_pin_di_range),
+	[PINCTRL_PIN_REG_DO] = MTK_RANGE(mt7986_pin_do_range),
+	[PINCTRL_PIN_REG_SMT] = MTK_RANGE(mt7986_pin_smt_range),
+	[PINCTRL_PIN_REG_IES] = MTK_RANGE(mt7986_pin_ies_range),
+	[PINCTRL_PIN_REG_DRV] = MTK_RANGE(mt7986_pin_drv_range),
+	[PINCTRL_PIN_REG_PU] = MTK_RANGE(mt7986_pin_pu_range),
+	[PINCTRL_PIN_REG_PD] = MTK_RANGE(mt7986_pin_pd_range),
+	[PINCTRL_PIN_REG_PUPD] = MTK_RANGE(mt7986_pin_pupd_range),
+	[PINCTRL_PIN_REG_R0] = MTK_RANGE(mt7986_pin_r0_range),
+	[PINCTRL_PIN_REG_R1] = MTK_RANGE(mt7986_pin_r1_range),
+};
+
+static const struct mtk_pin_desc mt7986_pins[] = {
+	MT7986_TYPE0_PIN(0, "SYS_WATCHDOG"),
+	MT7986_TYPE0_PIN(1, "WF2G_LED"),
+	MT7986_TYPE0_PIN(2, "WF5G_LED"),
+	MT7986_TYPE0_PIN(3, "I2C_SCL"),
+	MT7986_TYPE0_PIN(4, "I2C_SDA"),
+	MT7986_TYPE0_PIN(5, "GPIO_0"),
+	MT7986_TYPE0_PIN(6, "GPIO_1"),
+	MT7986_TYPE0_PIN(7, "GPIO_2"),
+	MT7986_TYPE0_PIN(8, "GPIO_3"),
+	MT7986_TYPE0_PIN(9, "GPIO_4"),
+	MT7986_TYPE0_PIN(10, "GPIO_5"),
+	MT7986_TYPE0_PIN(11, "GPIO_6"),
+	MT7986_TYPE0_PIN(12, "GPIO_7"),
+	MT7986_TYPE0_PIN(13, "GPIO_8"),
+	MT7986_TYPE0_PIN(14, "GPIO_9"),
+	MT7986_TYPE0_PIN(15, "GPIO_10"),
+	MT7986_TYPE0_PIN(16, "GPIO_11"),
+	MT7986_TYPE0_PIN(17, "GPIO_12"),
+	MT7986_TYPE0_PIN(18, "GPIO_13"),
+	MT7986_TYPE0_PIN(19, "GPIO_14"),
+	MT7986_TYPE0_PIN(20, "GPIO_15"),
+	MT7986_TYPE0_PIN(21, "PWM0"),
+	MT7986_TYPE0_PIN(22, "PWM1"),
+	MT7986_TYPE0_PIN(23, "SPI0_CLK"),
+	MT7986_TYPE0_PIN(24, "SPI0_MOSI"),
+	MT7986_TYPE0_PIN(25, "SPI0_MISO"),
+	MT7986_TYPE0_PIN(26, "SPI0_CS"),
+	MT7986_TYPE0_PIN(27, "SPI0_HOLD"),
+	MT7986_TYPE0_PIN(28, "SPI0_WP"),
+	MT7986_TYPE0_PIN(29, "SPI1_CLK"),
+	MT7986_TYPE0_PIN(30, "SPI1_MOSI"),
+	MT7986_TYPE0_PIN(31, "SPI1_MISO"),
+	MT7986_TYPE0_PIN(32, "SPI1_CS"),
+	MT7986_TYPE0_PIN(33, "SPI2_CLK"),
+	MT7986_TYPE0_PIN(34, "SPI2_MOSI"),
+	MT7986_TYPE0_PIN(35, "SPI2_MISO"),
+	MT7986_TYPE0_PIN(36, "SPI2_CS"),
+	MT7986_TYPE0_PIN(37, "SPI2_HOLD"),
+	MT7986_TYPE0_PIN(38, "SPI2_WP"),
+	MT7986_TYPE0_PIN(39, "UART0_RXD"),
+	MT7986_TYPE0_PIN(40, "UART0_TXD"),
+	MT7986_TYPE0_PIN(41, "PCIE_PERESET_N"),
+	MT7986_TYPE0_PIN(42, "UART1_RXD"),
+	MT7986_TYPE0_PIN(43, "UART1_TXD"),
+	MT7986_TYPE0_PIN(44, "UART1_CTS"),
+	MT7986_TYPE0_PIN(45, "UART1_RTS"),
+	MT7986_TYPE0_PIN(46, "UART2_RXD"),
+	MT7986_TYPE0_PIN(47, "UART2_TXD"),
+	MT7986_TYPE0_PIN(48, "UART2_CTS"),
+	MT7986_TYPE0_PIN(49, "UART2_RTS"),
+	MT7986_TYPE0_PIN(50, "EMMC_DATA_0"),
+	MT7986_TYPE0_PIN(51, "EMMC_DATA_1"),
+	MT7986_TYPE0_PIN(52, "EMMC_DATA_2"),
+	MT7986_TYPE0_PIN(53, "EMMC_DATA_3"),
+	MT7986_TYPE0_PIN(54, "EMMC_DATA_4"),
+	MT7986_TYPE0_PIN(55, "EMMC_DATA_5"),
+	MT7986_TYPE0_PIN(56, "EMMC_DATA_6"),
+	MT7986_TYPE0_PIN(57, "EMMC_DATA_7"),
+	MT7986_TYPE0_PIN(58, "EMMC_CMD"),
+	MT7986_TYPE0_PIN(59, "EMMC_CK"),
+	MT7986_TYPE0_PIN(60, "EMMC_DSL"),
+	MT7986_TYPE0_PIN(61, "EMMC_RSTB"),
+	MT7986_TYPE0_PIN(62, "PCM_DTX"),
+	MT7986_TYPE0_PIN(63, "PCM_DRX"),
+	MT7986_TYPE0_PIN(64, "PCM_CLK"),
+	MT7986_TYPE0_PIN(65, "PCM_FS"),
+	MT7986_TYPE0_PIN(66, "MT7531_INT"),
+	MT7986_TYPE0_PIN(67, "SMI_MDC"),
+	MT7986_TYPE0_PIN(68, "SMI_MDIO"),
+	MT7986_TYPE1_PIN(69, "WF0_DIG_RESETB"),
+	MT7986_TYPE1_PIN(70, "WF0_CBA_RESETB"),
+	MT7986_TYPE1_PIN(71, "WF0_XO_REQ"),
+	MT7986_TYPE1_PIN(72, "WF0_TOP_CLK"),
+	MT7986_TYPE1_PIN(73, "WF0_TOP_DATA"),
+	MT7986_TYPE1_PIN(74, "WF0_HB1"),
+	MT7986_TYPE1_PIN(75, "WF0_HB2"),
+	MT7986_TYPE1_PIN(76, "WF0_HB3"),
+	MT7986_TYPE1_PIN(77, "WF0_HB4"),
+	MT7986_TYPE1_PIN(78, "WF0_HB0"),
+	MT7986_TYPE1_PIN(79, "WF0_HB0_B"),
+	MT7986_TYPE1_PIN(80, "WF0_HB5"),
+	MT7986_TYPE1_PIN(81, "WF0_HB6"),
+	MT7986_TYPE1_PIN(82, "WF0_HB7"),
+	MT7986_TYPE1_PIN(83, "WF0_HB8"),
+	MT7986_TYPE1_PIN(84, "WF0_HB9"),
+	MT7986_TYPE1_PIN(85, "WF0_HB10"),
+	MT7986_TYPE1_PIN(86, "WF1_DIG_RESETB"),
+	MT7986_TYPE1_PIN(87, "WF1_CBA_RESETB"),
+	MT7986_TYPE1_PIN(88, "WF1_XO_REQ"),
+	MT7986_TYPE1_PIN(89, "WF1_TOP_CLK"),
+	MT7986_TYPE1_PIN(90, "WF1_TOP_DATA"),
+	MT7986_TYPE1_PIN(91, "WF1_HB1"),
+	MT7986_TYPE1_PIN(92, "WF1_HB2"),
+	MT7986_TYPE1_PIN(93, "WF1_HB3"),
+	MT7986_TYPE1_PIN(94, "WF1_HB4"),
+	MT7986_TYPE1_PIN(95, "WF1_HB0"),
+	MT7986_TYPE1_PIN(96, "WF1_HB0_B"),
+	MT7986_TYPE1_PIN(97, "WF1_HB5"),
+	MT7986_TYPE1_PIN(98, "WF1_HB6"),
+	MT7986_TYPE1_PIN(99, "WF1_HB7"),
+	MT7986_TYPE1_PIN(100, "WF1_HB8"),
+};
+
+static const struct mtk_io_type_desc mt7986_io_type_desc[] = {
+	[IO_TYPE_GRP0] = {
+		.name = "18OD33",
+		.bias_set = mtk_pinconf_bias_set_pupd_r1_r0,
+		.drive_set = mtk_pinconf_drive_set_v1,
+		.input_enable = mtk_pinconf_input_enable_v1,
+	},
+	[IO_TYPE_GRP1] = {
+		.name = "18A01",
+		.bias_set = mtk_pinconf_bias_set_pu_pd,
+		.drive_set = mtk_pinconf_drive_set_v1,
+		.input_enable = mtk_pinconf_input_enable_v1,
+	},
+};
+
+/* List all groups consisting of these pins dedicated to the enablement of
+ * certain hardware block and the corresponding mode for all of the pins.
+ * The hardware probably has multiple combinations of these pinouts.
+ */
+
+static int mt7986_watchdog_pins[] = { 0, };
+static int mt7986_watchdog_funcs[] = { 1, };
+
+static int mt7986_wifi_led_pins[] = { 1, 2, };
+static int mt7986_wifi_led_funcs[] = { 1, 1, };
+
+static int mt7986_i2c_pins[] = { 3, 4, };
+static int mt7986_i2c_funcs[] = { 1, 1, };
+
+static int mt7986_uart1_0_pins[] = { 7, 8, 9, 10, };
+static int mt7986_uart1_0_funcs[] = { 3, 3, 3, 3, };
+
+static int mt7986_spi1_0_pins[] = { 11, 12, 13, 14, };
+static int mt7986_spi1_0_funcs[] = { 3, 3, 3, 3, };
+
+static int mt7986_pwm1_1_pins[] = { 20, };
+static int mt7986_pwm1_1_funcs[] = { 2, };
+
+static int mt7986_pwm0_pins[] = { 21, };
+static int mt7986_pwm0_funcs[] = { 1, };
+
+static int mt7986_pwm1_0_pins[] = { 22, };
+static int mt7986_pwm1_0_funcs[] = { 1, };
+
+static int mt7986_emmc_45_pins[] = {
+	22, 23, 24, 25, 26, 27, 28, 29, 30, 31, 32, };
+static int mt7986_emmc_45_funcs[] = { 2, 2, 2, 2, 2, 2, 2, 2, 2, 2, 2, };
+
+static int mt7986_snfi_pins[] = { 23, 24, 25, 26, 27, 28, };
+static int mt7986_snfi_funcs[] = { 1, 1, 1, 1, 1, 1, };
+
+static int mt7986_spi1_1_pins[] = { 23, 24, 25, 26, };
+static int mt7986_spi1_1_funcs[] = { 3, 3, 3, 3, };
+
+static int mt7986_uart1_1_pins[] = { 23, 24, 25, 26, };
+static int mt7986_uart1_1_funcs[] = { 4, 4, 4, 4, };
+
+static int mt7986_spi1_2_pins[] = { 29, 30, 31, 32, };
+static int mt7986_spi1_2_funcs[] = { 1, 1, 1, 1, };
+
+static int mt7986_uart1_2_pins[] = { 29, 30, 31, 32, };
+static int mt7986_uart1_2_funcs[] = { 3, 3, 3, 3, };
+
+static int mt7986_uart2_0_pins[] = { 29, 30, 31, 32, };
+static int mt7986_uart2_0_funcs[] = { 4, 4, 4, 4, };
+
+static int mt7986_spi0_pins[] = { 33, 34, 35, 36, };
+static int mt7986_spi0_funcs[] = { 1, 1, 1, 1, };
+
+static int mt7986_spi0_wp_hold_pins[] = { 37, 38, };
+static int mt7986_spi0_wp_hold_funcs[] = { 1, 1, };
+
+static int mt7986_uart2_1_pins[] = { 33, 34, 35, 36, };
+static int mt7986_uart2_1_funcs[] = { 3, 3, 3, 3, };
+
+static int mt7986_uart1_3_rx_tx_pins[] = { 35, 36, };
+static int mt7986_uart1_3_rx_tx_funcs[] = { 2, 2, };
+
+static int mt7986_uart1_3_cts_rts_pins[] = { 37, 38, };
+static int mt7986_uart1_3_cts_rts_funcs[] = { 2, 2, };
+
+static int mt7986_spi1_3_pins[] = { 33, 34, 35, 36, };
+static int mt7986_spi1_3_funcs[] = { 4, 4, 4, 4, };
+
+static int mt7986_uart0_pins[] = { 39, 40, };
+static int mt7986_uart0_funcs[] = { 1, 1, };
+
+static int mt7986_pcie_reset_pins[] = { 41, };
+static int mt7986_pcie_reset_funcs[] = { 1, };
+
+static int mt7986_uart1_pins[] = { 42, 43, 44, 45, };
+static int mt7986_uart1_funcs[] = { 1, 1, 1, 1, };
+
+static int mt7986_uart2_pins[] = { 46, 47, 48, 49, };
+static int mt7986_uart2_funcs[] = { 1, 1, 1, 1, };
+
+static int mt7986_emmc_51_pins[] = {
+	50, 51, 52, 53, 54, 55, 56, 57, 58, 59, 60, 61, };
+static int mt7986_emmc_51_funcs[] = { 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, };
+
+static int mt7986_pcm_pins[] = { 62, 63, 64, 65, };
+static int mt7986_pcm_funcs[] = { 1, 1, 1, 1, };
+
+static int mt7986_i2s_pins[] = { 62, 63, 64, 65, };
+static int mt7986_i2s_funcs[] = { 1, 1, 1, 1, };
+
+static int mt7986_switch_int_pins[] = { 66, };
+static int mt7986_switch_int_funcs[] = { 1, };
+
+static int mt7986_mdc_mdio_pins[] = { 67, 68, };
+static int mt7986_mdc_mdio_funcs[] = { 1, 1, };
+
+static int mt7986_wf_2g_pins[] = {74, 75, 76, 77, 78, 79, 80, 81, 82, 83, };
+static int mt7986_wf_2g_funcs[] = {1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, };
+
+static int mt7986_wf_5g_pins[] = {91, 92, 93, 94, 95, 96, 97, 98, 99, 100, };
+static int mt7986_wf_5g_funcs[] = {1, 1, 1, 1, 1, 1, 1, 1, 1, 1, };
+
+static int mt7986_wf_dbdc_pins[] = {
+	74, 75, 76, 77, 78, 79, 80, 81, 82, 83, 84, 85, };
+static int mt7986_wf_dbdc_funcs[] = {
+	2, 2, 2, 2, 2, 2, 2, 2, 2, 2, 2, 2, };
+
+static int mt7986_pcie_clk_pins[] = { 9, };
+static int mt7986_pcie_clk_funcs[] = { 1, };
+
+static int mt7986_pcie_wake_pins[] = { 10, };
+static int mt7986_pcie_wake_funcs[] = { 1, };
+
+static const struct mtk_group_desc mt7986_groups[] = {
+	PINCTRL_PIN_GROUP("watchdog", mt7986_watchdog),
+	PINCTRL_PIN_GROUP("wifi_led", mt7986_wifi_led),
+	PINCTRL_PIN_GROUP("i2c", mt7986_i2c),
+	PINCTRL_PIN_GROUP("uart1_0", mt7986_uart1_0),
+	PINCTRL_PIN_GROUP("pcie_clk", mt7986_pcie_clk),
+	PINCTRL_PIN_GROUP("pcie_wake", mt7986_pcie_wake),
+	PINCTRL_PIN_GROUP("spi1_0", mt7986_spi1_0),
+	PINCTRL_PIN_GROUP("pwm1_1", mt7986_pwm1_1),
+	PINCTRL_PIN_GROUP("pwm0", mt7986_pwm0),
+	PINCTRL_PIN_GROUP("pwm1_0", mt7986_pwm1_0),
+	PINCTRL_PIN_GROUP("emmc_45", mt7986_emmc_45),
+	PINCTRL_PIN_GROUP("snfi", mt7986_snfi),
+	PINCTRL_PIN_GROUP("spi1_1", mt7986_spi1_1),
+	PINCTRL_PIN_GROUP("uart1_1", mt7986_uart1_1),
+	PINCTRL_PIN_GROUP("spi1_2", mt7986_spi1_2),
+	PINCTRL_PIN_GROUP("uart1_2", mt7986_uart1_2),
+	PINCTRL_PIN_GROUP("uart2_0", mt7986_uart2_0),
+	PINCTRL_PIN_GROUP("spi0", mt7986_spi0),
+	PINCTRL_PIN_GROUP("spi0_wp_hold", mt7986_spi0_wp_hold),
+	PINCTRL_PIN_GROUP("uart2_1", mt7986_uart2_1),
+	PINCTRL_PIN_GROUP("uart1_3_rx_tx", mt7986_uart1_3_rx_tx),
+	PINCTRL_PIN_GROUP("uart1_3_cts_rts", mt7986_uart1_3_cts_rts),
+	PINCTRL_PIN_GROUP("spi1_3", mt7986_spi1_3),
+	PINCTRL_PIN_GROUP("uart0", mt7986_uart0),
+	PINCTRL_PIN_GROUP("switch_int", mt7986_switch_int),
+	PINCTRL_PIN_GROUP("mdc_mdio", mt7986_mdc_mdio),
+	PINCTRL_PIN_GROUP("pcie_pereset", mt7986_pcie_reset),
+	PINCTRL_PIN_GROUP("uart1", mt7986_uart1),
+	PINCTRL_PIN_GROUP("uart2", mt7986_uart2),
+	PINCTRL_PIN_GROUP("emmc_51", mt7986_emmc_51),
+	PINCTRL_PIN_GROUP("pcm", mt7986_pcm),
+	PINCTRL_PIN_GROUP("i2s", mt7986_i2s),
+	PINCTRL_PIN_GROUP("wf_2g", mt7986_wf_2g),
+	PINCTRL_PIN_GROUP("wf_5g", mt7986_wf_5g),
+	PINCTRL_PIN_GROUP("wf_dbdc", mt7986_wf_dbdc),
+};
+
+/* Joint those groups owning the same capability in user point of view which
+ * allows that people tend to use through the device tree.
+ */
+
+static const char *const mt7986_audio_groups[] = { "pcm", "i2s" };
+static const char *const mt7986_emmc_groups[] = { "emmc_45", "emmc_51", };
+static const char *const mt7986_ethernet_groups[] = { "switch_int",
+	"mdc_mdio", };
+static const char *const mt7986_i2c_groups[] = { "i2c", };
+static const char *const mt7986_led_groups[] = { "wifi_led", };
+static const char *const mt7986_flash_groups[] = { "snfi", };
+static const char *const mt7986_pcie_groups[] = { "pcie_clk", "pcie_wake",
+	"pcie_pereset" };
+static const char *const mt7986_pwm_groups[] = { "pwm0", "pwm1_0", "pwm1_1", };
+static const char *const mt7986_spi_groups[] = { "spi0", "spi0_wp_hold",
+	"spi1_0", "spi1_1", "spi1_2", "spi1_3", };
+static const char *const mt7986_uart_groups[] = { "uart1_0", "uart1_1",
+	"uart1_2", "uart1_3_rx_tx", "uart1_3_cts_rts", "uart2_0", "uart2_1",
+	"uart0", "uart1", "uart2", };
+static const char *const mt7986_wdt_groups[] = { "watchdog", };
+static const char *const mt7986_wf_groups[] = { "wf_2g", "wf_5g", "wf_dbdc", };
+
+static const struct mtk_function_desc mt7986_functions[] = {
+	{"audio", mt7986_audio_groups, ARRAY_SIZE(mt7986_audio_groups)},
+	{"emmc", mt7986_emmc_groups, ARRAY_SIZE(mt7986_emmc_groups)},
+	{"eth", mt7986_ethernet_groups, ARRAY_SIZE(mt7986_ethernet_groups)},
+	{"i2c", mt7986_i2c_groups, ARRAY_SIZE(mt7986_i2c_groups)},
+	{"led", mt7986_led_groups, ARRAY_SIZE(mt7986_led_groups)},
+	{"flash", mt7986_flash_groups, ARRAY_SIZE(mt7986_flash_groups)},
+	{"pcie", mt7986_pcie_groups, ARRAY_SIZE(mt7986_pcie_groups)},
+	{"pwm", mt7986_pwm_groups, ARRAY_SIZE(mt7986_pwm_groups)},
+	{"spi", mt7986_spi_groups, ARRAY_SIZE(mt7986_spi_groups)},
+	{"uart", mt7986_uart_groups, ARRAY_SIZE(mt7986_uart_groups)},
+	{"watchdog", mt7986_wdt_groups, ARRAY_SIZE(mt7986_wdt_groups)},
+	{"wifi", mt7986_wf_groups, ARRAY_SIZE(mt7986_wf_groups)},
+};
+
+static struct mtk_pinctrl_soc mt7986_data = {
+	.name = "mt7986_pinctrl",
+	.reg_cal = mt7986_reg_cals,
+	.pins = mt7986_pins,
+	.npins = ARRAY_SIZE(mt7986_pins),
+	.grps = mt7986_groups,
+	.ngrps = ARRAY_SIZE(mt7986_groups),
+	.funcs = mt7986_functions,
+	.nfuncs = ARRAY_SIZE(mt7986_functions),
+	.io_type = mt7986_io_type_desc,
+	.ntype = ARRAY_SIZE(mt7986_io_type_desc),
+	.gpio_mode = 0,
+	.base_names = mt7986_pinctrl_register_base_names,
+	.nbase_names = ARRAY_SIZE(mt7986_pinctrl_register_base_names),
+	.base_calc = 1,
+};
+
+static int mtk_pinctrl_mt7986_probe(struct udevice *dev)
+{
+	return mtk_pinctrl_common_probe(dev, &mt7986_data);
+}
+
+static const struct udevice_id mt7986_pctrl_match[] = {
+	{.compatible = "mediatek,mt7986-pinctrl"},
+	{ /* sentinel */ }
+};
+
+U_BOOT_DRIVER(mt7986_pinctrl) = {
+	.name = "mt7986_pinctrl",
+	.id = UCLASS_PINCTRL,
+	.of_match = mt7986_pctrl_match,
+	.ops = &mtk_pinctrl_ops,
+	.probe = mtk_pinctrl_mt7986_probe,
+	.priv_auto = sizeof(struct mtk_pinctrl_priv),
+};
