From patchwork Sat Sep 17 20:26:27 2022
Content-Type: text/plain; charset="utf-8"
MIME-Version: 1.0
Content-Transfer-Encoding: 8bit
X-Patchwork-Submitter: Daniel Golle <daniel@makrotopia.org>
X-Patchwork-Id: 12979242
X-Patchwork-Delegate: kvalo@adurom.com
Return-Path: <linux-wireless-owner@kernel.org>
Date: Sat, 17 Sep 2022 21:26:27 +0100
From: Daniel Golle <daniel@makrotopia.org>
To: linux-wireless@vger.kernel.org, Stanislaw Gruszka <stf_xl@wp.pl>,
        Helmut Schaa <helmut.schaa@googlemail.com>
Cc: Kalle Valo <kvalo@kernel.org>,
        "David S. Miller" <davem@davemloft.net>,
        Eric Dumazet <edumazet@google.com>,
        Jakub Kicinski <kuba@kernel.org>,
        Paolo Abeni <pabeni@redhat.com>,
        Johannes Berg <johannes.berg@intel.com>
Subject: [PATCH v3 01/16] rt2x00: define RF5592 in init_eeprom routine
Message-ID: 
 <d7eccb2c7b8ec4cd360fa2007796abffc35abb0d.1663445157.git.daniel@makrotopia.org>
References: <cover.1663445157.git.daniel@makrotopia.org>
MIME-Version: 1.0
Content-Disposition: inline
In-Reply-To: <cover.1663445157.git.daniel@makrotopia.org>
Precedence: bulk
List-ID: <linux-wireless.vger.kernel.org>
X-Mailing-List: linux-wireless@vger.kernel.org

From: Tomislav Požega <pozega.tomislav@gmail.com>

Fix incorrect RF value encoded in EEPROM on devices with Ralink Rt5592
PCIe radio (a single chip 2T2R 802.11abgn solution).

Signed-off-by: Tomislav Požega <pozega.tomislav@gmail.com>
Signed-off-by: Daniel Golle <daniel@makrotopia.org>
Acked-by: Stanislaw Gruszka <stf_xl@wp.pl>
---
 drivers/net/wireless/ralink/rt2x00/rt2800lib.c | 2 ++
 1 file changed, 2 insertions(+)

--- a/drivers/net/wireless/ralink/rt2x00/rt2800lib.c
+++ b/drivers/net/wireless/ralink/rt2x00/rt2800lib.c
@@ -9435,6 +9435,8 @@ static int rt2800_init_eeprom(struct rt2
 		rf = RF3853;
 	else if (rt2x00_rt(rt2x00dev, RT5350))
 		rf = RF5350;
+	else if (rt2x00_rt(rt2x00dev, RT5592))
+		rf = RF5592;
 	else
 		rf = rt2x00_get_field16(eeprom, EEPROM_NIC_CONF0_RF_TYPE);
 
