From 240d98e6ad0aed3c11236aa40a60bbd6fe01fae5 Mon Sep 17 00:00:00 2001
From: Weijie Gao <weijie.gao@mediatek.com>
Date: Mon, 25 Jul 2022 10:50:46 +0800
Subject: [PATCH 45/71] env: add support for NMBM upper MTD layer

Add an env driver for NMBM upper MTD layer

Signed-off-by: Weijie Gao <weijie.gao@mediatek.com>
---
 cmd/nvedit.c           |   3 +-
 env/Kconfig            |  19 ++++-
 env/Makefile           |   1 +
 env/env.c              |   3 +
 env/nmbm.c             | 155 +++++++++++++++++++++++++++++++++++++++++
 include/env_internal.h |   1 +
 tools/Makefile         |   1 +
 7 files changed, 180 insertions(+), 3 deletions(-)
 create mode 100644 env/nmbm.c

--- a/cmd/nvedit.c
+++ b/cmd/nvedit.c
@@ -50,6 +50,7 @@ DECLARE_GLOBAL_DATA_PTR;
 	defined(CONFIG_ENV_IS_IN_EXT4)		|| \
 	defined(CONFIG_ENV_IS_IN_MTD)		|| \
 	defined(CONFIG_ENV_IS_IN_NAND)		|| \
+	defined(CONFIG_ENV_IS_IN_NMBM)		|| \
 	defined(CONFIG_ENV_IS_IN_NVRAM)		|| \
 	defined(CONFIG_ENV_IS_IN_ONENAND)	|| \
 	defined(CONFIG_ENV_IS_IN_SATA)		|| \
@@ -64,7 +65,7 @@ DECLARE_GLOBAL_DATA_PTR;
 #if	!defined(ENV_IS_IN_DEVICE)		&& \
 	!defined(CONFIG_ENV_IS_NOWHERE)
 # error Define one of CONFIG_ENV_IS_IN_{EEPROM|FLASH|MMC|FAT|EXT4|MTD|\
-NAND|NVRAM|ONENAND|SATA|SPI_FLASH|REMOTE|UBI} or CONFIG_ENV_IS_NOWHERE
+NAND|NMBM|NVRAM|ONENAND|SATA|SPI_FLASH|REMOTE|UBI} or CONFIG_ENV_IS_NOWHERE
 #endif
 
 /*
--- a/env/Kconfig
+++ b/env/Kconfig
@@ -37,7 +37,7 @@ config ENV_IS_NOWHERE
 		     !ENV_IS_IN_MMC && !ENV_IS_IN_NAND && \
 		     !ENV_IS_IN_NVRAM && !ENV_IS_IN_ONENAND && \
 		     !ENV_IS_IN_REMOTE && !ENV_IS_IN_SPI_FLASH && \
-		     !ENV_IS_IN_UBI && !ENV_IS_IN_MTD
+		     !ENV_IS_IN_UBI && !ENV_IS_IN_NMBM && !ENV_IS_IN_MTD
 	help
 	  Define this if you don't want to or can't have an environment stored
 	  on a storage medium. In this case the environment will still exist
@@ -285,6 +285,21 @@ config ENV_IS_IN_NAND
 	  Currently, CONFIG_ENV_OFFSET_REDUND is not supported when
 	  using CONFIG_ENV_OFFSET_OOB.
 
+config ENV_IS_IN_NMBM
+	bool "Environment in a NMBM upper MTD layer"
+	depends on !CHAIN_OF_TRUST
+	depends on NMBM_MTD
+	help
+	  Define this if you have a NMBM upper MTD which you want to use for
+	  the environment.
+
+	  - CONFIG_ENV_OFFSET:
+	  - CONFIG_ENV_SIZE:
+
+	  These two #defines specify the offset and size of the environment
+	  area within the first NAND device.  CONFIG_ENV_OFFSET must be
+	  aligned to an erase block boundary.
+
 config ENV_IS_IN_NVRAM
 	bool "Environment in a non-volatile RAM"
 	depends on !CHAIN_OF_TRUST
@@ -561,7 +576,7 @@ config ENV_MTD_NAME
 config ENV_OFFSET
 	hex "Environment offset"
 	depends on ENV_IS_IN_EEPROM || ENV_IS_IN_MMC || ENV_IS_IN_NAND || \
-		    ENV_IS_IN_SPI_FLASH || ENV_IS_IN_MTD
+		    ENV_IS_IN_SPI_FLASH || ENV_IS_IN_NMBM || ENV_IS_IN_MTD
 	default 0x3f8000 if ARCH_ROCKCHIP && ENV_IS_IN_MMC
 	default 0x140000 if ARCH_ROCKCHIP && ENV_IS_IN_SPI_FLASH
 	default 0xF0000 if ARCH_SUNXI
--- a/env/Makefile
+++ b/env/Makefile
@@ -28,6 +28,7 @@ obj-$(CONFIG_$(SPL_TPL_)ENV_IS_IN_FAT) +
 obj-$(CONFIG_$(SPL_TPL_)ENV_IS_IN_EXT4) += ext4.o
 obj-$(CONFIG_$(SPL_TPL_)ENV_IS_IN_MTD) += mtd.o
 obj-$(CONFIG_$(SPL_TPL_)ENV_IS_IN_NAND) += nand.o
+obj-$(CONFIG_$(SPL_TPL_)ENV_IS_IN_NMBM) += nmbm.o
 obj-$(CONFIG_$(SPL_TPL_)ENV_IS_IN_SPI_FLASH) += sf.o
 obj-$(CONFIG_$(SPL_TPL_)ENV_IS_IN_FLASH) += flash.o
 
--- a/env/env.c
+++ b/env/env.c
@@ -75,6 +75,9 @@ static enum env_location env_locations[]
 #ifdef CONFIG_ENV_IS_IN_NAND
 	ENVL_NAND,
 #endif
+#ifdef CONFIG_ENV_IS_IN_NMBM
+	ENVL_NMBM,
+#endif
 #ifdef CONFIG_ENV_IS_IN_NVRAM
 	ENVL_NVRAM,
 #endif
--- /dev/null
+++ b/env/nmbm.c
@@ -0,0 +1,155 @@
+/* SPDX-License-Identifier: GPL-2.0 */
+/*
+ * Copyright (C) 2020 MediaTek Inc. All Rights Reserved.
+ *
+ * Author: Weijie Gao <weijie.gao@mediatek.com>
+ */
+
+#include <command.h>
+#include <env.h>
+#include <env_internal.h>
+#include <errno.h>
+#include <linux/kernel.h>
+#include <linux/stddef.h>
+#include <linux/types.h>
+#include <malloc.h>
+#include <memalign.h>
+#include <search.h>
+
+#include <nmbm/nmbm-mtd.h>
+
+#if defined(CONFIG_CMD_SAVEENV) && defined(CONFIG_NMBM_MTD)
+#define CMD_SAVEENV
+#endif
+
+#if defined(ENV_IS_EMBEDDED)
+env_t *env_ptr = &environment;
+#else /* ! ENV_IS_EMBEDDED */
+env_t *env_ptr;
+#endif /* ENV_IS_EMBEDDED */
+
+DECLARE_GLOBAL_DATA_PTR;
+
+static int env_nmbm_init(void)
+{
+#if defined(ENV_IS_EMBEDDED)
+	int crc1_ok = 0, crc2_ok = 0;
+	env_t *tmp_env1;
+
+	tmp_env1 = env_ptr;
+	crc1_ok = crc32(0, tmp_env1->data, ENV_SIZE) == tmp_env1->crc;
+
+	if (!crc1_ok && !crc2_ok) {
+		gd->env_addr	= 0;
+		gd->env_valid	= ENV_INVALID;
+
+		return 0;
+	} else if (crc1_ok && !crc2_ok) {
+		gd->env_valid = ENV_VALID;
+	}
+
+	if (gd->env_valid == ENV_VALID)
+		env_ptr = tmp_env1;
+
+	gd->env_addr = (ulong)env_ptr->data;
+
+#else /* ENV_IS_EMBEDDED */
+	gd->env_addr	= (ulong)&default_environment[0];
+	gd->env_valid	= ENV_VALID;
+#endif /* ENV_IS_EMBEDDED */
+
+	return 0;
+}
+
+#ifdef CMD_SAVEENV
+static int env_nmbm_save(void)
+{
+	ALLOC_CACHE_ALIGN_BUFFER(env_t, env_new, 1);
+	struct mtd_info *mtd;
+	struct erase_info ei;
+	int ret = 0;
+
+	ret = env_export(env_new);
+	if (ret)
+		return ret;
+
+	mtd = nmbm_mtd_get_upper_by_index(0);
+	if (!mtd)
+		return 1;
+
+	printf("Erasing on NMBM...\n");
+	memset(&ei, 0, sizeof(ei));
+
+	ei.mtd = mtd;
+	ei.addr = CONFIG_ENV_OFFSET;
+	ei.len = CONFIG_ENV_SIZE;
+
+	if (mtd_erase(mtd, &ei))
+		return 1;
+
+	printf("Writing on NMBM... ");
+	ret = mtd_write(mtd, CONFIG_ENV_OFFSET, CONFIG_ENV_SIZE, NULL,
+			(u_char *)env_new);
+	puts(ret ? "FAILED!\n" : "OK\n");
+
+	return !!ret;
+}
+#endif /* CMD_SAVEENV */
+
+static int readenv(size_t offset, u_char *buf)
+{
+	struct mtd_info *mtd;
+	struct mtd_oob_ops ops;
+	int ret;
+	size_t len = CONFIG_ENV_SIZE;
+
+	mtd = nmbm_mtd_get_upper_by_index(0);
+	if (!mtd)
+		return 1;
+
+	ops.mode = MTD_OPS_AUTO_OOB;
+	ops.ooblen = 0;
+	while(len > 0) {
+		ops.datbuf = buf;
+		ops.len = min(len, (size_t)mtd->writesize);
+		ops.oobbuf = NULL;
+
+		ret = mtd_read_oob(mtd, offset, &ops);
+		if (ret)
+			return 1;
+
+		buf += mtd->writesize;
+		len -= mtd->writesize;
+		offset += mtd->writesize;
+	}
+
+	return 0;
+}
+
+static int env_nmbm_load(void)
+{
+#if !defined(ENV_IS_EMBEDDED)
+	ALLOC_CACHE_ALIGN_BUFFER(char, buf, CONFIG_ENV_SIZE);
+	int ret;
+
+	ret = readenv(CONFIG_ENV_OFFSET, (u_char *)buf);
+	if (ret) {
+		env_set_default("readenv() failed", 0);
+		return -EIO;
+	}
+
+	return env_import(buf, 1, H_EXTERNAL);
+#endif /* ! ENV_IS_EMBEDDED */
+
+	return 0;
+}
+
+U_BOOT_ENV_LOCATION(nmbm) = {
+	.location	= ENVL_NMBM,
+	ENV_NAME("NMBM")
+	.load		= env_nmbm_load,
+#if defined(CMD_SAVEENV)
+	.save		= env_save_ptr(env_nmbm_save),
+#endif
+	.init		= env_nmbm_init,
+};
--- a/include/env_internal.h
+++ b/include/env_internal.h
@@ -132,6 +132,7 @@ enum env_location {
 	ENVL_MMC,
 	ENVL_MTD,
 	ENVL_NAND,
+	ENVL_NMBM,
 	ENVL_NVRAM,
 	ENVL_ONENAND,
 	ENVL_REMOTE,
--- a/tools/Makefile
+++ b/tools/Makefile
@@ -43,6 +43,7 @@ ENVCRC-$(CONFIG_ENV_IS_IN_FLASH) = y
 ENVCRC-$(CONFIG_ENV_IS_IN_ONENAND) = y
 ENVCRC-$(CONFIG_ENV_IS_IN_MTD) = y
 ENVCRC-$(CONFIG_ENV_IS_IN_NAND) = y
+ENVCRC-$(CONFIG_ENV_IS_IN_NMBM) = y
 ENVCRC-$(CONFIG_ENV_IS_IN_NVRAM) = y
 ENVCRC-$(CONFIG_ENV_IS_IN_SPI_FLASH) = y
 CONFIG_BUILD_ENVCRC ?= $(ENVCRC-y)
