From 2b88563ee5aafd9571d965b7f2093a0f58d98a31 Mon Sep 17 00:00:00 2001
From: John Crispin <john@phrozen.org>
Date: Thu, 26 Nov 2020 12:02:21 +0100
Subject: net: dsa: Add support for rtl838x switch

* rename the target to realtek
* add refactored DSA driver
* add latest gpio driver
* lots of arch cleanups
* new irq driver
* additional boards

Submitted-by: Bert Vermeulen <bert@biot.com>
Submitted-by: Birger Koblitz <mail@birger-koblitz.de>
Submitted-by: Sander Vanheule <sander@svanheule.net>
Submitted-by: Bjørn Mork <bjorn@mork.no>
Submitted-by: John Crispin <john@phrozen.org>
---
 drivers/net/dsa/rtl83xx/Kconfig               | 2 ++
 drivers/net/dsa/rtl83xx/Makefile              | 1 +
 2 files changed, 3 insertions(+)

--- a/drivers/net/dsa/Kconfig
+++ b/drivers/net/dsa/Kconfig
@@ -68,6 +68,8 @@ config NET_DSA_QCA8K
 	  This enables support for the Qualcomm Atheros QCA8K Ethernet
 	  switch chips.
 
+source "drivers/net/dsa/rtl83xx/Kconfig"
+
 config NET_DSA_REALTEK_SMI
 	tristate "Realtek SMI Ethernet switch family support"
 	depends on NET_DSA
--- a/drivers/net/dsa/Makefile
+++ b/drivers/net/dsa/Makefile
@@ -23,3 +23,4 @@ obj-y				+= mv88e6xxx/
 obj-y				+= ocelot/
 obj-y				+= qca/
 obj-y				+= sja1105/
+obj-y				+= rtl83xx/
