From: Florian Fainelli <f.fainelli@gmail.com>
Subject: [PATCH v3 1/9] mtd: rawnand: brcmnand: Assign soc as early as possible
Date: Fri, 07 Jan 2022 10:46:06 -0800
Content-Type: text/plain; charset="utf-8"

In order to key off the brcmnand_probe() code in subsequent changes
depending upon ctrl->soc, assign that variable as early as possible,
instead of much later when we have checked that it is non-NULL.

Signed-off-by: Florian Fainelli <f.fainelli@gmail.com>
---
 drivers/mtd/nand/raw/brcmnand/brcmnand.c | 3 +--
 1 file changed, 1 insertion(+), 2 deletions(-)

--- a/drivers/mtd/nand/raw/brcmnand/brcmnand.c
+++ b/drivers/mtd/nand/raw/brcmnand/brcmnand.c
@@ -2949,6 +2949,7 @@ int brcmnand_probe(struct platform_devic
 
 	dev_set_drvdata(dev, ctrl);
 	ctrl->dev = dev;
+	ctrl->soc = soc;
 
 	init_completion(&ctrl->done);
 	init_completion(&ctrl->dma_done);
@@ -3089,8 +3090,6 @@ int brcmnand_probe(struct platform_devic
 	 * interesting ways
 	 */
 	if (soc) {
-		ctrl->soc = soc;
-
 		ret = devm_request_irq(dev, ctrl->irq, brcmnand_irq, 0,
 				       DRV_NAME, ctrl);
 
