This uses upstream qcom-ipq8064-v1.0.dtsi and modifies it by patches
instead of keeping a local version.
We drop partitions, LEDs and keys from the file as we will implement
them differently anyway.

--- a/arch/arm/boot/dts/qcom-ipq8064-v1.0.dtsi
+++ b/arch/arm/boot/dts/qcom-ipq8064-v1.0.dtsi
@@ -42,16 +42,6 @@
 					#size-cells = <1>;
 					spi-max-frequency = <50000000>;
 					reg = <0>;
-
-					partition@0 {
-						label = "rootfs";
-						reg = <0x0 0x1000000>;
-					};
-
-					partition@1 {
-						label = "scratch";
-						reg = <0x1000000 0x1000000>;
-					};
 				};
 			};
 		};
@@ -64,64 +54,5 @@
 			ports-implemented = <0x1>;
 			status = "okay";
 		};
-
-		gpio_keys {
-			compatible = "gpio-keys";
-			pinctrl-0 = <&buttons_pins>;
-			pinctrl-names = "default";
-
-			button@1 {
-				label = "reset";
-				linux,code = <KEY_RESTART>;
-				gpios = <&qcom_pinmux 54 GPIO_ACTIVE_LOW>;
-				linux,input-type = <1>;
-				debounce-interval = <60>;
-			};
-			button@2 {
-				label = "wps";
-				linux,code = <KEY_WPS_BUTTON>;
-				gpios = <&qcom_pinmux 65 GPIO_ACTIVE_LOW>;
-				linux,input-type = <1>;
-				debounce-interval = <60>;
-			};
-		};
-
-		leds {
-			compatible = "gpio-leds";
-			pinctrl-0 = <&leds_pins>;
-			pinctrl-names = "default";
-
-			led@7 {
-				label = "led_usb1";
-				gpios = <&qcom_pinmux 7 GPIO_ACTIVE_HIGH>;
-				linux,default-trigger = "usbdev";
-				default-state = "off";
-			};
-
-			led@8 {
-				label = "led_usb3";
-				gpios = <&qcom_pinmux 8 GPIO_ACTIVE_HIGH>;
-				linux,default-trigger = "usbdev";
-				default-state = "off";
-			};
-
-			led@9 {
-				label = "status_led_fail";
-				gpios = <&qcom_pinmux 9 GPIO_ACTIVE_HIGH>;
-				default-state = "off";
-			};
-
-			led@26 {
-				label = "sata_led";
-				gpios = <&qcom_pinmux 26 GPIO_ACTIVE_HIGH>;
-				default-state = "off";
-			};
-
-			led@53 {
-				label = "status_led_pass";
-				gpios = <&qcom_pinmux 53 GPIO_ACTIVE_HIGH>;
-				default-state = "off";
-			};
-		};
 	};
 };
