From 44ae4ed142265a6d50a9d3e6f4c395f97b6849ab Mon Sep 17 00:00:00 2001
From: Zhanyong Wang <zhanyong.wang@mediatek.com>
Date: Sat, 6 Nov 2021 20:06:30 +0800
Subject: [PATCH 2/5] nvmem: mtk-efuse: support minimum one byte access stride
 and granularity

In order to support nvmem bits property, should support minimum 1 byte
read stride and minimum 1 byte read granularity at the same time.

Signed-off-by: Chunfeng Yun <chunfeng.yun@mediatek.com>
Signed-off-by: Zhanyong Wang <zhanyong.wang@mediatek.com>
Change-Id: Iafe1ebf195d58a3e9e3518913f795d14a01dfd3b
---
 drivers/nvmem/mtk-efuse.c | 13 +++++++------
 1 file changed, 7 insertions(+), 6 deletions(-)

--- a/drivers/nvmem/mtk-efuse.c
+++ b/drivers/nvmem/mtk-efuse.c
@@ -19,11 +19,12 @@ static int mtk_reg_read(void *context,
 			unsigned int reg, void *_val, size_t bytes)
 {
 	struct mtk_efuse_priv *priv = context;
-	u32 *val = _val;
-	int i = 0, words = bytes / 4;
+	void __iomem *addr = priv->base + reg;
+	u8 *val = _val;
+	int i;
 
-	while (words--)
-		*val++ = readl(priv->base + reg + (i++ * 4));
+	for (i = 0; i < bytes; i++, val++)
+		*val = readb(addr + i);
 
 	return 0;
 }
@@ -45,8 +46,8 @@ static int mtk_efuse_probe(struct platfo
 	if (IS_ERR(priv->base))
 		return PTR_ERR(priv->base);
 
-	econfig.stride = 4;
-	econfig.word_size = 4;
+	econfig.stride = 1;
+	econfig.word_size = 1;
 	econfig.reg_read = mtk_reg_read;
 	econfig.size = resource_size(res);
 	econfig.priv = priv;
