// SPDX-License-Identifier: GPL-2.0-or-later OR MIT
// Copyright (c) 2021 Cezary Jackiewicz
// Copyright (c) 2021, 2022 Lech Perczak
#include "qca956x.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>

/ {
	aliases {
		led-boot = &led_debug;
		led-failsafe = &led_debug;
		led-running = &led_debug;
		led-upgrade = &led_debug;
		label-mac-device = &eth0;
	};

	leds {
		compatible = "gpio-leds";
		pinctrl-names = "default";
		pinctrl-0 = <&enable_wlan_led_gpio>;

		/* Hidden SMD LED below signal strength LEDs.
		 * Visible through slits underside of the case,
		 * and slightly through the case below signal state LEDs
		 */
		led_debug: led-0 {
			function = LED_FUNCTION_DEBUG;
			gpios = <&gpio 7 GPIO_ACTIVE_LOW>;
			default-state = "on";
		};

		led-1 {
			function = LED_FUNCTION_WLAN;
			color = <LED_COLOR_ID_BLUE>;
			gpios = <&gpio 19 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy1tpt";
		};
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 2 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};

		wps {
			label = "wps";
			linux,code = <KEY_WPS_BUTTON>;
			gpios = <&gpio 1 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};

		wifi {
			label = "wifi";
			linux,code = <KEY_RFKILL>;
			gpios = <&gpio 8 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};
	};

	/* This GPIO is used to reset whole board _including_ the modem */
	gpio-restart {
		compatible = "gpio-restart";
		gpios = <&gpio 5 GPIO_ACTIVE_HIGH>;
		active-delay = <3000>;
		inactive-delay = <1000>;
	};
};

&spi {
	status = "okay";

	boot_flash: flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <25000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;
		};
	};

	system_flash: flash@1 {
		compatible = "spi-nand";
		reg = <1>;
		spi-max-frequency = <25000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;
		};
	};
};

&mdio0 {
	status = "okay";

	phy0: ethernet-phy@0 {
		reg = <0>;
		phy-mode = "sgmii";

		qca,ar8327-initvals = <
			0x04 0x00080080 /* PORT0 PAD MODE CTRL */
			0x7c 0x0000007e /* PORT0_STATUS */
		>;
	};
};

&eth0 {
	status = "okay";

	phy-mode = "sgmii";
	phy-handle = <&phy0>;
};

&pcie {
	status = "okay";

	wifi_ath10k: wifi@0,0 {
		compatible = "qcom,ath10k";
		reg = <0x0 0 0 0 0>;
	};
};

&pinmux {
	enable_wlan_led_gpio: pinmux_wlan_led_gpio {
		pinctrl-single,bits = <0x10 0x0 0xff000000>;
	};
};

&wmac {
	status = "okay";
};

&usb_phy0 {
	status = "okay";
};

&usb0 {
	status = "okay";
};

&usb_phy1 {
	status = "okay";
};

&usb1 {
	status = "okay";
};
