// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "qcom-ipq4019.dtsi"
#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/soc/qcom,tcsr.h>

/ {
	model = "GL.iNet GL-AP1300";
	compatible = "glinet,gl-ap1300";

	aliases {
		led-boot = &led_power;
		led-failsafe = &led_power;
		led-running = &led_power;
		led-upgrade = &led_power;
		label-mac-device = &gmac0;
	};

	memory {
		device_type = "memory";
		reg = <0x80000000 0x10000000>;
	};

	chosen {
		bootargs-append = " ubi.mtd=ubi root=/dev/ubiblock0_1";
	};

	soc {
		rng@22000 {
			status = "okay";
		};

		mdio@90000 {
			status = "okay";
		};

		ess-psgmii@98000 {
			status = "okay";
		};

		tcsr@1949000 {
			compatible = "qcom,tcsr";
			reg = <0x1949000 0x100>;
			qcom,wifi_glb_cfg = <TCSR_WIFI_GLB_CFG>;
		};

		tcsr@194b000 {
			/* select hostmode */
			compatible = "qcom,tcsr";
			reg = <0x194b000 0x100>;
			qcom,usb-hsphy-mode-select = <TCSR_USB_HSPHY_HOST_MODE>;
			status = "okay";
		};

		ess_tcsr@1953000 {
			compatible = "qcom,tcsr";
			reg = <0x1953000 0x1000>;
			qcom,ess-interface-select = <TCSR_ESS_PSGMII>;
		};

		tcsr@1957000 {
			compatible = "qcom,tcsr";
			reg = <0x1957000 0x100>;
			qcom,wifi_noc_memtype_m0_m2 = <TCSR_WIFI_NOC_MEMTYPE_M0_M2>;
		};

		usb2@60f8800 {
			status = "okay";
		};

		usb3@8af8800 {
			status = "okay";
		};

		crypto@8e3a000 {
			status = "okay";
		};

		watchdog@b017000 {
			status = "okay";
		};

		ess-switch@c000000 {
			status = "okay";
			switch_lan_bmp = <0x18>;
			switch_wan_bmp = <0x20>;
		};

		edma@c080000 {
			status = "okay";
		};
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			gpios = <&tlmm 63 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led_power: power {
			label = "green:power";
			gpios = <&tlmm 2 GPIO_ACTIVE_HIGH>;
			default-state = "on";
		};

		wan {
			label = "green:wan";
			gpios = <&tlmm 3 GPIO_ACTIVE_HIGH>;
		};
	};
};

&blsp_dma {
	status = "okay";
};

&cryptobam {
	status = "okay";
};

&blsp1_spi1 {
	status = "okay";

	pinctrl-0 = <&spi0_pins>;
	pinctrl-names = "default";
	cs-gpios = <&tlmm 54 GPIO_ACTIVE_HIGH>, <&tlmm 5 GPIO_ACTIVE_HIGH>;

	flash@0 {
		status = "okay";

		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <24000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "SBL1";
				reg = <0x00000000 0x00040000>;
				read-only;
			};

			partition@40000 {
				label = "MIBIB";
				reg = <0x00040000 0x00020000>;
				read-only;
			};

			partition@60000 {
				label = "QSEE";
				reg = <0x00060000 0x00060000>;
				read-only;
			};

			partition@c0000 {
				label = "CDT";
				reg = <0x000c0000 0x00010000>;
				read-only;
			};

			partition@d0000 {
				label = "DDRPARAMS";
				reg = <0x000d0000 0x00010000>;
				read-only;
			};

			partition@e0000 {
				label = "APPSBLENV"; /* uboot env*/
				reg = <0x000e0000 0x00010000>;
			};

			partition@f0000 {
				label = "APPSBL"; /* uboot */
				reg = <0x000f0000 0x00080000>;
				read-only;
			};

			partition@170000 {
				label = "ART";
				reg = <0x00170000 0x00010000>;
				read-only;
				compatible = "nvmem-cells";
				#address-cells = <1>;
				#size-cells = <1>;

				precal_art_1000: precal@1000 {
					reg = <0x1000 0x2f20>;
				};

				precal_art_5000: precal@5000 {
					reg = <0x5000 0x2f20>;
				};
			};
		};
	};

	spi-nand@1 {
		status = "okay";

		compatible = "spi-nand";
		reg = <1>;
		spi-max-frequency = <24000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "ubi";
				reg = <0x00000000 0x08000000>;
			};
		};
	};
};

&blsp1_uart1 {
	pinctrl-0 = <&serial_pins>;
	pinctrl-names = "default";
	status = "okay";
};

&tlmm {
	serial_pins: serial_pinmux {
		mux {
			pins = "gpio60", "gpio61";
			function = "blsp_uart0";
			bias-disable;
		};
	};

	spi0_pins: spi0_pinmux {
		mux_spi {
			function = "blsp_spi0";
			pins = "gpio55", "gpio56", "gpio57";
			drive-strength = <12>;
			bias-disable;
		};

		mux_cs {
			function = "gpio";
			pins = "gpio54", "gpio5";
			drive-strength = <2>;
			bias-disable;
			output-high;
		};
	};
};

&usb2_hs_phy {
	status = "okay";
};

&usb3_hs_phy {
	status = "okay";
};

&usb3_ss_phy {
	status = "okay";
};

&wifi0 {
	status = "okay";
	nvmem-cell-names = "pre-calibration";
	nvmem-cells = <&precal_art_1000>;
	qcom,ath10k-calibration-variant = "GL-AP1300";
};

&wifi1 {
	status = "okay";
	nvmem-cell-names = "pre-calibration";
	nvmem-cells = <&precal_art_5000>;
	qcom,ath10k-calibration-variant = "GL-AP1300";
};
