From d25f3a74f30aace819163dfa54f2a4b8ca1dc932 Mon Sep 17 00:00:00 2001
From: "Russell King (Oracle)" <rmk+kernel@armlinux.org.uk>
Date: Tue, 26 Oct 2021 11:06:11 +0100
Subject: [PATCH] net: phylink: use supported_interfaces for phylink
 validation

If the network device supplies a supported interface bitmap, we can use
that during phylink's validation to simplify MAC drivers in two ways by
using the supported_interfaces bitmap to:

1. reject unsupported interfaces before calling into the MAC driver.
2. generate the set of all supported link modes across all supported
   interfaces (used mainly for SFP, but also some 10G PHYs.)

Suggested-by: Sean Anderson <sean.anderson@seco.com>
Signed-off-by: Russell King (Oracle) <rmk+kernel@armlinux.org.uk>
Signed-off-by: David S. Miller <davem@davemloft.net>
---
 drivers/net/phy/phylink.c | 36 ++++++++++++++++++++++++++++++++++++
 include/linux/phylink.h   | 12 ++++++++++--
 2 files changed, 46 insertions(+), 2 deletions(-)

--- a/drivers/net/phy/phylink.c
+++ b/drivers/net/phy/phylink.c
@@ -155,9 +155,45 @@ static const char *phylink_an_mode_str(u
 	return mode < ARRAY_SIZE(modestr) ? modestr[mode] : "unknown";
 }
 
+static int phylink_validate_any(struct phylink *pl, unsigned long *supported,
+				struct phylink_link_state *state)
+{
+	__ETHTOOL_DECLARE_LINK_MODE_MASK(all_adv) = { 0, };
+	__ETHTOOL_DECLARE_LINK_MODE_MASK(all_s) = { 0, };
+	__ETHTOOL_DECLARE_LINK_MODE_MASK(s);
+	struct phylink_link_state t;
+	int intf;
+
+	for (intf = 0; intf < PHY_INTERFACE_MODE_MAX; intf++) {
+		if (test_bit(intf, pl->config->supported_interfaces)) {
+			linkmode_copy(s, supported);
+
+			t = *state;
+			t.interface = intf;
+			pl->mac_ops->validate(pl->config, s, &t);
+			linkmode_or(all_s, all_s, s);
+			linkmode_or(all_adv, all_adv, t.advertising);
+		}
+	}
+
+	linkmode_copy(supported, all_s);
+	linkmode_copy(state->advertising, all_adv);
+
+	return phylink_is_empty_linkmode(supported) ? -EINVAL : 0;
+}
+
 static int phylink_validate(struct phylink *pl, unsigned long *supported,
 			    struct phylink_link_state *state)
 {
+	if (!phy_interface_empty(pl->config->supported_interfaces)) {
+		if (state->interface == PHY_INTERFACE_MODE_NA)
+			return phylink_validate_any(pl, supported, state);
+
+		if (!test_bit(state->interface,
+			      pl->config->supported_interfaces))
+			return -EINVAL;
+	}
+
 	pl->mac_ops->validate(pl->config, supported, state);
 
 	return phylink_is_empty_linkmode(supported) ? -EINVAL : 0;
--- a/include/linux/phylink.h
+++ b/include/linux/phylink.h
@@ -67,6 +67,8 @@ enum phylink_op_type {
  * @ovr_an_inband: if true, override PCS to MLO_AN_INBAND
  * @get_fixed_state: callback to execute to determine the fixed link state,
  *		     if MAC link is at %MLO_AN_FIXED mode.
+ * @supported_interfaces: bitmap describing which PHY_INTERFACE_MODE_xxx
+ *                        are supported by the MAC/PCS.
  */
 struct phylink_config {
 	struct device *dev;
@@ -134,8 +136,14 @@ struct phylink_mac_ops {
  * based on @state->advertising and/or @state->speed and update
  * @state->interface accordingly. See phylink_helper_basex_speed().
  *
- * When @state->interface is %PHY_INTERFACE_MODE_NA, phylink expects the
- * MAC driver to return all supported link modes.
+ * When @config->supported_interfaces has been set, phylink will iterate
+ * over the supported interfaces to determine the full capability of the
+ * MAC. The validation function must not print errors if @state->interface
+ * is set to an unexpected value.
+ *
+ * When @config->supported_interfaces is empty, phylink will call this
+ * function with @state->interface set to %PHY_INTERFACE_MODE_NA, and
+ * expects the MAC driver to return all supported link modes.
  *
  * If the @state->interface mode is not supported, then the @supported
  * mask must be cleared.
