From: Sebastian Gottschall <s.gottschall@newmedia-net.de>

Adds LED and GPIO Control support for 988x, 9887, 9888, 99x0, 9984 based
chipsets with on chipset connected led's using WMI Firmware API.  The LED
device will get available named as "ath10k-phyX" at sysfs and can be controlled
with various triggers.  adds also debugfs interface for gpio control.

This patch is specific for OpenWRt base, as is use old backported package
with old wireless source. Support for QCA9984 is removed and a simbol
is added to local-simbol file to export the actually compile the code 
with the ATH10K_LEDS simbol.


Signed-off-by: Sebastian Gottschall <s.gottschall@dd-wrt.com>
Reviewed-by: Steve deRosier <derosier@cal-sierra.com>
[kvalo: major reorg and cleanup]
Signed-off-by: Kalle Valo <kvalo@codeaurora.org>
Signed-off-by: Ansuel Smith <ansuelsmth@gmail.com>
---

v13:

* only compile tested!

* fix all checkpatch warnings

* fix commit log

* sizeof(struct ath10k_gpiocontrol) -> sizeof(*gpio)

* unsigned -> unsigned int

* remove GPIOLIB code, that should be added in a separate patch

* rename gpio.c to leds.c

* add leds.h

* rename some functions:

  ath10k_attach_led() -> ath10k_leds_register()
  ath10k_unregister_led() -> ath10k_leds_unregister()
  ath10k_reset_led_pin() -> ath10k_leds_start()

* call ath10k_leds_unregister() before ath10k_thermal_unregister() to preserve ordering

* call ath10k_leds_start() only from ath10k_core_start() and not from mac.c

* rename struct ath10k_gpiocontrol as anonymous function under struct
  ath10k::leds, no need for memory allocation

* merge ath10k_add_led() to ath10k_attach_led(), which is it's only caller

* remove #if IS_ENABLED() checks from most of places, memory savings from those were not worth it

* Kconfig help text improvement and move it lower in the menu, also don't enable it by default

* switch to set_brightness_blocking() so that the callback can sleep,
  then no need to use ath10k_wmi_cmd_send_nowait() and can take mutex
  to access ar->state

* don't touch ath10k_wmi_pdev_get_temperature()

* as QCA6174/QCA9377 are not (yet) supported don't add the command to WMI-TLV interface

* remove debugfs interface, that should be added in another patch

* cleanup includes


 drivers/net/wireless/ath/ath10k/Kconfig   |  10 +++
 drivers/net/wireless/ath/ath10k/Makefile  |   1 +
 drivers/net/wireless/ath/ath10k/core.c    |  22 +++++++
 drivers/net/wireless/ath/ath10k/core.h    |   9 ++-
 drivers/net/wireless/ath/ath10k/hw.h      |   1 +
 drivers/net/wireless/ath/ath10k/leds.c    | 103 ++++++++++++++++++++++++++++++
 drivers/net/wireless/ath/ath10k/leds.h    |  45 +++++++++++++
 drivers/net/wireless/ath/ath10k/mac.c     |   1 +
 drivers/net/wireless/ath/ath10k/wmi-ops.h |  32 ++++++++++
 drivers/net/wireless/ath/ath10k/wmi-tlv.c |   2 +
 drivers/net/wireless/ath/ath10k/wmi.c     |  54 ++++++++++++++++
 drivers/net/wireless/ath/ath10k/wmi.h     |  35 ++++++++++
 12 files changed, 314 insertions(+), 1 deletion(-)
 create mode 100644 drivers/net/wireless/ath/ath10k/leds.c
 create mode 100644 drivers/net/wireless/ath/ath10k/leds.h
--- a/drivers/net/wireless/ath/ath10k/Kconfig
+++ b/drivers/net/wireless/ath/ath10k/Kconfig
@@ -71,6 +71,16 @@ config ATH10K_DEBUGFS
 
 	  If unsure, say Y to make it easier to debug problems.
 
+config ATH10K_LEDS
+	bool "Atheros ath10k LED support"
+	depends on ATH10K
+	select MAC80211_LEDS
+	select LEDS_CLASS
+	select NEW_LEDS
+	default y
+	---help---
+	  This option is necessary, if you want LED support for chipset connected led pins. If unsure, say N.
+
 config ATH10K_SPECTRAL
 	bool "Atheros ath10k spectral scan support"
 	depends on ATH10K_DEBUGFS
--- a/drivers/net/wireless/ath/ath10k/Makefile
+++ b/drivers/net/wireless/ath/ath10k/Makefile
@@ -19,6 +19,7 @@ ath10k_core-$(CPTCFG_ATH10K_SPECTRAL) +=
 ath10k_core-$(CPTCFG_NL80211_TESTMODE) += testmode.o
 ath10k_core-$(CPTCFG_ATH10K_TRACING) += trace.o
 ath10k_core-$(CPTCFG_ATH10K_THERMAL) += thermal.o
+ath10k_core-$(CPTCFG_ATH10K_LEDS) += leds.o
 ath10k_core-$(CPTCFG_MAC80211_DEBUGFS) += debugfs_sta.o
 ath10k_core-$(CONFIG_PM) += wow.o
 ath10k_core-$(CONFIG_DEV_COREDUMP) += coredump.o
--- a/local-symbols
+++ b/local-symbols
@@ -166,6 +166,7 @@ ATH10K_DEBUG=
 ATH10K_DEBUGFS=
 ATH10K_SPECTRAL=
 ATH10K_THERMAL=
+ATH10K_LEDS=
 ATH10K_TRACING=
 ATH10K_DFS_CERTIFIED=
 WCN36XX=
--- a/drivers/net/wireless/ath/ath10k/core.c
+++ b/drivers/net/wireless/ath/ath10k/core.c
@@ -26,6 +26,7 @@
 #include "testmode.h"
 #include "wmi-ops.h"
 #include "coredump.h"
+#include "leds.h"
 
 unsigned int ath10k_debug_mask;
 EXPORT_SYMBOL(ath10k_debug_mask);
@@ -65,6 +66,7 @@ static const struct ath10k_hw_params ath
 		.dev_id = QCA988X_2_0_DEVICE_ID,
 		.bus = ATH10K_BUS_PCI,
 		.name = "qca988x hw2.0",
+		.led_pin = 1,
 		.patch_load_addr = QCA988X_HW_2_0_PATCH_LOAD_ADDR,
 		.uart_pin = 7,
 		.cc_wraparound_type = ATH10K_HW_CC_WRAP_SHIFTED_ALL,
@@ -138,6 +140,7 @@ static const struct ath10k_hw_params ath
 		.dev_id = QCA9887_1_0_DEVICE_ID,
 		.bus = ATH10K_BUS_PCI,
 		.name = "qca9887 hw1.0",
+		.led_pin = 1,
 		.patch_load_addr = QCA9887_HW_1_0_PATCH_LOAD_ADDR,
 		.uart_pin = 7,
 		.cc_wraparound_type = ATH10K_HW_CC_WRAP_SHIFTED_ALL,
@@ -355,6 +358,7 @@ static const struct ath10k_hw_params ath
 		.dev_id = QCA99X0_2_0_DEVICE_ID,
 		.bus = ATH10K_BUS_PCI,
 		.name = "qca99x0 hw2.0",
+		.led_pin = 17,
 		.patch_load_addr = QCA99X0_HW_2_0_PATCH_LOAD_ADDR,
 		.uart_pin = 7,
 		.otp_exe_param = 0x00000700,
@@ -397,6 +401,7 @@ static const struct ath10k_hw_params ath
 		.dev_id = QCA9984_1_0_DEVICE_ID,
 		.bus = ATH10K_BUS_PCI,
 		.name = "qca9984/qca9994 hw1.0",
+		.led_pin = 17,
 		.patch_load_addr = QCA9984_HW_1_0_PATCH_LOAD_ADDR,
 		.uart_pin = 7,
 		.cc_wraparound_type = ATH10K_HW_CC_WRAP_SHIFTED_EACH,
@@ -446,6 +451,7 @@ static const struct ath10k_hw_params ath
 		.dev_id = QCA9888_2_0_DEVICE_ID,
 		.bus = ATH10K_BUS_PCI,
 		.name = "qca9888 hw2.0",
+		.led_pin = 17,
 		.patch_load_addr = QCA9888_HW_2_0_PATCH_LOAD_ADDR,
 		.uart_pin = 7,
 		.cc_wraparound_type = ATH10K_HW_CC_WRAP_SHIFTED_EACH,
@@ -3158,6 +3164,10 @@ int ath10k_core_start(struct ath10k *ar,
 		goto err_hif_stop;
 	}
 
+	status = ath10k_leds_start(ar);
+	if (status)
+		goto err_hif_stop;
+
 	return 0;
 
 err_hif_stop:
@@ -3416,9 +3426,18 @@ static void ath10k_core_register_work(st
 		goto err_spectral_destroy;
 	}
 
+	status = ath10k_leds_register(ar);
+	if (status) {
+		ath10k_err(ar, "could not register leds: %d\n",
+			   status);
+		goto err_thermal_unregister;
+	}
+
 	set_bit(ATH10K_FLAG_CORE_REGISTERED, &ar->dev_flags);
 	return;
 
+err_thermal_unregister:
+	ath10k_thermal_unregister(ar);
 err_spectral_destroy:
 	ath10k_spectral_destroy(ar);
 err_debug_destroy:
@@ -3464,6 +3483,8 @@ void ath10k_core_unregister(struct ath10
 	if (!test_bit(ATH10K_FLAG_CORE_REGISTERED, &ar->dev_flags))
 		return;
 
+	ath10k_leds_unregister(ar);
+
 	ath10k_thermal_unregister(ar);
 	/* Stop spectral before unregistering from mac80211 to remove the
 	 * relayfs debugfs file cleanly. Otherwise the parent debugfs tree
--- a/drivers/net/wireless/ath/ath10k/core.h
+++ b/drivers/net/wireless/ath/ath10k/core.h
@@ -14,6 +14,7 @@
 #include <linux/pci.h>
 #include <linux/uuid.h>
 #include <linux/time.h>
+#include <linux/leds.h>
 
 #include "htt.h"
 #include "htc.h"
@@ -1256,6 +1257,13 @@ struct ath10k {
 	} testmode;
 
 	struct {
+		struct gpio_led wifi_led;
+		struct led_classdev cdev;
+		char label[48];
+		u32 gpio_state_pin;
+	} leds;
+
+	struct {
 		/* protected by data_lock */
 		u32 rx_crc_err_drop;
 		u32 fw_crash_counter;
--- a/drivers/net/wireless/ath/ath10k/hw.h
+++ b/drivers/net/wireless/ath/ath10k/hw.h
@@ -517,6 +517,7 @@ struct ath10k_hw_params {
 	const char *name;
 	u32 patch_load_addr;
 	int uart_pin;
+	int led_pin;
 	u32 otp_exe_param;
 
 	/* Type of hw cycle counter wraparound logic, for more info
--- /dev/null
+++ b/drivers/net/wireless/ath/ath10k/leds.c
@@ -0,0 +1,103 @@
+/*
+ * Copyright (c) 2005-2011 Atheros Communications Inc.
+ * Copyright (c) 2011-2017 Qualcomm Atheros, Inc.
+ * Copyright (c) 2018 Sebastian Gottschall <s.gottschall@dd-wrt.com>
+ * Copyright (c) 2018, The Linux Foundation. All rights reserved.
+ *
+ * Permission to use, copy, modify, and/or distribute this software for any
+ * purpose with or without fee is hereby granted, provided that the above
+ * copyright notice and this permission notice appear in all copies.
+ *
+ * THE SOFTWARE IS PROVIDED "AS IS" AND THE AUTHOR DISCLAIMS ALL WARRANTIES
+ * WITH REGARD TO THIS SOFTWARE INCLUDING ALL IMPLIED WARRANTIES OF
+ * MERCHANTABILITY AND FITNESS. IN NO EVENT SHALL THE AUTHOR BE LIABLE FOR
+ * ANY SPECIAL, DIRECT, INDIRECT, OR CONSEQUENTIAL DAMAGES OR ANY DAMAGES
+ * WHATSOEVER RESULTING FROM LOSS OF USE, DATA OR PROFITS, WHETHER IN AN
+ * ACTION OF CONTRACT, NEGLIGENCE OR OTHER TORTIOUS ACTION, ARISING OUT OF
+ * OR IN CONNECTION WITH THE USE OR PERFORMANCE OF THIS SOFTWARE.
+ */
+
+#include <linux/leds.h>
+
+#include "core.h"
+#include "wmi.h"
+#include "wmi-ops.h"
+
+#include "leds.h"
+
+static int ath10k_leds_set_brightness_blocking(struct led_classdev *led_cdev,
+					       enum led_brightness brightness)
+{
+	struct ath10k *ar = container_of(led_cdev, struct ath10k,
+					 leds.cdev);
+	struct gpio_led *led = &ar->leds.wifi_led;
+
+	mutex_lock(&ar->conf_mutex);
+
+	if (ar->state != ATH10K_STATE_ON)
+		goto out;
+
+	ar->leds.gpio_state_pin = (brightness != LED_OFF) ^ led->active_low;
+	ath10k_wmi_gpio_output(ar, led->gpio, ar->leds.gpio_state_pin);
+
+out:
+	mutex_unlock(&ar->conf_mutex);
+
+	return 0;
+}
+
+int ath10k_leds_start(struct ath10k *ar)
+{
+	if (ar->hw_params.led_pin == 0)
+		/* leds not supported */
+		return 0;
+
+	/* under some circumstances, the gpio pin gets reconfigured
+	 * to default state by the firmware, so we need to
+	 * reconfigure it this behaviour has only ben seen on
+	 * QCA9984 and QCA99XX devices so far
+	 */
+	ath10k_wmi_gpio_config(ar, ar->hw_params.led_pin, 0,
+			       WMI_GPIO_PULL_NONE, WMI_GPIO_INTTYPE_DISABLE);
+	ath10k_wmi_gpio_output(ar, ar->hw_params.led_pin, 1);
+
+	return 0;
+}
+
+int ath10k_leds_register(struct ath10k *ar)
+{
+	int ret;
+
+	if (ar->hw_params.led_pin == 0)
+		/* leds not supported */
+		return 0;
+
+	snprintf(ar->leds.label, sizeof(ar->leds.label), "ath10k-%s",
+		 wiphy_name(ar->hw->wiphy));
+	ar->leds.wifi_led.active_low = 1;
+	ar->leds.wifi_led.gpio = ar->hw_params.led_pin;
+	ar->leds.wifi_led.name = ar->leds.label;
+	ar->leds.wifi_led.default_state = LEDS_GPIO_DEFSTATE_KEEP;
+
+	ar->leds.cdev.name = ar->leds.label;
+	ar->leds.cdev.brightness_set_blocking = ath10k_leds_set_brightness_blocking;
+
+	/* FIXME: this assignment doesn't make sense as it's NULL, remove it? */
+	ar->leds.cdev.default_trigger = ar->leds.wifi_led.default_trigger;
+
+	ret = led_classdev_register(wiphy_dev(ar->hw->wiphy), &ar->leds.cdev);
+	if (ret)
+		return ret;
+
+	return 0;
+}
+
+void ath10k_leds_unregister(struct ath10k *ar)
+{
+	if (ar->hw_params.led_pin == 0)
+		/* leds not supported */
+		return;
+
+	led_classdev_unregister(&ar->leds.cdev);
+}
+
--- /dev/null
+++ b/drivers/net/wireless/ath/ath10k/leds.h
@@ -0,0 +1,41 @@
+/*
+ * Copyright (c) 2018, The Linux Foundation. All rights reserved.
+ *
+ * Permission to use, copy, modify, and/or distribute this software for any
+ * purpose with or without fee is hereby granted, provided that the above
+ * copyright notice and this permission notice appear in all copies.
+ *
+ * THE SOFTWARE IS PROVIDED "AS IS" AND THE AUTHOR DISCLAIMS ALL WARRANTIES
+ * WITH REGARD TO THIS SOFTWARE INCLUDING ALL IMPLIED WARRANTIES OF
+ * MERCHANTABILITY AND FITNESS. IN NO EVENT SHALL THE AUTHOR BE LIABLE FOR
+ * ANY SPECIAL, DIRECT, INDIRECT, OR CONSEQUENTIAL DAMAGES OR ANY DAMAGES
+ * WHATSOEVER RESULTING FROM LOSS OF USE, DATA OR PROFITS, WHETHER IN AN
+ * ACTION OF CONTRACT, NEGLIGENCE OR OTHER TORTIOUS ACTION, ARISING OUT OF
+ * OR IN CONNECTION WITH THE USE OR PERFORMANCE OF THIS SOFTWARE.
+ */
+#ifndef _LEDS_H_
+#define _LEDS_H_
+
+#include "core.h"
+
+#ifdef CPTCFG_ATH10K_LEDS
+void ath10k_leds_unregister(struct ath10k *ar);
+int ath10k_leds_start(struct ath10k *ar);
+int ath10k_leds_register(struct ath10k *ar);
+#else
+static inline void ath10k_leds_unregister(struct ath10k *ar)
+{
+}
+
+static inline int ath10k_leds_start(struct ath10k *ar)
+{
+	return 0;
+}
+
+static inline int ath10k_leds_register(struct ath10k *ar)
+{
+	return 0;
+}
+
+#endif
+#endif /* _LEDS_H_ */
--- a/drivers/net/wireless/ath/ath10k/mac.c
+++ b/drivers/net/wireless/ath/ath10k/mac.c
@@ -24,6 +24,7 @@
 #include "wmi-tlv.h"
 #include "wmi-ops.h"
 #include "wow.h"
+#include "leds.h"
 
 /*********/
 /* Rates */
--- a/drivers/net/wireless/ath/ath10k/wmi-ops.h
+++ b/drivers/net/wireless/ath/ath10k/wmi-ops.h
@@ -226,7 +226,10 @@ struct wmi_ops {
 			 const struct wmi_bb_timing_cfg_arg *arg);
 	struct sk_buff *(*gen_per_peer_per_tid_cfg)(struct ath10k *ar,
 						    const struct wmi_per_peer_per_tid_cfg_arg *arg);
+	struct sk_buff *(*gen_gpio_config)(struct ath10k *ar, u32 gpio_num,
+					   u32 input, u32 pull_type, u32 intr_mode);
 
+	struct sk_buff *(*gen_gpio_output)(struct ath10k *ar, u32 gpio_num, u32 set);
 };
 
 int ath10k_wmi_cmd_send(struct ath10k *ar, struct sk_buff *skb, u32 cmd_id);
@@ -1122,6 +1125,35 @@ ath10k_wmi_force_fw_hang(struct ath10k *
 	return ath10k_wmi_cmd_send(ar, skb, ar->wmi.cmd->force_fw_hang_cmdid);
 }
 
+static inline int ath10k_wmi_gpio_config(struct ath10k *ar, u32 gpio_num,
+					 u32 input, u32 pull_type, u32 intr_mode)
+{
+	struct sk_buff *skb;
+
+	if (!ar->wmi.ops->gen_gpio_config)
+		return -EOPNOTSUPP;
+
+	skb = ar->wmi.ops->gen_gpio_config(ar, gpio_num, input, pull_type, intr_mode);
+	if (IS_ERR(skb))
+		return PTR_ERR(skb);
+
+	return ath10k_wmi_cmd_send(ar, skb, ar->wmi.cmd->gpio_config_cmdid);
+}
+
+static inline int ath10k_wmi_gpio_output(struct ath10k *ar, u32 gpio_num, u32 set)
+{
+	struct sk_buff *skb;
+
+	if (!ar->wmi.ops->gen_gpio_config)
+		return -EOPNOTSUPP;
+
+	skb = ar->wmi.ops->gen_gpio_output(ar, gpio_num, set);
+	if (IS_ERR(skb))
+		return PTR_ERR(skb);
+
+	return ath10k_wmi_cmd_send(ar, skb, ar->wmi.cmd->gpio_output_cmdid);
+}
+
 static inline int
 ath10k_wmi_dbglog_cfg(struct ath10k *ar, u64 module_enable, u32 log_level)
 {
--- a/drivers/net/wireless/ath/ath10k/wmi-tlv.c
+++ b/drivers/net/wireless/ath/ath10k/wmi-tlv.c
@@ -4594,6 +4594,8 @@ static const struct wmi_ops wmi_tlv_ops
 	.gen_echo = ath10k_wmi_tlv_op_gen_echo,
 	.gen_vdev_spectral_conf = ath10k_wmi_tlv_op_gen_vdev_spectral_conf,
 	.gen_vdev_spectral_enable = ath10k_wmi_tlv_op_gen_vdev_spectral_enable,
+	/* .gen_gpio_config not implemented */
+	/* .gen_gpio_output not implemented */
 };
 
 static const struct wmi_peer_flags_map wmi_tlv_peer_flags_map = {
--- a/drivers/net/wireless/ath/ath10k/wmi.c
+++ b/drivers/net/wireless/ath/ath10k/wmi.c
@@ -7472,6 +7472,49 @@ ath10k_wmi_op_gen_peer_set_param(struct
 	return skb;
 }
 
+static struct sk_buff *ath10k_wmi_op_gen_gpio_config(struct ath10k *ar,
+						     u32 gpio_num, u32 input,
+						     u32 pull_type, u32 intr_mode)
+{
+	struct wmi_gpio_config_cmd *cmd;
+	struct sk_buff *skb;
+
+	skb = ath10k_wmi_alloc_skb(ar, sizeof(*cmd));
+	if (!skb)
+		return ERR_PTR(-ENOMEM);
+
+	cmd = (struct wmi_gpio_config_cmd *)skb->data;
+	cmd->pull_type = __cpu_to_le32(pull_type);
+	cmd->gpio_num = __cpu_to_le32(gpio_num);
+	cmd->input = __cpu_to_le32(input);
+	cmd->intr_mode = __cpu_to_le32(intr_mode);
+
+	ath10k_dbg(ar, ATH10K_DBG_WMI, "wmi gpio_config gpio_num 0x%08x input 0x%08x pull_type 0x%08x intr_mode 0x%08x\n",
+		   gpio_num, input, pull_type, intr_mode);
+
+	return skb;
+}
+
+static struct sk_buff *ath10k_wmi_op_gen_gpio_output(struct ath10k *ar,
+						     u32 gpio_num, u32 set)
+{
+	struct wmi_gpio_output_cmd *cmd;
+	struct sk_buff *skb;
+
+	skb = ath10k_wmi_alloc_skb(ar, sizeof(*cmd));
+	if (!skb)
+		return ERR_PTR(-ENOMEM);
+
+	cmd = (struct wmi_gpio_output_cmd *)skb->data;
+	cmd->gpio_num = __cpu_to_le32(gpio_num);
+	cmd->set = __cpu_to_le32(set);
+
+	ath10k_dbg(ar, ATH10K_DBG_WMI, "wmi gpio_output gpio_num 0x%08x set 0x%08x\n",
+		   gpio_num, set);
+
+	return skb;
+}
+
 static struct sk_buff *
 ath10k_wmi_op_gen_set_psmode(struct ath10k *ar, u32 vdev_id,
 			     enum wmi_sta_ps_mode psmode)
@@ -9160,6 +9203,9 @@ static const struct wmi_ops wmi_ops = {
 	.fw_stats_fill = ath10k_wmi_main_op_fw_stats_fill,
 	.get_vdev_subtype = ath10k_wmi_op_get_vdev_subtype,
 	.gen_echo = ath10k_wmi_op_gen_echo,
+	.gen_gpio_config = ath10k_wmi_op_gen_gpio_config,
+	.gen_gpio_output = ath10k_wmi_op_gen_gpio_output,
+
 	/* .gen_bcn_tmpl not implemented */
 	/* .gen_prb_tmpl not implemented */
 	/* .gen_p2p_go_bcn_ie not implemented */
@@ -9230,6 +9276,8 @@ static const struct wmi_ops wmi_10_1_ops
 	.fw_stats_fill = ath10k_wmi_10x_op_fw_stats_fill,
 	.get_vdev_subtype = ath10k_wmi_op_get_vdev_subtype,
 	.gen_echo = ath10k_wmi_op_gen_echo,
+	.gen_gpio_config = ath10k_wmi_op_gen_gpio_config,
+	.gen_gpio_output = ath10k_wmi_op_gen_gpio_output,
 	/* .gen_bcn_tmpl not implemented */
 	/* .gen_prb_tmpl not implemented */
 	/* .gen_p2p_go_bcn_ie not implemented */
@@ -9302,6 +9350,8 @@ static const struct wmi_ops wmi_10_2_ops
 	.gen_delba_send = ath10k_wmi_op_gen_delba_send,
 	.fw_stats_fill = ath10k_wmi_10x_op_fw_stats_fill,
 	.get_vdev_subtype = ath10k_wmi_op_get_vdev_subtype,
+	.gen_gpio_config = ath10k_wmi_op_gen_gpio_config,
+	.gen_gpio_output = ath10k_wmi_op_gen_gpio_output,
 	/* .gen_pdev_enable_adaptive_cca not implemented */
 };
 
@@ -9373,6 +9423,8 @@ static const struct wmi_ops wmi_10_2_4_o
 		ath10k_wmi_op_gen_pdev_enable_adaptive_cca,
 	.get_vdev_subtype = ath10k_wmi_10_2_4_op_get_vdev_subtype,
 	.gen_bb_timing = ath10k_wmi_10_2_4_op_gen_bb_timing,
+	.gen_gpio_config = ath10k_wmi_op_gen_gpio_config,
+	.gen_gpio_output = ath10k_wmi_op_gen_gpio_output,
 	/* .gen_bcn_tmpl not implemented */
 	/* .gen_prb_tmpl not implemented */
 	/* .gen_p2p_go_bcn_ie not implemented */
@@ -9454,6 +9506,8 @@ static const struct wmi_ops wmi_10_4_ops
 	.gen_pdev_bss_chan_info_req = ath10k_wmi_10_2_op_gen_pdev_bss_chan_info,
 	.gen_echo = ath10k_wmi_op_gen_echo,
 	.gen_pdev_get_tpc_config = ath10k_wmi_10_2_4_op_gen_pdev_get_tpc_config,
+	.gen_gpio_config = ath10k_wmi_op_gen_gpio_config,
+	.gen_gpio_output = ath10k_wmi_op_gen_gpio_output,
 };
 
 int ath10k_wmi_attach(struct ath10k *ar)
--- a/drivers/net/wireless/ath/ath10k/wmi.h
+++ b/drivers/net/wireless/ath/ath10k/wmi.h
@@ -3030,6 +3030,41 @@ enum wmi_10_4_feature_mask {
 
 };
 
+/* WMI_GPIO_CONFIG_CMDID */
+enum {
+	WMI_GPIO_PULL_NONE,
+	WMI_GPIO_PULL_UP,
+	WMI_GPIO_PULL_DOWN,
+};
+
+enum {
+	WMI_GPIO_INTTYPE_DISABLE,
+	WMI_GPIO_INTTYPE_RISING_EDGE,
+	WMI_GPIO_INTTYPE_FALLING_EDGE,
+	WMI_GPIO_INTTYPE_BOTH_EDGE,
+	WMI_GPIO_INTTYPE_LEVEL_LOW,
+	WMI_GPIO_INTTYPE_LEVEL_HIGH
+};
+
+/* WMI_GPIO_CONFIG_CMDID */
+struct wmi_gpio_config_cmd {
+	__le32 gpio_num;             /* GPIO number to be setup */
+	__le32 input;                /* 0 - Output/ 1 - Input */
+	__le32 pull_type;            /* Pull type defined above */
+	__le32 intr_mode;            /* Interrupt mode defined above (Input) */
+} __packed;
+
+/* WMI_GPIO_OUTPUT_CMDID */
+struct wmi_gpio_output_cmd {
+	__le32 gpio_num;    /* GPIO number to be setup */
+	__le32 set;         /* Set the GPIO pin*/
+} __packed;
+
+/* WMI_GPIO_INPUT_EVENTID */
+struct wmi_gpio_input_event {
+	__le32 gpio_num;    /* GPIO number which changed state */
+} __packed;
+
 struct wmi_ext_resource_config_10_4_cmd {
 	/* contains enum wmi_host_platform_type */
 	__le32 host_platform_config;
