From 21fdd8281de3022aee35dd5bfccc892bd46529a3 Mon Sep 17 00:00:00 2001
From: "Russell King (Oracle)" <rmk+kernel@armlinux.org.uk>
Date: Fri, 26 Aug 2022 08:43:35 +0100
Subject: [PATCH 2/6] net: sfp: move Alcatel Lucent 3FE46541AA fixup

Add a new fixup mechanism to the SFP quirks, and use it for this
module.

Signed-off-by: Russell King (Oracle) <rmk+kernel@armlinux.org.uk>
---
 drivers/net/phy/sfp.c | 14 +++++++++-----
 drivers/net/phy/sfp.h |  1 +
 2 files changed, 10 insertions(+), 5 deletions(-)

--- a/drivers/net/phy/sfp.c
+++ b/drivers/net/phy/sfp.c
@@ -310,6 +310,11 @@ static const struct of_device_id sfp_of_
 };
 MODULE_DEVICE_TABLE(of, sfp_of_match);
 
+static void sfp_fixup_long_startup(struct sfp *sfp)
+{
+	sfp->module_t_start_up = T_START_UP_BAD_GPON;
+}
+
 static void sfp_quirk_2500basex(const struct sfp_eeprom_id *id,
 				unsigned long *modes)
 {
@@ -340,6 +345,7 @@ static const struct sfp_quirk sfp_quirks
 		.vendor = "ALCATELLUCENT",
 		.part = "3FE46541AA",
 		.modes = sfp_quirk_2500basex,
+		.fixup = sfp_fixup_long_startup,
 	}, {
 		// Huawei MA5671A can operate at 2500base-X, but report 1.2GBd
 		// NRZ in their EEPROM
@@ -2029,11 +2035,7 @@ static int sfp_sm_mod_probe(struct sfp *
 	if (ret < 0)
 		return ret;
 
-	if (!memcmp(id.base.vendor_name, "ALCATELLUCENT   ", 16) &&
-	    !memcmp(id.base.vendor_pn, "3FE46541AA      ", 16))
-		sfp->module_t_start_up = T_START_UP_BAD_GPON;
-	else
-		sfp->module_t_start_up = T_START_UP;
+	sfp->module_t_start_up = T_START_UP;
 
 	if (!memcmp(id.base.vendor_name, "HUAWEI          ", 16) &&
 	    !memcmp(id.base.vendor_pn, "MA5671A         ", 16))
@@ -2042,6 +2044,8 @@ static int sfp_sm_mod_probe(struct sfp *
 		sfp->tx_fault_ignore = false;
 
 	sfp->quirk = sfp_lookup_quirk(&id);
+	if (sfp->quirk && sfp->quirk->fixup)
+		sfp->quirk->fixup(sfp);
 
 	return 0;
 }
--- a/drivers/net/phy/sfp.h
+++ b/drivers/net/phy/sfp.h
@@ -10,6 +10,7 @@ struct sfp_quirk {
 	const char *vendor;
 	const char *part;
 	void (*modes)(const struct sfp_eeprom_id *id, unsigned long *modes);
+	void (*fixup)(struct sfp *sfp);
 };
 
 struct sfp_socket_ops {
