From 46953f97224d56a12ccbe9c6acaa84ca0dab2780 Mon Sep 17 00:00:00 2001
From: Kangjie Lu <kjlu@umn.edu>
Date: Fri, 15 Mar 2019 12:04:32 -0500
Subject: [PATCH] brcmfmac: fix missing checks for kmemdup

In case kmemdup fails, the fix sets conn_info->req_ie_len and
conn_info->resp_ie_len to zero to avoid buffer overflows.

Signed-off-by: Kangjie Lu <kjlu@umn.edu>
Acked-by: Arend van Spriel <arend.vanspriel@broadcom.com>
Signed-off-by: Kalle Valo <kvalo@codeaurora.org>
---
 drivers/net/wireless/broadcom/brcm80211/brcmfmac/cfg80211.c | 4 ++++
 1 file changed, 4 insertions(+)

--- a/drivers/net/wireless/broadcom/brcm80211/brcmfmac/cfg80211.c
+++ b/drivers/net/wireless/broadcom/brcm80211/brcmfmac/cfg80211.c
@@ -5455,6 +5455,8 @@ static s32 brcmf_get_assoc_ies(struct br
 		conn_info->req_ie =
 		    kmemdup(cfg->extra_buf, conn_info->req_ie_len,
 			    GFP_KERNEL);
+		if (!conn_info->req_ie)
+			conn_info->req_ie_len = 0;
 	} else {
 		conn_info->req_ie_len = 0;
 		conn_info->req_ie = NULL;
@@ -5471,6 +5473,8 @@ static s32 brcmf_get_assoc_ies(struct br
 		conn_info->resp_ie =
 		    kmemdup(cfg->extra_buf, conn_info->resp_ie_len,
 			    GFP_KERNEL);
+		if (!conn_info->resp_ie)
+			conn_info->resp_ie_len = 0;
 	} else {
 		conn_info->resp_ie_len = 0;
 		conn_info->resp_ie = NULL;
