From e3b1d879ccda9ffd5332777bb1beeb2cc913faa8 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <rafal@milecki.pl>
Date: Sun, 21 Jul 2019 21:52:17 +0200
Subject: [PATCH] brcmfmac: don't net_ratelimit() CONSOLE messages on firmware
 crash
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Firmware crash is a pretty rare event and can't happen too frequently as
it has to be followed by a hardware reinitialization and config reload.
It should be safe to don't use net_ratelimit() when it happens.

For reporting & debugging purposes it's important to provide a complete
log as the last lines are actually the most important. This change
modifies brcmfmac to print all messages in an unlimited way in that
specific case. With this change there should be finally a backtrace of
firmware finally visible after a crash.

Signed-off-by: Rafał Miłecki <rafal@milecki.pl>
Acked-by: Arend van Spriel <arend.vanspriel@broadcom.com>
Signed-off-by: Kalle Valo <kvalo@codeaurora.org>
---
 drivers/net/wireless/broadcom/brcm80211/brcmfmac/pcie.c | 3 ++-
 1 file changed, 2 insertions(+), 1 deletion(-)

--- a/drivers/net/wireless/broadcom/brcm80211/brcmfmac/pcie.c
+++ b/drivers/net/wireless/broadcom/brcm80211/brcmfmac/pcie.c
@@ -804,7 +804,8 @@ static void brcmf_pcie_bus_console_read(
 		if (ch == '\n') {
 			console->log_str[console->log_idx] = 0;
 			if (error)
-				brcmf_err(bus, "CONSOLE: %s", console->log_str);
+				__brcmf_err(bus, __func__, "CONSOLE: %s",
+					    console->log_str);
 			else
 				pr_debug("CONSOLE: %s", console->log_str);
 			console->log_idx = 0;
