From 5300a7cd7ed2f88488ddba62947b9c6bb9663777 Mon Sep 17 00:00:00 2001
Message-Id: <5300a7cd7ed2f88488ddba62947b9c6bb9663777.1396122227.git.mschiffer@universe-factory.net>
From: Matthias Schiffer <mschiffer@universe-factory.net>
Date: Sat, 29 Mar 2014 20:26:08 +0100
Subject: [PATCH 1/2] MIPS: ath79: add support for QCA953x SoC

Note that the clock calculation looks very similar to the QCA955x, but the
meaning of the bits CPUCLK_FROM_CPUPLL and DDRCLK_FROM_DDRPLL is reversed.
---
 arch/mips/ath79/Kconfig                        |  6 +-
 arch/mips/ath79/clock.c                        | 78 ++++++++++++++++++++++++++
 arch/mips/ath79/common.c                       |  4 ++
 arch/mips/ath79/dev-common.c                   |  1 +
 arch/mips/ath79/dev-wmac.c                     | 20 +++++++
 arch/mips/ath79/early_printk.c                 |  1 +
 arch/mips/ath79/gpio.c                         |  4 +-
 arch/mips/ath79/irq.c                          |  4 ++
 arch/mips/ath79/setup.c                        |  8 ++-
 arch/mips/include/asm/mach-ath79/ar71xx_regs.h | 48 ++++++++++++++++
 arch/mips/include/asm/mach-ath79/ath79.h       | 11 ++++
 11 files changed, 182 insertions(+), 3 deletions(-)

--- a/arch/mips/ath79/Kconfig
+++ b/arch/mips/ath79/Kconfig
@@ -104,6 +104,10 @@ config SOC_AR934X
 	select PCI_AR724X if PCI
 	def_bool n
 
+config SOC_QCA953X
+	select USB_ARCH_HAS_EHCI
+	def_bool n
+
 config SOC_QCA955X
 	select HW_HAS_PCI
 	select PCI_AR724X if PCI
@@ -143,7 +147,7 @@ config ATH79_DEV_USB
 	def_bool n
 
 config ATH79_DEV_WMAC
-	depends on (SOC_AR913X || SOC_AR933X || SOC_AR934X || SOC_QCA955X)
+	depends on (SOC_AR913X || SOC_AR933X || SOC_AR934X || SOC_QCA953X || SOC_QCA955X)
 	def_bool n
 
 config ATH79_NVRAM
--- a/arch/mips/ath79/clock.c
+++ b/arch/mips/ath79/clock.c
@@ -358,6 +358,87 @@ static void __init ar934x_clocks_init(vo
 	iounmap(dpll_base);
 }
 
+static void __init qca953x_clocks_init(void)
+{
+	unsigned long ref_rate;
+	unsigned long cpu_rate;
+	unsigned long ddr_rate;
+	unsigned long ahb_rate;
+	u32 pll, out_div, ref_div, nint, frac, clk_ctrl, postdiv;
+	u32 cpu_pll, ddr_pll;
+
+	/* QCA953X only supports 25MHz ref_clk */
+	ref_rate = 25 * 1000 * 1000;
+
+	pll = ath79_pll_rr(QCA953X_PLL_CPU_CONFIG_REG);
+	out_div = (pll >> QCA953X_PLL_CPU_CONFIG_OUTDIV_SHIFT) &
+		  QCA953X_PLL_CPU_CONFIG_OUTDIV_MASK;
+	ref_div = (pll >> QCA953X_PLL_CPU_CONFIG_REFDIV_SHIFT) &
+		  QCA953X_PLL_CPU_CONFIG_REFDIV_MASK;
+	nint = (pll >> QCA953X_PLL_CPU_CONFIG_NINT_SHIFT) &
+	       QCA953X_PLL_CPU_CONFIG_NINT_MASK;
+	frac = (pll >> QCA953X_PLL_CPU_CONFIG_NFRAC_SHIFT) &
+	       QCA953X_PLL_CPU_CONFIG_NFRAC_MASK;
+
+	cpu_pll = nint * ref_rate / ref_div;
+	cpu_pll += frac * (ref_rate >> 6) / ref_div;
+	cpu_pll /= (1 << out_div);
+
+	pll = ath79_pll_rr(QCA953X_PLL_DDR_CONFIG_REG);
+	out_div = (pll >> QCA953X_PLL_DDR_CONFIG_OUTDIV_SHIFT) &
+		  QCA953X_PLL_DDR_CONFIG_OUTDIV_MASK;
+	ref_div = (pll >> QCA953X_PLL_DDR_CONFIG_REFDIV_SHIFT) &
+		  QCA953X_PLL_DDR_CONFIG_REFDIV_MASK;
+	nint = (pll >> QCA953X_PLL_DDR_CONFIG_NINT_SHIFT) &
+	       QCA953X_PLL_DDR_CONFIG_NINT_MASK;
+	frac = (pll >> QCA953X_PLL_DDR_CONFIG_NFRAC_SHIFT) &
+	       QCA953X_PLL_DDR_CONFIG_NFRAC_MASK;
+
+	ddr_pll = nint * ref_rate / ref_div;
+	ddr_pll += frac * (ref_rate >> 6) / (ref_div << 4);
+	ddr_pll /= (1 << out_div);
+
+	clk_ctrl = ath79_pll_rr(QCA953X_PLL_CLK_CTRL_REG);
+
+	postdiv = (clk_ctrl >> QCA953X_PLL_CLK_CTRL_CPU_POST_DIV_SHIFT) &
+		  QCA953X_PLL_CLK_CTRL_CPU_POST_DIV_MASK;
+
+	if (clk_ctrl & QCA953X_PLL_CLK_CTRL_CPU_PLL_BYPASS)
+		cpu_rate = ref_rate;
+	else if (clk_ctrl & QCA953X_PLL_CLK_CTRL_CPUCLK_FROM_CPUPLL)
+		cpu_rate = cpu_pll / (postdiv + 1);
+	else
+		cpu_rate = ddr_pll / (postdiv + 1);
+
+	postdiv = (clk_ctrl >> QCA953X_PLL_CLK_CTRL_DDR_POST_DIV_SHIFT) &
+		  QCA953X_PLL_CLK_CTRL_DDR_POST_DIV_MASK;
+
+	if (clk_ctrl & QCA953X_PLL_CLK_CTRL_DDR_PLL_BYPASS)
+		ddr_rate = ref_rate;
+	else if (clk_ctrl & QCA953X_PLL_CLK_CTRL_DDRCLK_FROM_DDRPLL)
+		ddr_rate = ddr_pll / (postdiv + 1);
+	else
+		ddr_rate = cpu_pll / (postdiv + 1);
+
+	postdiv = (clk_ctrl >> QCA953X_PLL_CLK_CTRL_AHB_POST_DIV_SHIFT) &
+		  QCA953X_PLL_CLK_CTRL_AHB_POST_DIV_MASK;
+
+	if (clk_ctrl & QCA953X_PLL_CLK_CTRL_AHB_PLL_BYPASS)
+		ahb_rate = ref_rate;
+	else if (clk_ctrl & QCA953X_PLL_CLK_CTRL_AHBCLK_FROM_DDRPLL)
+		ahb_rate = ddr_pll / (postdiv + 1);
+	else
+		ahb_rate = cpu_pll / (postdiv + 1);
+
+	ath79_add_sys_clkdev("ref", ref_rate);
+	ath79_add_sys_clkdev("cpu", cpu_rate);
+	ath79_add_sys_clkdev("ddr", ddr_rate);
+	ath79_add_sys_clkdev("ahb", ahb_rate);
+
+	clk_add_alias("wdt", NULL, "ref", NULL);
+	clk_add_alias("uart", NULL, "ref", NULL);
+}
+
 static void __init qca955x_clocks_init(void)
 {
 	unsigned long ref_rate;
@@ -453,6 +534,8 @@ void __init ath79_clocks_init(void)
 		ar933x_clocks_init();
 	else if (soc_is_ar934x())
 		ar934x_clocks_init();
+	else if (soc_is_qca953x())
+		qca953x_clocks_init();
 	else if (soc_is_qca955x())
 		qca955x_clocks_init();
 	else
--- a/arch/mips/ath79/common.c
+++ b/arch/mips/ath79/common.c
@@ -103,6 +103,8 @@ void ath79_device_reset_set(u32 mask)
 		reg = AR933X_RESET_REG_RESET_MODULE;
 	else if (soc_is_ar934x())
 		reg = AR934X_RESET_REG_RESET_MODULE;
+	else if (soc_is_qca953x())
+		reg = QCA953X_RESET_REG_RESET_MODULE;
 	else if (soc_is_qca955x())
 		reg = QCA955X_RESET_REG_RESET_MODULE;
 	else
@@ -131,6 +133,8 @@ void ath79_device_reset_clear(u32 mask)
 		reg = AR933X_RESET_REG_RESET_MODULE;
 	else if (soc_is_ar934x())
 		reg = AR934X_RESET_REG_RESET_MODULE;
+	else if (soc_is_qca953x())
+		reg = QCA953X_RESET_REG_RESET_MODULE;
 	else if (soc_is_qca955x())
 		reg = QCA955X_RESET_REG_RESET_MODULE;
 	else
--- a/arch/mips/ath79/dev-common.c
+++ b/arch/mips/ath79/dev-common.c
@@ -94,6 +94,7 @@ void __init ath79_register_uart(void)
 	    soc_is_ar724x() ||
 	    soc_is_ar913x() ||
 	    soc_is_ar934x() ||
+	    soc_is_qca953x() ||
 	    soc_is_qca955x()) {
 		ath79_uart_data[0].uartclk = uart_clk_rate;
 		platform_device_register(&ath79_uart_device);
@@ -157,6 +158,9 @@ void __init ath79_gpio_init(void)
 	} else if (soc_is_ar934x()) {
 		ath79_gpio_pdata.ngpios = AR934X_GPIO_COUNT;
 		ath79_gpio_pdata.oe_inverted = 1;
+	} else if (soc_is_qca953x()) {
+		ath79_gpio_pdata.ngpios = QCA953X_GPIO_COUNT;
+		ath79_gpio_pdata.oe_inverted = 1;
 	} else if (soc_is_qca955x()) {
 		ath79_gpio_pdata.ngpios = QCA955X_GPIO_COUNT;
 		ath79_gpio_pdata.oe_inverted = 1;
--- a/arch/mips/ath79/dev-usb.c
+++ b/arch/mips/ath79/dev-usb.c
@@ -236,6 +236,30 @@ static void __init ar934x_usb_setup(void
 			   &ath79_ehci_pdata_v2, sizeof(ath79_ehci_pdata_v2));
 }
 
+static void __init qca953x_usb_setup(void)
+{
+	u32 bootstrap;
+
+	bootstrap = ath79_reset_rr(QCA953X_RESET_REG_BOOTSTRAP);
+
+	ath79_device_reset_set(QCA953X_RESET_USBSUS_OVERRIDE);
+	udelay(1000);
+
+	ath79_device_reset_clear(QCA953X_RESET_USB_PHY);
+	udelay(1000);
+
+	ath79_device_reset_clear(QCA953X_RESET_USB_PHY_ANALOG);
+	udelay(1000);
+
+	ath79_device_reset_clear(QCA953X_RESET_USB_HOST);
+	udelay(1000);
+
+	ath79_usb_register("ehci-platform", -1,
+			   QCA953X_EHCI_BASE, QCA953X_EHCI_SIZE,
+			   ATH79_CPU_IRQ(3),
+			   &ath79_ehci_pdata_v2, sizeof(ath79_ehci_pdata_v2));
+}
+
 static void qca955x_usb_reset_notifier(struct platform_device *pdev)
 {
 	u32 base;
@@ -286,6 +310,8 @@ void __init ath79_register_usb(void)
 		ar933x_usb_setup();
 	else if (soc_is_ar934x())
 		ar934x_usb_setup();
+	else if (soc_is_qca953x())
+		qca953x_usb_setup();
 	else if (soc_is_qca955x())
 		qca955x_usb_setup();
 	else
--- a/arch/mips/ath79/dev-wmac.c
+++ b/arch/mips/ath79/dev-wmac.c
@@ -100,7 +100,7 @@ static int ar933x_wmac_reset(void)
 	return -ETIMEDOUT;
 }
 
-static int ar933x_r1_get_wmac_revision(void)
+static int ar93xx_get_soc_revision(void)
 {
 	return ath79_soc_rev;
 }
@@ -125,7 +125,7 @@ static void __init ar933x_wmac_setup(voi
 		ath79_wmac_data.is_clk_25mhz = true;
 
 	if (ath79_soc_rev == 1)
-		ath79_wmac_data.get_mac_revision = ar933x_r1_get_wmac_revision;
+		ath79_wmac_data.get_mac_revision = ar93xx_get_soc_revision;
 
 	ath79_wmac_data.external_reset = ar933x_wmac_reset;
 }
@@ -150,6 +150,21 @@ static void ar934x_wmac_setup(void)
 	ath79_wmac_data.get_mac_revision = ar93xx_get_soc_revision;
 }
 
+static void qca953x_wmac_setup(void)
+{
+	ath79_wmac_device.name = "qca953x_wmac";
+
+	ath79_wmac_resources[0].start = QCA953X_WMAC_BASE;
+	ath79_wmac_resources[0].end = QCA953X_WMAC_BASE + QCA953X_WMAC_SIZE - 1;
+	ath79_wmac_resources[1].start = ATH79_IP2_IRQ(1);
+	ath79_wmac_resources[1].end = ATH79_IP2_IRQ(1);
+
+	/* QCA953X only supports 25MHz ref_clk */
+	ath79_wmac_data.is_clk_25mhz = true;
+
+	ath79_wmac_data.get_mac_revision = ar93xx_get_soc_revision;
+}
+
 static void qca955x_wmac_setup(void)
 {
 	u32 t;
@@ -379,6 +394,8 @@ void __init ath79_register_wmac(u8 *cal_
 		ar933x_wmac_setup();
 	else if (soc_is_ar934x())
 		ar934x_wmac_setup();
+	else if (soc_is_qca953x())
+		qca953x_wmac_setup();
 	else if (soc_is_qca955x())
 		qca955x_wmac_setup();
 	else
--- a/arch/mips/ath79/early_printk.c
+++ b/arch/mips/ath79/early_printk.c
@@ -116,6 +116,8 @@ static void prom_putchar_init(void)
 	case REV_ID_MAJOR_AR9341:
 	case REV_ID_MAJOR_AR9342:
 	case REV_ID_MAJOR_AR9344:
+	case REV_ID_MAJOR_QCA9533:
+	case REV_ID_MAJOR_QCA9533_V2:
 	case REV_ID_MAJOR_QCA9556:
 	case REV_ID_MAJOR_QCA9558:
 		_prom_putchar = prom_putchar_ar71xx;
--- a/arch/mips/ath79/gpio.c
+++ b/arch/mips/ath79/gpio.c
@@ -31,7 +31,7 @@ static void __iomem *ath79_gpio_get_func
 	    soc_is_ar913x() ||
 	    soc_is_ar933x())
 		reg = AR71XX_GPIO_REG_FUNC;
-	else if (soc_is_ar934x())
+	else if (soc_is_ar934x() || soc_is_qca953x())
 		reg = AR934X_GPIO_REG_FUNC;
 	else
 		BUG();
@@ -64,7 +64,7 @@ void __init ath79_gpio_output_select(uns
 	unsigned int reg;
 	u32 t, s;
 
-	BUG_ON(!soc_is_ar934x());
+	BUG_ON(!soc_is_ar934x() && !soc_is_qca953x());
 
 	if (gpio >= AR934X_GPIO_COUNT)
 		return;
--- a/arch/mips/ath79/irq.c
+++ b/arch/mips/ath79/irq.c
@@ -62,6 +62,34 @@ static void ar934x_ip2_irq_init(void)
 	irq_set_chained_handler(ATH79_CPU_IRQ(2), ar934x_ip2_irq_dispatch);
 }
 
+static void qca953x_ip2_irq_dispatch(struct irq_desc *desc)
+{
+	u32 status;
+
+	status = ath79_reset_rr(QCA953X_RESET_REG_PCIE_WMAC_INT_STATUS);
+
+	if (status & QCA953X_PCIE_WMAC_INT_PCIE_ALL) {
+		ath79_ddr_wb_flush(3);
+		generic_handle_irq(ATH79_IP2_IRQ(0));
+	} else if (status & QCA953X_PCIE_WMAC_INT_WMAC_ALL) {
+		ath79_ddr_wb_flush(4);
+		generic_handle_irq(ATH79_IP2_IRQ(1));
+	} else {
+		spurious_interrupt();
+	}
+}
+
+static void qca953x_irq_init(void)
+{
+	int i;
+
+	for (i = ATH79_IP2_IRQ_BASE;
+	     i < ATH79_IP2_IRQ_BASE + ATH79_IP2_IRQ_COUNT; i++)
+		irq_set_chip_and_handler(i, &dummy_irq_chip, handle_level_irq);
+
+	irq_set_chained_handler(ATH79_CPU_IRQ(2), qca953x_ip2_irq_dispatch);
+}
+
 static void qca955x_ip2_irq_dispatch(struct irq_desc *desc)
 {
 	u32 status;
@@ -149,7 +177,7 @@ void __init arch_init_irq(void)
 	    soc_is_ar913x() || soc_is_ar933x()) {
 		irq_wb_chan2 = 3;
 		irq_wb_chan3 = 2;
-	} else if (soc_is_ar934x()) {
+	} else if (soc_is_ar934x() || soc_is_qca953x()) {
 		irq_wb_chan3 = 2;
 	}
 
@@ -160,6 +188,7 @@ void __init arch_init_irq(void)
 	else if (soc_is_ar724x() ||
 		 soc_is_ar933x() ||
 		 soc_is_ar934x() ||
+		 soc_is_qca953x() ||
 		 soc_is_qca955x())
 		misc_is_ar71xx = false;
 	else
@@ -170,6 +199,8 @@ void __init arch_init_irq(void)
 
 	if (soc_is_ar934x())
 		ar934x_ip2_irq_init();
+	else if (soc_is_qca953x())
+		qca953x_irq_init();
 	else if (soc_is_qca955x())
 		qca955x_irq_init();
 }
--- a/arch/mips/ath79/setup.c
+++ b/arch/mips/ath79/setup.c
@@ -60,6 +60,7 @@ static void __init ath79_detect_sys_type
 	u32 major;
 	u32 minor;
 	u32 rev = 0;
+	u32 ver = 1;
 
 	id = ath79_reset_rr(AR71XX_RESET_REG_REV_ID);
 	major = id & REV_ID_MAJOR_MASK;
@@ -152,6 +153,17 @@ static void __init ath79_detect_sys_type
 		rev = id & AR934X_REV_ID_REVISION_MASK;
 		break;
 
+	case REV_ID_MAJOR_QCA9533_V2:
+		ver = 2;
+		ath79_soc_rev = 2;
+		/* drop through */
+
+	case REV_ID_MAJOR_QCA9533:
+		ath79_soc = ATH79_SOC_QCA9533;
+		chip = "9533";
+		rev = id & QCA953X_REV_ID_REVISION_MASK;
+		break;
+
 	case REV_ID_MAJOR_QCA9556:
 		ath79_soc = ATH79_SOC_QCA9556;
 		chip = "9556";
@@ -168,11 +180,12 @@ static void __init ath79_detect_sys_type
 		panic("ath79: unknown SoC, id:0x%08x", id);
 	}
 
-	ath79_soc_rev = rev;
+	if (ver == 1)
+		ath79_soc_rev = rev;
 
-	if (soc_is_qca955x())
-		sprintf(ath79_sys_type, "Qualcomm Atheros QCA%s rev %u",
-			chip, rev);
+	if (soc_is_qca953x() || soc_is_qca955x())
+		sprintf(ath79_sys_type, "Qualcomm Atheros QCA%s ver %u rev %u",
+			chip, ver, rev);
 	else
 		sprintf(ath79_sys_type, "Atheros AR%s rev %u", chip, rev);
 	pr_info("SoC: %s\n", ath79_sys_type);
--- a/arch/mips/include/asm/mach-ath79/ar71xx_regs.h
+++ b/arch/mips/include/asm/mach-ath79/ar71xx_regs.h
@@ -105,6 +105,21 @@
 #define AR934X_SRIF_BASE	(AR71XX_APB_BASE + 0x00116000)
 #define AR934X_SRIF_SIZE	0x1000
 
+#define QCA953X_GMAC_BASE	(AR71XX_APB_BASE + 0x00070000)
+#define QCA953X_GMAC_SIZE	0x14
+#define QCA953X_WMAC_BASE	(AR71XX_APB_BASE + 0x00100000)
+#define QCA953X_WMAC_SIZE	0x20000
+#define QCA953X_EHCI_BASE	0x1b000000
+#define QCA953X_EHCI_SIZE	0x200
+#define QCA953X_SRIF_BASE	(AR71XX_APB_BASE + 0x00116000)
+#define QCA953X_SRIF_SIZE	0x1000
+
+#define QCA953X_PCI_CFG_BASE0	0x14000000
+#define QCA953X_PCI_CTRL_BASE0	(AR71XX_APB_BASE + 0x000f0000)
+#define QCA953X_PCI_CRP_BASE0	(AR71XX_APB_BASE + 0x000c0000)
+#define QCA953X_PCI_MEM_BASE0	0x10000000
+#define QCA953X_PCI_MEM_SIZE	0x02000000
+
 #define QCA955X_PCI_MEM_BASE0	0x10000000
 #define QCA955X_PCI_MEM_BASE1	0x12000000
 #define QCA955X_PCI_MEM_SIZE	0x02000000
@@ -180,6 +195,12 @@
 #define AR934X_OTP_INTF3_ADDRESS			0x3100c
 #define AR934X_OTP_PGENB_SETUP_HOLD_TIME_ADDRESS	0x31034
 
+#define QCA953X_DDR_REG_FLUSH_GE0	0x9c
+#define QCA953X_DDR_REG_FLUSH_GE1	0xa0
+#define QCA953X_DDR_REG_FLUSH_USB	0xa4
+#define QCA953X_DDR_REG_FLUSH_PCIE	0xa8
+#define QCA953X_DDR_REG_FLUSH_WMAC	0xac
+
 /*
  * PLL block
  */
@@ -289,6 +310,44 @@
 
 #define AR934X_PLL_SWITCH_CLOCK_CONTROL_MDIO_CLK_SEL	BIT(6)
 
+#define QCA953X_PLL_CPU_CONFIG_REG		0x00
+#define QCA953X_PLL_DDR_CONFIG_REG		0x04
+#define QCA953X_PLL_CLK_CTRL_REG		0x08
+#define QCA953X_PLL_SWITCH_CLOCK_CONTROL_REG	0x24
+#define QCA953X_PLL_ETH_XMII_CONTROL_REG	0x2c
+#define QCA953X_PLL_ETH_SGMII_CONTROL_REG	0x48
+
+#define QCA953X_PLL_CPU_CONFIG_NFRAC_SHIFT	0
+#define QCA953X_PLL_CPU_CONFIG_NFRAC_MASK	0x3f
+#define QCA953X_PLL_CPU_CONFIG_NINT_SHIFT	6
+#define QCA953X_PLL_CPU_CONFIG_NINT_MASK	0x3f
+#define QCA953X_PLL_CPU_CONFIG_REFDIV_SHIFT	12
+#define QCA953X_PLL_CPU_CONFIG_REFDIV_MASK	0x1f
+#define QCA953X_PLL_CPU_CONFIG_OUTDIV_SHIFT	19
+#define QCA953X_PLL_CPU_CONFIG_OUTDIV_MASK	0x7
+
+#define QCA953X_PLL_DDR_CONFIG_NFRAC_SHIFT	0
+#define QCA953X_PLL_DDR_CONFIG_NFRAC_MASK	0x3ff
+#define QCA953X_PLL_DDR_CONFIG_NINT_SHIFT	10
+#define QCA953X_PLL_DDR_CONFIG_NINT_MASK	0x3f
+#define QCA953X_PLL_DDR_CONFIG_REFDIV_SHIFT	16
+#define QCA953X_PLL_DDR_CONFIG_REFDIV_MASK	0x1f
+#define QCA953X_PLL_DDR_CONFIG_OUTDIV_SHIFT	23
+#define QCA953X_PLL_DDR_CONFIG_OUTDIV_MASK	0x7
+
+#define QCA953X_PLL_CLK_CTRL_CPU_PLL_BYPASS		BIT(2)
+#define QCA953X_PLL_CLK_CTRL_DDR_PLL_BYPASS		BIT(3)
+#define QCA953X_PLL_CLK_CTRL_AHB_PLL_BYPASS		BIT(4)
+#define QCA953X_PLL_CLK_CTRL_CPU_POST_DIV_SHIFT		5
+#define QCA953X_PLL_CLK_CTRL_CPU_POST_DIV_MASK		0x1f
+#define QCA953X_PLL_CLK_CTRL_DDR_POST_DIV_SHIFT		10
+#define QCA953X_PLL_CLK_CTRL_DDR_POST_DIV_MASK		0x1f
+#define QCA953X_PLL_CLK_CTRL_AHB_POST_DIV_SHIFT		15
+#define QCA953X_PLL_CLK_CTRL_AHB_POST_DIV_MASK		0x1f
+#define QCA953X_PLL_CLK_CTRL_CPUCLK_FROM_CPUPLL		BIT(20)
+#define QCA953X_PLL_CLK_CTRL_DDRCLK_FROM_DDRPLL		BIT(21)
+#define QCA953X_PLL_CLK_CTRL_AHBCLK_FROM_DDRPLL		BIT(24)
+
 #define QCA955X_PLL_CPU_CONFIG_REG		0x00
 #define QCA955X_PLL_DDR_CONFIG_REG		0x04
 #define QCA955X_PLL_CLK_CTRL_REG		0x08
@@ -365,6 +424,10 @@
 #define AR934X_RESET_REG_BOOTSTRAP		0xb0
 #define AR934X_RESET_REG_PCIE_WMAC_INT_STATUS	0xac
 
+#define QCA953X_RESET_REG_RESET_MODULE		0x1c
+#define QCA953X_RESET_REG_BOOTSTRAP		0xb0
+#define QCA953X_RESET_REG_PCIE_WMAC_INT_STATUS	0xac
+
 #define QCA955X_RESET_REG_RESET_MODULE		0x1c
 #define QCA955X_RESET_REG_BOOTSTRAP		0xb0
 #define QCA955X_RESET_REG_EXT_INT_STATUS	0xac
@@ -460,6 +523,27 @@
 #define AR934X_RESET_MBOX		BIT(1)
 #define AR934X_RESET_I2S		BIT(0)
 
+#define QCA953X_RESET_USB_EXT_PWR	BIT(29)
+#define QCA953X_RESET_EXTERNAL		BIT(28)
+#define QCA953X_RESET_RTC		BIT(27)
+#define QCA953X_RESET_FULL_CHIP		BIT(24)
+#define QCA953X_RESET_GE1_MDIO		BIT(23)
+#define QCA953X_RESET_GE0_MDIO		BIT(22)
+#define QCA953X_RESET_CPU_NMI		BIT(21)
+#define QCA953X_RESET_CPU_COLD		BIT(20)
+#define QCA953X_RESET_DDR		BIT(16)
+#define QCA953X_RESET_USB_PHY_PLL_PWD_EXT BIT(15)
+#define QCA953X_RESET_GE1_MAC		BIT(13)
+#define QCA953X_RESET_ETH_SWITCH_ANALOG	BIT(12)
+#define QCA953X_RESET_USB_PHY_ANALOG	BIT(11)
+#define QCA953X_RESET_GE0_MAC		BIT(9)
+#define QCA953X_RESET_ETH_SWITCH	BIT(8)
+#define QCA953X_RESET_PCIE_PHY		BIT(7)
+#define QCA953X_RESET_PCIE		BIT(6)
+#define QCA953X_RESET_USB_HOST		BIT(5)
+#define QCA953X_RESET_USB_PHY		BIT(4)
+#define QCA953X_RESET_USBSUS_OVERRIDE	BIT(3)
+
 #define QCA955X_RESET_HOST		BIT(31)
 #define QCA955X_RESET_SLIC		BIT(30)
 #define QCA955X_RESET_HDMA		BIT(29)
@@ -513,6 +597,13 @@
 #define AR934X_BOOTSTRAP_SDRAM_DISABLED BIT(1)
 #define AR934X_BOOTSTRAP_DDR1		BIT(0)
 
+#define QCA953X_BOOTSTRAP_SW_OPTION2	BIT(12)
+#define QCA953X_BOOTSTRAP_SW_OPTION1	BIT(11)
+#define QCA953X_BOOTSTRAP_EJTAG_MODE	BIT(5)
+#define QCA953X_BOOTSTRAP_REF_CLK	BIT(4)
+#define QCA953X_BOOTSTRAP_SDRAM_DISABLED BIT(1)
+#define QCA953X_BOOTSTRAP_DDR1		BIT(0)
+
 #define QCA955X_BOOTSTRAP_REF_CLK_40	BIT(4)
 
 #define AR934X_PCIE_WMAC_INT_WMAC_MISC		BIT(0)
@@ -533,6 +624,24 @@
 	 AR934X_PCIE_WMAC_INT_PCIE_RC1 | AR934X_PCIE_WMAC_INT_PCIE_RC2 | \
 	 AR934X_PCIE_WMAC_INT_PCIE_RC3)
 
+#define QCA953X_PCIE_WMAC_INT_WMAC_MISC		BIT(0)
+#define QCA953X_PCIE_WMAC_INT_WMAC_TX		BIT(1)
+#define QCA953X_PCIE_WMAC_INT_WMAC_RXLP		BIT(2)
+#define QCA953X_PCIE_WMAC_INT_WMAC_RXHP		BIT(3)
+#define QCA953X_PCIE_WMAC_INT_PCIE_RC		BIT(4)
+#define QCA953X_PCIE_WMAC_INT_PCIE_RC0		BIT(5)
+#define QCA953X_PCIE_WMAC_INT_PCIE_RC1		BIT(6)
+#define QCA953X_PCIE_WMAC_INT_PCIE_RC2		BIT(7)
+#define QCA953X_PCIE_WMAC_INT_PCIE_RC3		BIT(8)
+#define QCA953X_PCIE_WMAC_INT_WMAC_ALL \
+	(QCA953X_PCIE_WMAC_INT_WMAC_MISC | QCA953X_PCIE_WMAC_INT_WMAC_TX | \
+	 QCA953X_PCIE_WMAC_INT_WMAC_RXLP | QCA953X_PCIE_WMAC_INT_WMAC_RXHP)
+
+#define QCA953X_PCIE_WMAC_INT_PCIE_ALL \
+	(QCA953X_PCIE_WMAC_INT_PCIE_RC | QCA953X_PCIE_WMAC_INT_PCIE_RC0 | \
+	 QCA953X_PCIE_WMAC_INT_PCIE_RC1 | QCA953X_PCIE_WMAC_INT_PCIE_RC2 | \
+	 QCA953X_PCIE_WMAC_INT_PCIE_RC3)
+
 #define QCA955X_EXT_INT_WMAC_MISC		BIT(0)
 #define QCA955X_EXT_INT_WMAC_TX			BIT(1)
 #define QCA955X_EXT_INT_WMAC_RXLP		BIT(2)
@@ -575,6 +684,8 @@
 #define REV_ID_MAJOR_AR9341		0x0120
 #define REV_ID_MAJOR_AR9342		0x1120
 #define REV_ID_MAJOR_AR9344		0x2120
+#define REV_ID_MAJOR_QCA9533		0x0140
+#define REV_ID_MAJOR_QCA9533_V2		0x0160
 #define REV_ID_MAJOR_QCA9556		0x0130
 #define REV_ID_MAJOR_QCA9558		0x1130
 
@@ -597,6 +708,8 @@
 
 #define AR934X_REV_ID_REVISION_MASK	0xf
 
+#define QCA953X_REV_ID_REVISION_MASK	0xf
+
 #define QCA955X_REV_ID_REVISION_MASK	0xf
 
 /*
@@ -644,6 +757,25 @@
 #define AR934X_GPIO_REG_OUT_FUNC5	0x40
 #define AR934X_GPIO_REG_FUNC		0x6c
 
+#define QCA953X_GPIO_REG_OUT_FUNC0	0x2c
+#define QCA953X_GPIO_REG_OUT_FUNC1	0x30
+#define QCA953X_GPIO_REG_OUT_FUNC2	0x34
+#define QCA953X_GPIO_REG_OUT_FUNC3	0x38
+#define QCA953X_GPIO_REG_OUT_FUNC4	0x3c
+#define QCA953X_GPIO_REG_IN_ENABLE0	0x44
+#define QCA953X_GPIO_REG_FUNC		0x6c
+
+#define QCA953X_GPIO_OUT_MUX_SPI_CS1		10
+#define QCA953X_GPIO_OUT_MUX_SPI_CS2		11
+#define QCA953X_GPIO_OUT_MUX_SPI_CS0		9
+#define QCA953X_GPIO_OUT_MUX_SPI_CLK		8
+#define QCA953X_GPIO_OUT_MUX_SPI_MOSI		12
+#define QCA953X_GPIO_OUT_MUX_LED_LINK1		41
+#define QCA953X_GPIO_OUT_MUX_LED_LINK2		42
+#define QCA953X_GPIO_OUT_MUX_LED_LINK3		43
+#define QCA953X_GPIO_OUT_MUX_LED_LINK4		44
+#define QCA953X_GPIO_OUT_MUX_LED_LINK5		45
+
 #define QCA955X_GPIO_REG_OUT_FUNC0	0x2c
 #define QCA955X_GPIO_REG_OUT_FUNC1	0x30
 #define QCA955X_GPIO_REG_OUT_FUNC2	0x34
@@ -658,6 +790,7 @@
 #define AR913X_GPIO_COUNT		22
 #define AR933X_GPIO_COUNT		30
 #define AR934X_GPIO_COUNT		23
+#define QCA953X_GPIO_COUNT		18
 #define QCA955X_GPIO_COUNT		24
 
 /*
@@ -681,6 +814,24 @@
 #define AR934X_SRIF_DPLL2_OUTDIV_SHIFT	13
 #define AR934X_SRIF_DPLL2_OUTDIV_MASK	0x7
 
+#define QCA953X_SRIF_CPU_DPLL1_REG	0x1c0
+#define QCA953X_SRIF_CPU_DPLL2_REG	0x1c4
+#define QCA953X_SRIF_CPU_DPLL3_REG	0x1c8
+
+#define QCA953X_SRIF_DDR_DPLL1_REG	0x240
+#define QCA953X_SRIF_DDR_DPLL2_REG	0x244
+#define QCA953X_SRIF_DDR_DPLL3_REG	0x248
+
+#define QCA953X_SRIF_DPLL1_REFDIV_SHIFT	27
+#define QCA953X_SRIF_DPLL1_REFDIV_MASK	0x1f
+#define QCA953X_SRIF_DPLL1_NINT_SHIFT	18
+#define QCA953X_SRIF_DPLL1_NINT_MASK	0x1ff
+#define QCA953X_SRIF_DPLL1_NFRAC_MASK	0x0003ffff
+
+#define QCA953X_SRIF_DPLL2_LOCAL_PLL	BIT(30)
+#define QCA953X_SRIF_DPLL2_OUTDIV_SHIFT	13
+#define QCA953X_SRIF_DPLL2_OUTDIV_MASK	0x7
+
 #define AR71XX_GPIO_FUNC_STEREO_EN		BIT(17)
 #define AR71XX_GPIO_FUNC_SLIC_EN		BIT(16)
 #define AR71XX_GPIO_FUNC_SPI_CS2_EN		BIT(13)
@@ -887,6 +1038,16 @@
 #define AR934X_ETH_CFG_RDV_DELAY_SHIFT  16
 
 /*
+ * QCA953X GMAC Interface
+ */
+#define QCA953X_GMAC_REG_ETH_CFG		0x00
+
+#define QCA953X_ETH_CFG_SW_ONLY_MODE		BIT(6)
+#define QCA953X_ETH_CFG_SW_PHY_SWAP		BIT(7)
+#define QCA953X_ETH_CFG_SW_APB_ACCESS		BIT(9)
+#define QCA953X_ETH_CFG_SW_ACC_MSB_FIRST	BIT(13)
+
+/*
  * QCA955X GMAC Interface
  */
 
--- a/arch/mips/include/asm/mach-ath79/ath79.h
+++ b/arch/mips/include/asm/mach-ath79/ath79.h
@@ -32,6 +32,7 @@ enum ath79_soc_type {
 	ATH79_SOC_AR9341,
 	ATH79_SOC_AR9342,
 	ATH79_SOC_AR9344,
+	ATH79_SOC_QCA9533,
 	ATH79_SOC_QCA9556,
 	ATH79_SOC_QCA9558,
 };
@@ -100,6 +101,16 @@ static inline int soc_is_ar934x(void)
 	return soc_is_ar9341() || soc_is_ar9342() || soc_is_ar9344();
 }
 
+static inline int soc_is_qca9533(void)
+{
+	return ath79_soc == ATH79_SOC_QCA9533;
+}
+
+static inline int soc_is_qca953x(void)
+{
+	return soc_is_qca9533();
+}
+
 static inline int soc_is_qca9556(void)
 {
 	return ath79_soc == ATH79_SOC_QCA9556;
