/dts-v1/;

#include "bcm6368.dtsi"

#include <dt-bindings/input/input.h>

/ {
	model = "Broadcom BCM96368MVNgr reference board";
	compatible = "brcm,bcm96368mvngr", "brcm,bcm6368";

	chosen {
		bootargs = "rootfstype=squashfs,jffs2 noinitrd console=ttyS0,115200";
		stdout-path = "serial0:115200n8";
	};

	gpio-leds {
		compatible = "gpio-leds";

		dsl_green {
			label = "96368MVNgr:green:adsl";
			gpios = <&pinctrl 2 1>;
		};
		inet_fail_green {
			label = "96368MVNgr:green:inet-fail";
			gpios = <&pinctrl 3 0>;
		};
		inet_green {
			label = "96368MVNgr:green:inet";
			gpios = <&pinctrl 5 0>;
		};
		power_green {
			label = "96368MVNgr:green:power";
			gpios = <&pinctrl 22 0>;
			default-state = "on";
		};
		wps_green {
			label = "96368MVNgr:green:wps";
			gpios = <&pinctrl 23 1>;
		};
	};
};

&pflash {
	status = "ok";

	partitions {
		compatible = "brcm,bcm963xx-cfe-nor-partitions";
	};
};

&pinctrl {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_pci>;
};

&uart0 {
	status = "ok";
};
