From 45e934873f9147f692dddbb61abc088f4c8059d7 Mon Sep 17 00:00:00 2001
From: Yangbo Lu <yangbo.lu@nxp.com>
Date: Wed, 17 Jan 2018 14:51:29 +0800
Subject: [PATCH 03/30] arch: support layerscape
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

This is an integrated patch for layerscape arch support.

Signed-off-by: Madalin Bucur <madalin.bucur@nxp.com>
Signed-off-by: Nipun Gupta <nipun.gupta@nxp.com>
Signed-off-by: Zhao Qiang <B45475@freescale.com>
Signed-off-by: Camelia Groza <camelia.groza@nxp.com>
Signed-off-by: Haiying Wang <Haiying.wang@freescale.com>
Signed-off-by: Pan Jiafei <Jiafei.Pan@nxp.com>
Signed-off-by: Po Liu <po.liu@nxp.com>
Signed-off-by: Bharat Bhushan <Bharat.Bhushan@nxp.com>
Signed-off-by: Jianhua Xie <jianhua.xie@nxp.com>
Signed-off-by: Horia Geantă <horia.geanta@nxp.com>
Signed-off-by: Yangbo Lu <yangbo.lu@nxp.com>
---
 arch/arm/include/asm/delay.h          | 16 +++++++++
 arch/arm/include/asm/io.h             | 31 ++++++++++++++++++
 arch/arm/include/asm/mach/map.h       |  4 +--
 arch/arm/include/asm/pgtable.h        |  7 ++++
 arch/arm/kernel/bios32.c              | 43 ++++++++++++++++++++++++
 arch/arm/mm/dma-mapping.c             |  1 +
 arch/arm/mm/ioremap.c                 |  7 ++++
 arch/arm/mm/mmu.c                     |  9 +++++
 arch/arm64/include/asm/cache.h        |  2 +-
 arch/arm64/include/asm/io.h           | 30 +++++++++++++++++
 arch/arm64/include/asm/pci.h          |  4 +++
 arch/arm64/include/asm/pgtable-prot.h |  1 +
 arch/arm64/include/asm/pgtable.h      |  5 +++
 arch/arm64/kernel/pci.c               | 62 +++++++++++++++++++++++++++++++++++
 arch/arm64/mm/dma-mapping.c           |  6 ++++
 15 files changed, 225 insertions(+), 3 deletions(-)

--- a/arch/arm/include/asm/delay.h
+++ b/arch/arm/include/asm/delay.h
@@ -57,6 +57,22 @@ extern void __bad_udelay(void);
 			__const_udelay((n) * UDELAY_MULT)) :		\
 	  __udelay(n))
 
+#define spin_event_timeout(condition, timeout, delay)                          \
+({                                                                             \
+	typeof(condition) __ret;                                               \
+	int i = 0;							       \
+	while (!(__ret = (condition)) && (i++ < timeout)) {		       \
+		if (delay)                                                     \
+			udelay(delay);                                         \
+		else                                                           \
+			cpu_relax();					       \
+		udelay(1);						       \
+	}								       \
+	if (!__ret)                                                            \
+		__ret = (condition);                                           \
+	__ret;		                                                       \
+})
+
 /* Loop-based definitions for assembly code. */
 extern void __loop_delay(unsigned long loops);
 extern void __loop_udelay(unsigned long usecs);
--- a/arch/arm/include/asm/io.h
+++ b/arch/arm/include/asm/io.h
@@ -129,6 +129,7 @@ static inline u32 __raw_readl(const vola
 #define MT_DEVICE_NONSHARED	1
 #define MT_DEVICE_CACHED	2
 #define MT_DEVICE_WC		3
+#define MT_MEMORY_RW_NS		4
 /*
  * types 4 onwards can be found in asm/mach/map.h and are undefined
  * for ioremap
@@ -220,6 +221,34 @@ extern int pci_ioremap_io(unsigned int o
 #endif
 #endif
 
+/* access ports */
+#define setbits32(_addr, _v) iowrite32be(ioread32be(_addr) |  (_v), (_addr))
+#define clrbits32(_addr, _v) iowrite32be(ioread32be(_addr) & ~(_v), (_addr))
+
+#define setbits16(_addr, _v) iowrite16be(ioread16be(_addr) |  (_v), (_addr))
+#define clrbits16(_addr, _v) iowrite16be(ioread16be(_addr) & ~(_v), (_addr))
+
+#define setbits8(_addr, _v) iowrite8(ioread8(_addr) |  (_v), (_addr))
+#define clrbits8(_addr, _v) iowrite8(ioread8(_addr) & ~(_v), (_addr))
+
+/* Clear and set bits in one shot.  These macros can be used to clear and
+ * set multiple bits in a register using a single read-modify-write.  These
+ * macros can also be used to set a multiple-bit bit pattern using a mask,
+ * by specifying the mask in the 'clear' parameter and the new bit pattern
+ * in the 'set' parameter.
+ */
+
+#define clrsetbits_be32(addr, clear, set) \
+	iowrite32be((ioread32be(addr) & ~(clear)) | (set), (addr))
+#define clrsetbits_le32(addr, clear, set) \
+	iowrite32le((ioread32le(addr) & ~(clear)) | (set), (addr))
+#define clrsetbits_be16(addr, clear, set) \
+	iowrite16be((ioread16be(addr) & ~(clear)) | (set), (addr))
+#define clrsetbits_le16(addr, clear, set) \
+	iowrite16le((ioread16le(addr) & ~(clear)) | (set), (addr))
+#define clrsetbits_8(addr, clear, set) \
+	iowrite8((ioread8(addr) & ~(clear)) | (set), (addr))
+
 /*
  *  IO port access primitives
  *  -------------------------
@@ -408,6 +437,8 @@ void __iomem *ioremap_wc(resource_size_t
 #define ioremap_wc ioremap_wc
 #define ioremap_wt ioremap_wc
 
+void __iomem *ioremap_cache_ns(resource_size_t res_cookie, size_t size);
+
 void iounmap(volatile void __iomem *iomem_cookie);
 #define iounmap iounmap
 
--- a/arch/arm/include/asm/mach/map.h
+++ b/arch/arm/include/asm/mach/map.h
@@ -21,9 +21,9 @@ struct map_desc {
 	unsigned int type;
 };
 
-/* types 0-3 are defined in asm/io.h */
+/* types 0-4 are defined in asm/io.h */
 enum {
-	MT_UNCACHED = 4,
+	MT_UNCACHED = 5,
 	MT_CACHECLEAN,
 	MT_MINICLEAN,
 	MT_LOW_VECTORS,
--- a/arch/arm/include/asm/pgtable.h
+++ b/arch/arm/include/asm/pgtable.h
@@ -118,6 +118,13 @@ extern pgprot_t		pgprot_s2_device;
 #define pgprot_noncached(prot) \
 	__pgprot_modify(prot, L_PTE_MT_MASK, L_PTE_MT_UNCACHED)
 
+#define pgprot_cached(prot) \
+	__pgprot_modify(prot, L_PTE_MT_MASK, L_PTE_MT_DEV_CACHED)
+
+#define pgprot_cached_ns(prot) \
+	__pgprot_modify(prot, L_PTE_MT_MASK, L_PTE_MT_DEV_CACHED | \
+			L_PTE_MT_DEV_NONSHARED)
+
 #define pgprot_writecombine(prot) \
 	__pgprot_modify(prot, L_PTE_MT_MASK, L_PTE_MT_BUFFERABLE)
 
--- a/arch/arm/kernel/bios32.c
+++ b/arch/arm/kernel/bios32.c
@@ -11,6 +11,8 @@
 #include <linux/slab.h>
 #include <linux/init.h>
 #include <linux/io.h>
+#include <linux/of_irq.h>
+#include <linux/pcieport_if.h>
 
 #include <asm/mach-types.h>
 #include <asm/mach/map.h>
@@ -64,6 +66,47 @@ void pcibios_report_status(u_int status_
 }
 
 /*
+ * Check device tree if the service interrupts are there
+ */
+int pcibios_check_service_irqs(struct pci_dev *dev, int *irqs, int mask)
+{
+	int ret, count = 0;
+	struct device_node *np = NULL;
+
+	if (dev->bus->dev.of_node)
+		np = dev->bus->dev.of_node;
+
+	if (np == NULL)
+		return 0;
+
+	if (!IS_ENABLED(CONFIG_OF_IRQ))
+		return 0;
+
+	/* If root port doesn't support MSI/MSI-X/INTx in RC mode,
+	 * request irq for aer
+	 */
+	if (mask & PCIE_PORT_SERVICE_AER) {
+		ret = of_irq_get_byname(np, "aer");
+		if (ret > 0) {
+			irqs[PCIE_PORT_SERVICE_AER_SHIFT] = ret;
+			count++;
+		}
+	}
+
+	if (mask & PCIE_PORT_SERVICE_PME) {
+		ret = of_irq_get_byname(np, "pme");
+		if (ret > 0) {
+			irqs[PCIE_PORT_SERVICE_PME_SHIFT] = ret;
+			count++;
+		}
+	}
+
+	/* TODO: add more service interrupts if there it is in the device tree*/
+
+	return count;
+}
+
+/*
  * We don't use this to fix the device, but initialisation of it.
  * It's not the correct use for this, but it works.
  * Note that the arbiter/ISA bridge appears to be buggy, specifically in
--- a/arch/arm/mm/dma-mapping.c
+++ b/arch/arm/mm/dma-mapping.c
@@ -2410,6 +2410,7 @@ void arch_setup_dma_ops(struct device *d
 
 	set_dma_ops(dev, dma_ops);
 }
+EXPORT_SYMBOL(arch_setup_dma_ops);
 
 void arch_teardown_dma_ops(struct device *dev)
 {
--- a/arch/arm/mm/ioremap.c
+++ b/arch/arm/mm/ioremap.c
@@ -398,6 +398,13 @@ void __iomem *ioremap_wc(resource_size_t
 }
 EXPORT_SYMBOL(ioremap_wc);
 
+void __iomem *ioremap_cache_ns(resource_size_t res_cookie, size_t size)
+{
+	return arch_ioremap_caller(res_cookie, size, MT_MEMORY_RW_NS,
+				   __builtin_return_address(0));
+}
+EXPORT_SYMBOL(ioremap_cache_ns);
+
 /*
  * Remap an arbitrary physical address space into the kernel virtual
  * address space as memory. Needed when the kernel wants to execute
--- a/arch/arm/mm/mmu.c
+++ b/arch/arm/mm/mmu.c
@@ -313,6 +313,13 @@ static struct mem_type mem_types[] __ro_
 		.prot_sect = PMD_TYPE_SECT | PMD_SECT_AP_WRITE,
 		.domain    = DOMAIN_KERNEL,
 	},
+	[MT_MEMORY_RW_NS] = {
+		.prot_pte  = L_PTE_PRESENT | L_PTE_YOUNG | L_PTE_DIRTY |
+			     L_PTE_XN,
+		.prot_l1   = PMD_TYPE_TABLE,
+		.prot_sect = PMD_TYPE_SECT | PMD_SECT_AP_WRITE | PMD_SECT_XN,
+		.domain    = DOMAIN_KERNEL,
+	},
 	[MT_ROM] = {
 		.prot_sect = PMD_TYPE_SECT,
 		.domain    = DOMAIN_KERNEL,
@@ -644,6 +651,7 @@ static void __init build_mem_type_table(
 	}
 	kern_pgprot |= PTE_EXT_AF;
 	vecs_pgprot |= PTE_EXT_AF;
+	mem_types[MT_MEMORY_RW_NS].prot_pte |= PTE_EXT_AF | cp->pte;
 
 	/*
 	 * Set PXN for user mappings
@@ -672,6 +680,7 @@ static void __init build_mem_type_table(
 	mem_types[MT_MEMORY_RWX].prot_pte |= kern_pgprot;
 	mem_types[MT_MEMORY_RW].prot_sect |= ecc_mask | cp->pmd;
 	mem_types[MT_MEMORY_RW].prot_pte |= kern_pgprot;
+	mem_types[MT_MEMORY_RW_NS].prot_sect |= ecc_mask | cp->pmd;
 	mem_types[MT_MEMORY_DMA_READY].prot_pte |= kern_pgprot;
 	mem_types[MT_MEMORY_RWX_NONCACHED].prot_sect |= ecc_mask;
 	mem_types[MT_ROM].prot_sect |= cp->pmd;
--- a/arch/arm64/include/asm/cache.h
+++ b/arch/arm64/include/asm/cache.h
@@ -18,7 +18,7 @@
 
 #include <asm/cachetype.h>
 
-#define L1_CACHE_SHIFT		7
+#define L1_CACHE_SHIFT		6
 #define L1_CACHE_BYTES		(1 << L1_CACHE_SHIFT)
 
 /*
--- a/arch/arm64/include/asm/io.h
+++ b/arch/arm64/include/asm/io.h
@@ -171,6 +171,8 @@ extern void __iomem *ioremap_cache(phys_
 #define ioremap_nocache(addr, size)	__ioremap((addr), (size), __pgprot(PROT_DEVICE_nGnRE))
 #define ioremap_wc(addr, size)		__ioremap((addr), (size), __pgprot(PROT_NORMAL_NC))
 #define ioremap_wt(addr, size)		__ioremap((addr), (size), __pgprot(PROT_DEVICE_nGnRE))
+#define ioremap_cache_ns(addr, size)   __ioremap((addr), (size), \
+                                                __pgprot(PROT_NORMAL_NS))
 #define iounmap				__iounmap
 
 /*
@@ -184,6 +186,34 @@ extern void __iomem *ioremap_cache(phys_
 #define iowrite32be(v,p)	({ __iowmb(); __raw_writel((__force __u32)cpu_to_be32(v), p); })
 #define iowrite64be(v,p)	({ __iowmb(); __raw_writeq((__force __u64)cpu_to_be64(v), p); })
 
+/* access ports */
+#define setbits32(_addr, _v) iowrite32be(ioread32be(_addr) |  (_v), (_addr))
+#define clrbits32(_addr, _v) iowrite32be(ioread32be(_addr) & ~(_v), (_addr))
+
+#define setbits16(_addr, _v) iowrite16be(ioread16be(_addr) |  (_v), (_addr))
+#define clrbits16(_addr, _v) iowrite16be(ioread16be(_addr) & ~(_v), (_addr))
+
+#define setbits8(_addr, _v) iowrite8(ioread8(_addr) |  (_v), (_addr))
+#define clrbits8(_addr, _v) iowrite8(ioread8(_addr) & ~(_v), (_addr))
+
+/* Clear and set bits in one shot.  These macros can be used to clear and
+ * set multiple bits in a register using a single read-modify-write.  These
+ * macros can also be used to set a multiple-bit bit pattern using a mask,
+ * by specifying the mask in the 'clear' parameter and the new bit pattern
+ * in the 'set' parameter.
+ */
+
+#define clrsetbits_be32(addr, clear, set) \
+	iowrite32be((ioread32be(addr) & ~(clear)) | (set), (addr))
+#define clrsetbits_le32(addr, clear, set) \
+	iowrite32le((ioread32le(addr) & ~(clear)) | (set), (addr))
+#define clrsetbits_be16(addr, clear, set) \
+	iowrite16be((ioread16be(addr) & ~(clear)) | (set), (addr))
+#define clrsetbits_le16(addr, clear, set) \
+	iowrite16le((ioread16le(addr) & ~(clear)) | (set), (addr))
+#define clrsetbits_8(addr, clear, set) \
+	iowrite8((ioread8(addr) & ~(clear)) | (set), (addr))
+
 #include <asm-generic/io.h>
 
 /*
--- a/arch/arm64/include/asm/pci.h
+++ b/arch/arm64/include/asm/pci.h
@@ -31,6 +31,10 @@ static inline int pci_get_legacy_ide_irq
 	return -ENODEV;
 }
 
+#define HAVE_PCI_MMAP
+extern int pci_mmap_page_range(struct pci_dev *dev, struct vm_area_struct *vma,
+			       enum pci_mmap_state mmap_state,
+			       int write_combine);
 static inline int pci_proc_domain(struct pci_bus *bus)
 {
 	return 1;
--- a/arch/arm64/include/asm/pgtable-prot.h
+++ b/arch/arm64/include/asm/pgtable-prot.h
@@ -48,6 +48,7 @@
 #define PROT_NORMAL_NC		(PROT_DEFAULT | PTE_PXN | PTE_UXN | PTE_DIRTY | PTE_WRITE | PTE_ATTRINDX(MT_NORMAL_NC))
 #define PROT_NORMAL_WT		(PROT_DEFAULT | PTE_PXN | PTE_UXN | PTE_DIRTY | PTE_WRITE | PTE_ATTRINDX(MT_NORMAL_WT))
 #define PROT_NORMAL		(PROT_DEFAULT | PTE_PXN | PTE_UXN | PTE_DIRTY | PTE_WRITE | PTE_ATTRINDX(MT_NORMAL))
+#define PROT_NORMAL_NS         (PTE_TYPE_PAGE | PTE_AF | PTE_PXN | PTE_UXN | PTE_DIRTY | PTE_WRITE | PTE_ATTRINDX(MT_NORMAL))
 
 #define PROT_SECT_DEVICE_nGnRE	(PROT_SECT_DEFAULT | PMD_SECT_PXN | PMD_SECT_UXN | PMD_ATTRINDX(MT_DEVICE_nGnRE))
 #define PROT_SECT_NORMAL	(PROT_SECT_DEFAULT | PMD_SECT_PXN | PMD_SECT_UXN | PMD_ATTRINDX(MT_NORMAL))
--- a/arch/arm64/include/asm/pgtable.h
+++ b/arch/arm64/include/asm/pgtable.h
@@ -367,6 +367,11 @@ static inline int pmd_protnone(pmd_t pmd
 	__pgprot_modify(prot, PTE_ATTRINDX_MASK, PTE_ATTRINDX(MT_DEVICE_nGnRnE) | PTE_PXN | PTE_UXN)
 #define pgprot_writecombine(prot) \
 	__pgprot_modify(prot, PTE_ATTRINDX_MASK, PTE_ATTRINDX(MT_NORMAL_NC) | PTE_PXN | PTE_UXN)
+#define pgprot_cached(prot) \
+	__pgprot_modify(prot, PTE_ATTRINDX_MASK, PTE_ATTRINDX(MT_NORMAL) | \
+			PTE_PXN | PTE_UXN)
+#define pgprot_cached_ns(prot) \
+	__pgprot(pgprot_val(pgprot_cached(prot)) ^ PTE_SHARED)
 #define pgprot_device(prot) \
 	__pgprot_modify(prot, PTE_ATTRINDX_MASK, PTE_ATTRINDX(MT_DEVICE_nGnRE) | PTE_PXN | PTE_UXN)
 #define __HAVE_PHYS_MEM_ACCESS_PROT
--- a/arch/arm64/kernel/pci.c
+++ b/arch/arm64/kernel/pci.c
@@ -17,6 +17,8 @@
 #include <linux/mm.h>
 #include <linux/of_pci.h>
 #include <linux/of_platform.h>
+#include <linux/of_irq.h>
+#include <linux/pcieport_if.h>
 #include <linux/pci.h>
 #include <linux/pci-acpi.h>
 #include <linux/pci-ecam.h>
@@ -53,6 +55,66 @@ int pcibios_alloc_irq(struct pci_dev *de
 
 	return 0;
 }
+
+/*
+ * Check device tree if the service interrupts are there
+ */
+int pcibios_check_service_irqs(struct pci_dev *dev, int *irqs, int mask)
+{
+	int ret, count = 0;
+	struct device_node *np = NULL;
+
+	if (dev->bus->dev.of_node)
+		np = dev->bus->dev.of_node;
+
+	if (np == NULL)
+		return 0;
+
+	if (!IS_ENABLED(CONFIG_OF_IRQ))
+		return 0;
+
+	/* If root port doesn't support MSI/MSI-X/INTx in RC mode,
+	 * request irq for aer
+	 */
+	if (mask & PCIE_PORT_SERVICE_AER) {
+		ret = of_irq_get_byname(np, "aer");
+		if (ret > 0) {
+			irqs[PCIE_PORT_SERVICE_AER_SHIFT] = ret;
+			count++;
+		}
+	}
+
+	if (mask & PCIE_PORT_SERVICE_PME) {
+		ret = of_irq_get_byname(np, "pme");
+		if (ret > 0) {
+			irqs[PCIE_PORT_SERVICE_PME_SHIFT] = ret;
+			count++;
+		}
+	}
+
+	/* TODO: add more service interrupts if there it is in the device tree*/
+
+	return count;
+}
+
+int pci_mmap_page_range(struct pci_dev *dev, struct vm_area_struct *vma,
+			enum pci_mmap_state mmap_state, int write_combine)
+{
+	if (mmap_state == pci_mmap_io)
+		return -EINVAL;
+
+	/*
+	 * Mark this as IO
+	 */
+	vma->vm_page_prot = pgprot_noncached(vma->vm_page_prot);
+
+	if (remap_pfn_range(vma, vma->vm_start, vma->vm_pgoff,
+			     vma->vm_end - vma->vm_start,
+			     vma->vm_page_prot))
+		return -EAGAIN;
+
+	return 0;
+}
 
 /*
  * raw_pci_read/write - Platform-specific PCI config space access.
--- a/arch/arm64/mm/dma-mapping.c
+++ b/arch/arm64/mm/dma-mapping.c
@@ -30,6 +30,7 @@
 #include <linux/swiotlb.h>
 
 #include <asm/cacheflush.h>
+#include <../../../drivers/staging/fsl-mc/include/mc-bus.h>
 
 static int swiotlb __ro_after_init;
 
@@ -925,6 +926,10 @@ static int __init __iommu_dma_init(void)
 	if (!ret)
 		ret = register_iommu_dma_ops_notifier(&pci_bus_type);
 #endif
+#ifdef CONFIG_FSL_MC_BUS
+	if (!ret)
+		ret = register_iommu_dma_ops_notifier(&fsl_mc_bus_type);
+#endif
 	return ret;
 }
 arch_initcall(__iommu_dma_init);
@@ -978,3 +983,4 @@ void arch_setup_dma_ops(struct device *d
 	dev->archdata.dma_coherent = coherent;
 	__iommu_setup_dma_ops(dev, dma_base, size, iommu);
 }
+EXPORT_SYMBOL(arch_setup_dma_ops);
