From 25bf2b5836c892f091651d8a3384c9c57ce1b400 Mon Sep 17 00:00:00 2001
From: Jonas Gorski <jogo@openwrt.org>
Date: Thu, 26 Jun 2014 12:51:00 +0200
Subject: [PATCH 46/48] MIPS: BCM63XX: add support for matching the board_info
 by dtb

Allow using the passed dtb's compatible property to match board_info
structs instead of nvram's boardname field, which is not unique anyway.

Signed-off-by: Jonas Gorski <jogo@openwrt.org>
---
 arch/mips/bcm63xx/boards/board_bcm963xx.c |   15 +++++++++++++++
 arch/mips/bcm63xx/boards/board_common.c   |   18 ++++++++++++++++++
 arch/mips/bcm63xx/boards/board_common.h   |    3 +++
 3 files changed, 36 insertions(+)

--- a/arch/mips/bcm63xx/boards/board_bcm963xx.c
+++ b/arch/mips/bcm63xx/boards/board_bcm963xx.c
@@ -695,6 +695,10 @@ static const struct board_info __initcon
 #endif
 };
 
+static struct of_device_id const bcm963xx_boards_dt[] = {
+	{ },
+};
+
 /*
  * early init callback, read nvram data from flash and checksum it
  */
@@ -706,6 +710,7 @@ void __init board_bcm963xx_init(void)
 	char *board_name = NULL;
 	u32 val;
 	struct bcm_hcs *hcs;
+	const struct of_device_id *board_match;
 
 	/* read base address of boot chip select (0)
 	 * 6328/6362 do not have MPI but boot from a fixed address
@@ -745,6 +750,16 @@ void __init board_bcm963xx_init(void)
 	} else {
 		board_name = bcm63xx_nvram_get_name();
 	}
+
+	/* find board by compat */
+	board_match = bcm63xx_match_board(bcm963xx_boards_dt);
+	if (board_match) {
+		board_early_setup(board_match->data,
+				  bcm63xx_nvram_get_mac_address);
+
+		return;
+	}
+
 	/* find board by name */
 	for (i = 0; i < ARRAY_SIZE(bcm963xx_boards); i++) {
 		if (strncmp(board_name, bcm963xx_boards[i]->name, 16))
--- a/arch/mips/bcm63xx/boards/board_common.c
+++ b/arch/mips/bcm63xx/boards/board_common.c
@@ -243,3 +243,21 @@ int __init board_register_devices(void)
 
 	return 0;
 }
+
+const struct of_device_id * __init bcm63xx_match_board(const struct of_device_id *m)
+{
+	const struct of_device_id *match;
+	unsigned long dt_root;
+
+	if (!IS_ENABLED(CONFIG_OF) || !initial_boot_params)
+		return NULL;
+
+	dt_root = of_get_flat_dt_root();
+
+	for (match = m; match->compatible[0]; match++) {
+		if (of_flat_dt_is_compatible(dt_root, match->compatible))
+			return match;
+	}
+
+	return NULL;
+}
--- a/arch/mips/bcm63xx/boards/board_common.h
+++ b/arch/mips/bcm63xx/boards/board_common.h
@@ -1,11 +1,14 @@
 #ifndef __BOARD_COMMON_H
 #define __BOARD_COMMON_H
 
+#include <linux/of.h>
 #include <board_bcm963xx.h>
 
 void board_early_setup(const struct board_info *board,
 		       int (*get_mac_address)(u8 mac[ETH_ALEN]));
 
+const struct of_device_id *bcm63xx_match_board(const struct of_device_id *);
+
 #if defined(CONFIG_BOARD_BCM963XX)
 void board_bcm963xx_init(void);
 #else
